arXiv:0911.2334v1 [nlin.AO] 12 Nov 2009

PHYSCON 2009, Catania, Italy, September, 1–September, 4 2009

FEEDBACK-DEPENDENT CONTROL OF STOCHASTIC SYNCHRONIZATION IN COUPLED NEURAL SYSTEMS

Philipp Hövel, Sarang A. Shah, Markus A. Dahlem, and Eckehard Schöll^∗

Institut für Theoretische Physik, Technische Universität Berlin, Hardenbergstraße 38, 10623 Berlin, Germany ∗schoell@physik.tu-berlin.de

Abstract We investigate the synchronization dynamics of two coupled noise-driven FitzHugh-Nagumo systems, representing two neural populations. For certain choices of the noise intensities and coupling strength, we find cooperative stochastic dynamics such as frequency synchronization and phase synchronization, where the degree of synchronization can be quantified by the ratio of the interspike interval of the two excitable neural populations and the phase synchronization index, respectively. The stochastic synchronization can be either enhanced or suppressed by local time-delayed feedback control, depending upon the delay time and the coupling strength. The control depends crucially upon the coupling scheme of the control force, i.e., whether the control force is generated from the activator or inhibitor signal, and applied to either component. For inhibitor self-coupling, synchronization is most strongly enhanced, whereas for activator self-coupling there exist distinct values of the delay time where the synchronization is strongly suppressed even in the strong synchronization regime. For cross-coupling strongly modulated behavior is found.

Key words Synchronization, noise, coupling, time-delayed feedback

1 Introduction The control of unstable or irregular states of nonlinear dynamic systems has many applications in different fields of physics, chemistry, biology, and medicine (Schöll and Schuster, 2008). A particularly simple and efficient control scheme is time-delayed feedback (Pyragas, 1992) which occurs naturally in a number of biological systems including neural networks where both propagation delays and local neurovascular couplings lead to time delays (Haken, 2006; Wilson, 1999; Gerstner and Kistler, 2002). Moreover, time-delayed feedback loops might be deliberately implemented to control neural disturbances, e.g., to suppress undesired synchrony of firing neurons in Parkinson’s disease or epilepsy (Schiff et al., 1994; Rosenblum and Pikovsky, 2004a; Popovych et al., 2005). Here we study coupled neural systems subject to noise and timedelayed feedback (Hauschildt et al., 2006; Hövel et al., 2009; Schöll et al., 2009a; Schöll et al., 2009b). In particular we focus upon the question how stochastic synchronization of noise-induced oscillations of two coupled neural populations can be controlled by timedelayed feedback, and how robust this is with respect to different coupling schemes of the control force. Time-delayed feedback control of noise-induced oscillations was demonstrated in a single excitable system (Janson et al., 2004; Balanov et al., 2004; Prager et al., 2007; Pototsky and Janson, 2008). The simplest network configuration displaying features of neural interaction consists of two coupled excitable systems. In order to grasp the complicated interaction between billions of neurons in large neural networks, those are often lumped into groups of neural populations each of which can be represented as an effective excitable element that is mutually coupled to the other elements (Rosenblum and Pikovsky, 2004b; Popovych et al., 2005). In this sense the simplest model which may reveal features of interacting neurons consists of two coupled neural oscillators. Each of these will be represented by a simplified FitzHugh-Nagumo (FHN) system (FitzHugh, 1960; Nagumo et al., 1962), which is often used as a generic model for neurons, or more generally, excitable systems (Lindner et al., 2004). This paper is organized as follow: We introduce the model equations and the feedback scheme in Sec. 2. Sec. 3 is devoted to two measures of the stochastic synchronization. These are investigated for different coupling schemes of the feedback in Sec. 4. Finally, we conlcude in Sec. 5.

2 Model Equations Neurons are excitable units which can emit spikes or bursts of electrical signals, i.e., the system rests in a stable steady state, but after it is excited beyond a threshold, it emits a pulse. In the following, we consider electrically coupled neurons modelled by the FitzHugh-

Figure 1. Schematic diagram of two coupled FitzHugh-Nagumo systems with time-delayed feedback applied to the first subsystem.

K and τ denote the feedback gain and time delay, respectively, and C is the coupling strength.

Nagumo system in the excitable regime:

ε_1 du_1 dt = f (u_1, v_1) + C (u_2 − u_1) (1a) dv_1 dt = g (u_1, v_1) + D_1ξ_1 (1b)

ε_2 du_2 dt = f (u_2, v_2) + C (u_1 − u_2) (2a) dv_2 dt = g (u_2, v_2) + D_2ξ_2 (2b)

with f (u_i, v_i) = u_i −u^3_i /3−v_i and g (u_i, v_i) = u_i +a (i = 1, 2). The fast activator variables u_i (i = 1, 2) refer to the transmembrane voltage, and the slow inhibitor variables v_i are related to the electrical conductance of the relevant ion currents. The parameter a is the excitability parameter. For the purposes of this paper, a is fixed at 1.05, such that there are no autonomous oscillations (excitable regime). C is the diffusive coupling strength between u_1 and u_2. To introduce different time scales for both systems, ε_1 is set to 0.005 and ε_2 is set to 0.1. Both systems, when uncoupled, are driven entirely by independent noise sources, which in the above equations are represented by ξ_i (i = 1, 2, Gaussian white noise with zero mean and unity variance). D_i is the noise intensity, and for the purposes of this paper, D_2 will be held fixed at 0.09 (Hauschildt et al., 2006).

The control force which we apply only to the first of the neural populations as schematically depicted in Fig. 1 is known as time-delay autosynchronization (TDAS) or time-delayed feedback control. This method was initially introduced by Pyragas (Pyragas, 1992) for controlling periodic orbits in chaotic systems. It has been effective in a variety of experimental applications at controlling oscillatory behavior and can be easily implemented in many analog devices (Schöll and Schuster, 2008). TDAS constructs a feedback F from the difference between the current value of a control signal w and the value for that quantity at time t − τ.

The difference is then multiplied by the gain coefficient K F (t) = K[w(t − τ) − w(t)], (3) where w determines which components of the system enter the feedback as will be discussed in the following. The variable w in the control force can be either the activator u_1 or the inhibitor v_1. Also, the control force can either be applied to the activator or the inhibitor differential equation. These possibilities lead to two self-coupling schemes (uu and vv) where either the activator is coupled to the activator equation or the inhibitor is coupled to the inhibitor equation, and two cross-coupling schemes (uv and vu). Thus, Eqs. (1) of the first subsystem can be rewritten including timedelayed feedback as ( ε_1^{du1}_{dtdv1} dt ) = ( f (u_1, v_1) + C (u_2 − u_1) g (u_1, v_1) + D_1ξ_1 ) (4) +K ( A_{uu} A_{uv} A_{vu} A_{vv} ) ( u_1(t − τ) − u_1(t) v_1(t − τ) − v_1(t) ) ,

where the coupling matrix elements A_{ij} with i, j ∈ {u, v} define the specific coupling scheme. Next, we will discuss cooperative stochastic dynamics resulting in frequency synchronization and phase synchronization in the following Sections.

3 Measures of Synchronization A measure of frequency synchronization is the ratio of the interspike intervals (ISI) of the two neural populations (Hauschildt et al., 2006; Hövel et al., 2009). The respective average ISI of each neural population is denoted by ⟨T_1⟩ and ⟨T_2⟩. The ratio ⟨T_1⟩/⟨T_2⟩ compares the average time scales of both systems, where unity ratio describes two systems spiking at the same average frequency. It is for this reason that the ISI ratio is often considered as a measure of frequency synchronization. It does not contain information about the phase of synchronization, and a given ISI ratio can also result from different ISI distributions.

In order to account for the phase difference between two systems, one can define a phase (Pikovsky et al., 1996; Pikovsky et al., 2001; Hauschildt et al., 2006) φ(t) = 2π t − t_{i−1} t_i − t_{i−1} + 2π(i − 1) (5)

where i = 1, 2, . . . . t_i denotes the time of the ith spike. The phase difference between two consecutive spikes is 2π. The phase difference of 1:1 synchronization is

Δφ(t) = |φ_1(t) − φ_2(t)| , (6)

where φ_1(t) and φ_2(t) are the phases of the first and second system, respectively. Two systems that are

Figure 2. (Color online) Panels (a) and (b) show the ratio of interspike intervals ⟨T1⟩/⟨T2⟩ and the phase synchronization index γ of the two subsystems as color code in dependence on the coupling strength C and noise intensity D1, respectively. No control is applied to the system. The dots mark the parameter choice for different synchronization regimes used in the following. Other parameters:

ε_1 = 0.005, ε_2 = 0.1, a = 1.05, and D_2 = 0.09.

phase synchronized at a given time satisfy Δφ = 0. Finally, the overall time-averaged phase synchronization of two systems can be quantified using the synchronization index γ = √ ⟨cos Δφ(t)⟩^2 + ⟨sin Δφ(t)⟩^2. (7)

A value of 0 indicates no synchronization, while a value of unity indicates perfect synchronization. Figure 2 depicts both measures for stochastic synchronization in the (D_1, C) plane, both exhibiting very similar behavior. Panel (a) refers to the frequency synchronization characterized by the ratio of the average ISIs ⟨T_1⟩/⟨T_2⟩ and panel (b) shows the phase synchronization index γ. The green dots mark parameter values used in Sec. 4. Note that both panels share the same color code. For a small value of D_1 and large coupling strength, the two subsystems display well synchronized behavior, ⟨T_1⟩/⟨T_2⟩ ≈ 1 and γ ≈ 1. The timescales in the interacting systems adjust themselves to 1 : 1 synchronization. On average, they show the same number of spikes and the two subsystems are in-phase which is indicated by yellow color. The two subsystems are less synchronized in the dark blue and black regions. In the following we show the ratio of the average interspike interval ⟨T_1⟩/⟨T_2⟩ and the phase synchronization index γ which are color coded in the (τ, K) plane for fixed combinations of D_1 and C. For each coupling scheme of time-delayed feedback control (cross-coupling schemes uv and vu and self-coupling schemes uu and vv) we present a selection of (D_1, C) values. In all cases, only one element of the coupling matrix A is equal to unity and all other elements are zero.

4 Coupling Schemes After the introduction of the system and the coupling schemes, we will present results on frequency and phase synchronization in the following. We consider 16 different combinations of the noise intensity D_1 and the coupling strength C which are marked as green dots in Fig. 2. The ordering of panels in Figs. 3 to 10 is the following: The rows correspond to fixed coupling strength chosen as C = 0.01, 0.21, 0.41, and 0.61 from bottom to top. The columns in each figure are calculated for constant noise intensity D_1 = 0.01, 0.34, 0.67, and 1.0 from left to right.

4.1 Frequency Synchronization Figures 3 to 6 show frequency synchronization measured by the ratio of average interspike intervals ⟨T_1⟩/⟨T_2⟩ calculated from the summarized activator variable u_Σ = u_1 + u_2 as color code in dependence on the feedback gain K and the time delay τ. The system’s parameters are fixed in each panel as described above. Figures 3 and 6 correspond to selfcoupling (uu- and vv-coupling) and Figs. 4 and 5 depict the cross-coupling schemes (uv- and vu-coupling). The dynamics in the white regions is outside the excitable regime and does not show noise-induced spiking, but rather the system exhibits large-amplitude selfsustained oscillations.

Figure 3. uu-coupling: Ratio of average interspike intervals

⟨T_1⟩/⟨T_2⟩ as color code. Rows and columns correspond to con-

stant coupling strength C and noise intensity D1, respectively, as marked in Fig. 2 as green dots, and specified in the text. Other parameters as in Fig. 2.

One can see that appropriate tuning of the control parameters leads to enhanced or deteriorated synchronization displayed by bright yellow and dark blue areas, respectively. In each figure, all panels show qualitatively similar features like a modulation of the ratio ⟨T_1⟩/⟨T_2⟩ whose range between maximum and minimum depends on D_1 and C. Comparing the rows, the systems are less (more strongly) synchronized for

Figure 4. uv-coupling: Ratio of average interspike intervals

⟨T_1⟩/⟨T_2⟩ as color code. Rows and columns correspond to con-

stant coupling strength C and noise intensity D1, respectively. Other parameters as in Fig. 2.

Figure 5. vu-coupling: Ratio of average interspike intervals

⟨T_1⟩/⟨T_2⟩ as color code. Rows and columns correspond to con-

stant coupling strength C and noise intensity D1, respectively. Other parameters as in Fig. 2.

small (large) values of C indicated by dark blue (yellow) color. As the noise intensity D_1 increases, the dynamics of the coupled subsystems is more and more noise-dominated and the dependence on the time delay τ becomes less pronounced.

Note the symmetry in the cross-coupling schemes shown as Figs. 4 and 5 between K and its negative value −K for the inverse cross-coupling. The reason is that enhancing the activator yields a similar effects on the dynamics as diminishing the inhibitor variable.

Figure 6. vv-coupling: Ratio of average interspike intervals

⟨T_1⟩/⟨T_2⟩ as color code. Rows and columns correspond to con-

stant coupling strength C and noise intensity D1, respectively. Other parameters as in Fig. 2.

4.2 Phase Synchronization Figures 7 to 10 depict the phase synchronization index γ as color code depending on the control parameters K and τ for uu-, uv-, vu-, and vv-coupling, respectively. The noise intensity D_1 and coupling strength C are fixed for each panel as described in Sec. 4.1.

Figure 7. uu-coupling: Phase synchronization index γ. Noise intensity D1 and coupling strength C chosen as described in Sec. 4.1. Other parameters as in Fig. 2.

Comparing Figs. 7 to 10 with the respective plots for frequency synchronization, i.e., Figs. 3 to 6, one can see that both types of synchronization coincide qualitatively, but the phase synchronization index is more sensitive to the modulation features. Similar to the case of frequency synchronization, time delayed feedback can lead to either enhancement or suppression of phase synchronization depending on the specific choice of the feedback gain K and time delay τ indicated by yellow and dark blue regions. In general, these effects become less sensitive on the time delay as D_1 increases. For larger values of C, the two subsystems show enhanced phase synchronization.

Figure 8. uv-coupling: Phase synchronization index γ. Noise intensity D1 and coupling strength C chosen as described in Sec. 4.1. Other parameters as in Fig. 2.

Figure 9. vu-coupling: Phase synchronization index γ. Noise intensity D1 and coupling strength C chosen as described in Sec. 4.1. Other parameters as in Fig. 2.

Figure 10. vv-coupling: Phase synchronization index γ. Noise intensity D1 and coupling strength C chosen as described in Sec. 4.1. Other parameters as in Fig. 2.

5 Conclusion In summary, we have shown that stochastic synchronization in two coupled neural populations can be tuned by local time-delayed feedback control of one population. Synchronization can be either enhanced or suppressed, depending upon the delay time and the coupling strength. The control dependents crucially upon the coupling scheme of the control force. For inhibitor self-coupling (vv) synchronization is most strongly enhanced, whereas for activator self-coupling (uu) there exist distinct values of τ where the synchronization is strongly suppressed even in the strong synchronization regime. For cross-coupling (uv, vu) there is mixed behavior, and both schemes exhibit a strong symmetry with respect to inverting the sign of K. These observations might be important in the context of the deliberate application of control with the aim of suppressing synchronization, e.g. as therapeutic measures for Parkinson’s disease.

Acknowledgements This work was supported by DFG in the framework of Sfb 555 (Complex Nonlinear Processes). S. A. S. acknowledges support of the Deutsche Akademische Austauschdienst (DAAD) in the framework of the program Research Internships in Science and Engineering (RISE).

References Balanov, A. G., N. B. Janson and E. Schöll (2004). Control of noise-induced oscillations by delayed feedback. Physica D 199, 1–12.

FitzHugh, R. (1960). Thresholds and plateaus in the Hodgkin-Huxley nerve equations. J. Gen. Physiol. 43(5), 867–896.

Gerstner, W. and W. Kistler (2002). Spiking neuron models. Cambridge University Press. Cambridge. Haken, H. (2006). Brain Dynamics: Synchronization and Activity Patterns in Pulse-Coupled Neural Nets with Delays and Noise. Springer Verlag GmbH. Berlin.

Hauschildt, B., N. B. Janson, A. G. Balanov and E. Schöll (2006). Noise-induced cooperative dynamics and its control in coupled neuron models. Phys. Rev. E 74, 051906.

Hövel, P., M. A. Dahlem and E. Schöll (2009). Control of synchronization in coupled neural systems by time-delayed feedback. Int. J. Bifur. Chaos (in print). (arXiv:0809.0819v1).

Janson, N. B., A. G. Balanov and E. Schöll (2004). Delayed feedback as a means of control of noise-induced motion. Phys. Rev. Lett. 93, 010601.

Lindner, B., J. García-Ojalvo, A. Neiman and Lutz Schimansky-Geier (2004). Effects of noise in excitable systems. Phys. Rep. 392, 321–424. Nagumo, J., S. Arimoto and S. Yoshizawa. (1962). An active pulse transmission line simulating nerve axon.. Proc. IRE 50, 2061–2070.

Pikovsky, A., M. G. Rosenblum and J. Kurths (1996). Synchronisation in a population of globally coupled chaotic oscillators. Europhys. Lett. 34, 165. Pikovsky, A., M. G. Rosenblum and J. Kurths (2001). Synchronization, A Universal Concept in Nonlinear Sciences. Cambridge University Press. Cambridge. Popovych, O. V., C. Hauptmann and Peter A. Tass (2005). Effective desynchronization by nonlinear delayed feedback. Phys. Rev. Lett. 94, 164102. Pototsky, Andrey and N. B. Janson (2008). Excitable systems with noise and delay, with applications to control: Renewal theory approach. Phys. Rev. E 77(3), 031113.

Prager, T., H. P. Lerch, Lutz Schimansky-Geier and E. Schöll (2007). Increase of coherence in excitable systems by delayed feedback. J. Phys. A 40, 11045– 11055.

Pyragas, K. (1992). Continuous control of chaos by self-controlling feedback. Phys. Lett. A 170, 421. Rosenblum, M. G. and A. Pikovsky (2004a). Controlling synchronization in an ensemble of globally coupled oscillators. Phys. Rev. Lett. 92, 114102. Rosenblum, M. G. and A. Pikovsky (2004b). Delayed feedback control of collective synchrony: An approach to suppression of pathological brain rhythms. Phys. Rev. E 70, 041904.

Schiff, S. J., K. Jerger, D. H. Duong, T. Chang, M. L. Spano and W. L. Ditto (1994). Controlling chaos in the brain. Nature (London) 370, 615.

Schöll, E. and Schuster, H. G., Eds.) (2008). Handbook of Chaos Control. Wiley-VCH. Weinheim. Second completely revised and enlarged edition.

Schöll, E., G. Hiller, P. Hövel and M. A. Dahlem

(2009a). Time-delayed feedback in neurosystems. Phil. Trans. R. Soc. A 367, 1079–1096.

Schöll, E., P. Hövel, V. Flunkert and M. A. Dahlem (2009b). Time-delayed feedback control: from simple models to lasers and neural systems. In: Complex Time-Delay Systems (F. M. Atay, Ed.). Springer. Berlin.

Wilson, H. R. (1999). Spikes, Decisions, and Actions: The Dynamical Foundations of Neuroscience. Oxford University Press. Oxford.