arXiv:1001.4124v1 [physics.soc-ph] 23 Jan 2010

JSIAM Letters Vol.** (****) pp.1– © **** Japan Society for Industrial and Applied Mathematics

Excluded Volume Effect in Queueing Theory

Daichi Yanagisawa^{1,2}, Akiyasu Tomoeda^{3,4}, Rui Jiang^5 and Katsuhiro Nishinari^{4,6,1}

Department of Aeronautics and Astronautics, School of Engineering, The University of Tokyo, Tokyo 113-8656, Japan^1 Research Fellow of the Japan Society for the Promotion of Science, Tokyo 102-8471, Japan^2 Meiji Institute for Advanced Study of Mathematical Sciences, Meiji University, Kanagawa 214-8571, Japan^3 Research Center for Advanced Science and Technology, The University of Tokyo, Tokyo 153- 8904, Japan^4 School of Engineering Science, University of Science and Technology of China, Hefei 230026, China^5 PRESTO, Japan Science and Technology Agency, Tokyo 102-0075, Japan^6

E-mail tt087068@mail.ecc.u-tokyo.ac.jp

Received

Abstract We have introduced excluded volume effect, which is an important factor to model a realistic pedestrian queue, into queueing theory. The probability distributions of pedestrian number and pedestrian waiting time in a queue have been calculated exactly. Due to time needed to close up the queue, the mean number of pedestrians increases as pedestrian arrival probability (λ) and leaving probability (μ) increase even if the ratio between them (i.e., ρ = λ/μ) remains constant. Furthermore, at a given ρ, the mean waiting time does not increase monotonically with the service time (which is inverse to μ), a minimum could be reached instead.

Keywords Queueing Theory, Asymmetric Simple Exclusion Process, Pedestrian Dynamics Research Activity Group Applied Integrable Systems

1. Introduction

Queueing theory [1] is one of the most famous and important theory in these days since it is applied to many systems in the real world such as traffic systems [2], production systems [3], networks [4], and so on. The mathematical formulation for mean waiting time, which is usually calculated by Little’s theorem [1], is widely used due to its simplicity. In the queueing theory, the state of a queue is represented by the number of jobs, which are vehicles, pedestrians, and packets in networks. When there are some jobs in the queue, one job is always receiving service, and when it leaves the queue, the service for next job starts immediately. This phenomenon is suitable for a queue of packets since operation for next packet starts instantly by a computer. However, it is not realistic for a queue of vehicles and pedestrians since there is a delay of moving to service window due to the excluded volume effect which is not included in the queueing theory.

The excluded volume effect is studied in detail by analyzing the asymmetric simple exclusion process (ASEP) [5]. Many traffic models and pedestrian dynamics models are developed by extending ASEP [6, 7]. They are very successful since the excluded volume effect works adequately to represent real movement of vehicles and pedestrians. Therefore, we introduce the excluded volume effect into the queueing theory for the first time in this paper to develop a practical theory for a pedestrian queue. The probability distributions and the means of both pedestrian number and pedestrian waiting time in a queue are calculated exactly and compared with those obtained from normal queueing models.

2. Models and Mathematical Analysis

2.1 Outline of the Three Queueing Models

As a comparison, in addition to our excluded volume effect introduced queue (E-Queue), we briefly review normal queue (N-Queue) with continuous time (N- Queue (C)) (which is the most famous queueing model known as M/M/1 [1]), as well as that with discrete time (N-Queue (P)). In E-Queue and N-Queue (P), parallel update is adopted because it is realistic for one dimensional pedestrian dynamics [8]. Fig. 1 is a schematic view of N-Queue (P) and E-Queue. At each time step a pedestrian arrives at the queue with probability λ and a pedestrian at the service window (pedestrian A) leaves the queue with probability μ. In N-Queue (P) (Fig. 1 (a)), pedestrian B moves to the service window as soon as pedestrian A leaves the queue. In contrast, pedestrian B cannot move to the service window at time step t+1 in E-Queue (Fig. 1 (b)) due to the excluded volume effect, he/she moves there at time step t + 2.

2.2 Master Equations for N-Queue (P)

Since mathematical analysis on N-Queue (C) is described in detail in many books [1], we start from N- Queue (P). The master equations in the stationary state are described as follows:

P (0) = (1 − λ)P (0) + (1 − λ)μP (1), (1)

P (1) = λP (0) + (1 − λ)μP (2)

– 1 –

Fig. 1. Schematic views of time variation of queueing states. (a) N-Queue (P). (b) E-Queue. The cell at the right end in the queue is the service window. λ ∈ [0, 1] and μ ∈ [0, 1] represent the arrival probability and the service probability, respectively.

+ {λμ + (1 − λ)(1 − μ)}P (1), (2)

P (n) = λ(1 − μ)P (n − 1) + (1 − λ)μP (n + 1)

+ {λμ + (1 − λ)(1 − μ)}P (n) (n ≥ 2), (3)

where P (n) represents the probability that there are n ∈ [0, ∞) pedestrians in the queue. Note that the stationary state exits only when λ < λ_{cr} is satisfied. λ_{cr} is a critical value of λ, and when λ ≥ λ_{cr}, queue length tends to infinity. By solving these recurrence equations among three terms, we obtain P (n), and P_W (t) (t ∈ [0, ∞)) (Probability distribution of the waiting time, i.e., time between a pedestrian arrives at the queue and leaves there.), N = ∑_∞ n=0 nP (n) (Mean number of pedestrians in the queue), and W = ∑_∞ t=0 tP_W (t) (Mean waiting time) are calculated as shown in Tab. 1.

2.3 Exact Solution for E-Queue

In E-Queue, the state is determined not only by pedestrian number n. Fortunately, due to deterministic movement of pedestrians in the queue (i.e., pedestrians move one cell in one time step if their proceeding cell is vacant), two consecutive vacant cells never appear in the stationary state. As a result, there are 2^n states when there are n pedestrians in the queue since we only need to consider whether there is a vacant cell or not in front of each pedestrian. Schematic views of the stationary states in the case n = 2 are depicted in Fig. 2.

Our target in this paper is to obtain probability distributions of pedestrian number and pedestrian waiting

Fig. 2. Schematic views of the stationary states of E-Queue in the case n = 2. (a) Group A. The service window is occupied by a pedestrian. (b) Group B. The service window is vacant.

Fig. 3. State transition diagram of E-Queue.

time, so that the 2^n states do not need to be distinguished completely. The important point is that whether the service window is occupied or not. Thus, the 2^n states are divided into two groups A and B. The service window is occupied in group A and it is vacant in group B. For instance, two states belonging to group A, and the other two states belonging to group B in the case n = 2 as shown in Fig. 2.

We describe the sum of the probabilities of the stationary states in group A as P_A(n) and that in group B as P_B (n) when there are n pedestrians in the queue. Thus, P (n) = P_A(n) + P_B (n). Note that we have P_A(0) = 0 and P_B (0) = P (0). The state transition diagram of E- Queue is depicted as Fig. 3 and the master equations in the stationary state are described as follows:

P_A(1) = (1 − λ)(1 − μ)P_A(1) + λP_B (0)

+ (1 − λ)P_B (1), (4)

P_A(n) = λ(1 − μ)P_A(n − 1)

+ (1 − λ)(1 − μ)P_A(n) + λP_B (n − 1)

+ (1 − λ)P_B (n) (n ≥ 2), (5)

P_B (0) = (1 − λ)P_B (0) + (1 − λ)μP_A(1), (6)

P_B (n) = λμP_A(n) + (1 − λ)μP_A(n + 1)

(n ≥ 1). (7)

These equations could also be obtained by reducing the master equations where all 2^n states are distinguished [9]. Solving the equations with normalization condition ∑_∞ n=0 P (n) = 1, we obtain the solutions in Tab. 1 in the case λ < λ_{cr}. The probability distribution of the waiting time P_W (t) is also calculated as

P_W (t) =f(t, 1)P (0) + Q(t,2)∑

n=1 [f(t − n, n)μP_A(n)]+ Q(t−1,2) ∑ n=1 [ f(t − n, n + 1){(1 − μ)P_A(n) + P_B (n)} ] (8) where Q(a, b) returns a quotient of a/b, and f(t, n) = ( t − 1 n − 1 ) μ^n(1 − μ)^{t−n} is the negative binomial distribu-

tion. The means, i.e., N and W , are also obtained and described in Tab. 1.

– 2 –

JSIAM Letters Vol. ** (****) pp.1– Daichi Yanagisawa et al.

Table 1. Mathematical formulations of physical quantities of three queueing models. The parameter ρ = λ/μ represents the ratio between the mean service time (1/μ) and the mean arrival time (1/λ). The expressions of P (n) and P_W (t) in the table are valid for N-Queue (C) when n ≥ 0 and t ≥ 0, respectively, whereas, those are valid in the two parallel update’s queues only when n ≥ 1 and t ≥ 1. P_W (0) = 0 for N-Queue (P) and E-Queue. Note that the Little’s theorem N = λW is satisfied in all three models.

Type N-Queue (C) N-Queue (P) E-Queue Other Expressions for E-Queue λ_{cr} μ μ μ 1 + μ PA(n) = r^{n−1} λ (1 − λ)μ P (0)

P (0) 1 − ρ 1 − ρ 1 − ρ 1 − λ P (n) (1 − ρ)ρ^n 1 − ρ 1 − μ ( 1 − μ 1 − λ ρ )_n ( 1 − ρ 1 − λ ) r^n 1 − μ + λμ PB (n) = r^{n−1} λ^2 (1 − λ)^2μ

P (0) N ρ 1 − ρ (1 − λ) ρ 1 − ρ ρ 1 −^ρ_{1−λ} P_W (t) μ(1 − ρ) exp[−μ(1 − ρ)t] μ(1 − ρ) 1 − λ ( 1 − μ 1 − λ )_{t−1} ( μ − λ 1 − λ ) ( 1 1 − λ − μ )_{t−1} r = 1 − μ + λμ (1 − λ)^2 ρ W 1 λ ρ 1 − ρ 1 − λ λ ρ 1 − ρ ρ λ ( 1 −^ρ_{1−λ} )

3. N-Queue V.S. E-Queue

In this section, we compare physical quantities of the three queueing models. Note that λ and μ are probabilities in N-Queue (P) and E-Queue, while they are rates in N-Queue (C). Besides, t is discrete in the former models, whereas it is continuous in the latter one. However, if we regard one time step in the former two models as unit time in N-Queue (C), we can compare the physical quantities of the models in the same time scale. The physical quantities are described by three parameters, which are λ, μ, and ρ as in Tab. 1. However, since ρ = λ/μ, there are only two independent variables; thus, we use ρ and μ as independent ones in the following. Then, λ becomes a function of ρ and μ described as λ(ρ, μ) = ρμ.

3.1 Critical Value λ_{cr}

In N-Queues, the critical value λ_{cr} = μ. In E-Queue, λ_{cr} = μ/(1 + μ). Since μ/(1 + μ) ≤ μ , the region where stationary state exists in ρ − μ space is smaller in E- Queue than in N-Queues. Due to time needed to close up vacant cells, which equals to one time step, the length of E-Queue diverges easier than that of N-Queues.

3.2 Mean Pedestrian Number in a Queue

This subsection focuses on mean pedestrian number N in a queue, which are denoted as N_1, N_2 and N_3 in N-Queue (C), N-Queue (P), and E-Queue, respectively. As can be seen from Tab. 1 and Fig. 4 (a),

(i) At given μ, N_1, N_2 and N_3 increase monotonically with the increase of ρ, which is defined as ρ = λ/μ.

(ii) At given ρ, N_1 = N_2 = N_3 when μ → 0 (which implies λ → 0). With the increase of μ, N_1 remains unchanged, N_2 decreases and N_3 increases.

In N-Queue (C), in an infinitesimal time interval Δt, the arrival probability and the leaving probability are λΔt and μΔt, which tends to zero. Thus, changing λ and μ implies a rescaling of time interval, which does not change probability distribution of pedestrian number. Therefore, N_1 is independent of μ. In N-Queue (P), P (0) is independent of μ; however, since the common ratio in P (n) (_{1−μ} 1−ρμ ρ ) decreases with the increase of μ, P (n) becomes narrower and higher as in Fig. 4 (b).

Consequently, N_2 decreases as μ increases. In E-Queue, with the increase of μ, P (0) dramatically decreases as in Fig. 4 (b) and the common ratio r increases when ρ > 1/(2 + μ), so that P (n) becomes wider and lower; thus, N_3 increases. We would also like to explain this phenomenon intuitively. A pedestrian takes “the time of closing up” plus “the service time”, denoted as an “extended service time”, to go through the service window. When μ increases the extended service time does not sufficiently decrease since the time of closing up remains

Fig. 4. (a) Mean number of pedestrians N against the ratio between service and arrival time ρ. (b) Probability distributions of pedestrian number in a queue.

– 3 –

Fig. 5. Mean waiting time W against the mean service time 1/μ.

as a constant. At given ρ, the increase of μ implies the increase of λ, hence, N_3 increases as μ increases.

3.3 Mean Waiting Time in a Queue

Figure 5 shows the variation of W against 1/μ, which is a mean service time, in the case ρ is constant. With the increase of 1/μ, W increases linearly in N-Queue (C) and quasi-linearly in N-Queue (P), which coincides with our intuition. W also increases quasi-linearly in E- Queue when 1/μ is large; however, when 1/μ is small, it surprisingly achieves minimum W_{min}(= ρ/(1 − √ ρ)^2) at 1/μ_{min} (= ρ/(1 − √ ρ)), increases as 1/μ further decreases, and diverges at 1/μ_{cr} (= ρ/(1 − ρ)). Since the Little’s theorem N = λW [1] is satisfied in all three models, W = (1/μ)(N/ρ). At a given ρ, with the increase of 1/μ, N does not change in N-Queue (C) and increases in N-Queue (P), thus W increases in both cases. In contrast, N decreases with the increase of 1/μ in E-Queue, hence, the minimum could be reached.

As we have seen in Fig 5, E-Queue becomes similar to N-Queues when service time is large and different from it when service time is small. Thus, it is useful to know quantitatively when we should consider the excluded volume effect from the perspective of application. In Fig. 6, the ρ-μ plane is divided by the curve R = 1.1, where R is a ratio between W in N-Queue (C) and E-Queue described as R(ρ, μ) = W_{E-Queue}/W_{N-Queue (C)} In the lower-left region in Fig. 6 R < 1.1, and the difference of W is not critically large, so that it may be allowed to use N-Queue (C) for simple calculation when both ρ and μ are small. In contrast, R > 1.1 and the difference is crucial in the upper-right region, therefore, the excluded volume effect should be considered when both ρ and μ are large. Note that Fig. 6 is an example of the dividing curve, and it is possible to depict the other curves by determining R as a different value. Thus, this diagram is helpful to know the error quantitatively and make a decision whether to use N-Queue or E-Queue for designing a queueing system for pedestrians.

4. Conclusion

In this paper, we have newly introduced the excluded volume effect into the queueing model and obtained the

Fig. 6. Curve of R = 1.1 on the ρ − μ plane.

probability distributions and the means of the number of pedestrians and the waiting time exactly. Such physical quantities of the new model are compared with those of previous models which do not include the excluded volume effect. When the service time is large enough, all models become similar; however, when the service time becomes small, the time of closing up the queue dominates and the waiting time surprisingly increases in the excluded volume effect introduced queueing model. We also obtain the diagram to examine when the effect of the excluded volume effect becomes prominent.

To construct a more realistic model, the movement in the queue should be stochastic since pedestrians do not homogenously close up the queue. Furthermore, the length of a queue should be also calculated exactly, and the validity of the model should be verified by real experiments or observations in the near future.

Finally, we would like to mention that this work is financially supported by JSPS and JST.

References

[1] G. Bolch, S. Greiner, H. de Meer, and K. S. Trivedi, Queueing Networks and Markov Chains. A Wiley-Interscience Publication, U.S.A., 1998.

[2] D. Helbing, R. Jiang, and M. Treiber, Analytical investigation of oscillations in intersecting flows of pedestrian and vehicle traffic, Phys. Rev. E, 72, 046130, 2005.

[3] D. Helbing, M. Treiber, and A. Kesting, Understanding interarrival and interdeparture time statistics from interactions in queueing systems, Physica A, 363, 62–72, 2006.

[4] S. Kasahara, Internet Traffic Modeling -Towards Queueing Theory for the Internet Design-, TECHNICAL REPORT OF IEICE, 101(649), 25–30, 2002. (in Japanese).

[5] R. A. Blythe and M. R. Evans, Nonequilibrium steady states of matrix product form: A solver’s guide, J. Phys. A: Math. Gen., 40, R333, 2007.

[6] D. Chowdhury, L. Santen, and A. Schadschneider, Statistical physics of vehicular traffic and some related systems, Phys. Rep., 329, 199, 2000.

[7] D. Helbing, Traffic and related self-driven many-particle systems, Rev. Mod. Phys., 73, 1067–1141, 2001.

[8] C. Rogsch, A. Schadschneider, A. Seyfried, and W. Klingsch, How to Select the “Right One” - Update Schemes for Pedestrian Movementin Simulation and Reality, Traffic and Granular Flow ’09, to be published.

[9] D. Yanagisawa, et al, in preparation.

– 4 –