arXiv:1011.5726v1 [astro-ph.SR] 26 Nov 2010

Astron. Nachr. / AN XXX, No. X, 1 – 7 (2011) / DOI

The Tayler instability of toroidal magnetic fields in a columnar gallium experiment

G. Rüdiger^{1,2,⋆}, M. Schultz^1, and M. Gellert^1

1 Astrophysikalisches Institut Potsdam, An der Sternwarte 16, D-14482 Potsdam, Germany 2 Forschungszentrum Dresden Rossendorf, P.O. Box 510119, D-01314 Dresden, Germany

Received 2010, accepted 2010 Published online XXX

Key words instabilities – magnetohydrodynamics (MHD)

The nonaxisymmetric Tayler instability of toroidal magnetic fields due to axial electric currents is studied for conducting incompressible fluids between two coaxial cylinders without endplates. The inner cylinder is considered as so thin that even the limit of Rin → 0 can be computed. The magnetic Prandtl number is varied over many orders of magnitudes but the azimuthal mode number of the perturbations is fixed to m = 1. In the linear approximation the critical magnetic field amplitudes and the growth rates of the instability are determined for both resting and rotating cylinders. Without rotation the critical Hartmann numbers do not depend on the magnetic Prandtl number but this is not true for the growth rates. For given product of viscosity and magnetic diffusivity the growth rates for small and large magnetic Prandtl number are much smaller than those for Pm = 1. For gallium under the influence of a magnetic field at the outer cylinder of 1 kG the resulting growth time is 5 s. The minimum electric current through a container of 10 cm diameter to excite the kink-type instability is 3.20 kA. For a rotating container both the critical magnetic field and the related growth times are larger than for the resting column.

© 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim

1 Motivation

A known instability of toroidal fields is the current-driven (‘kink-type’) Tayler instability (TI) which is basically nonaxisymmetric (Tayler 1957; Vandakurov 1972; Tayler 1973; Acheson 1978). The toroidal field becomes unstable against nonaxisymmetric perturbations for a sufficiently large magnetic field amplitude depending on the radial profile of the field. A global rigid rotation of the system stabilizes the TI, i.e. much higher field amplitudes can be kept stable. For the rapidly rotating regime Ω > Ω_A (with Ω_A is the Alfvén frequency of the toroidal field) the stability becomes complete, i.e. all possible modes in incompressible fluids of uniform density are stable (Pitts & Tayler 1985). We shall demonstrate in the present paper how this instability and its stabilization by rigid rotation can experimentally be realized with fluid conductors like sodium or gallium. There is so far no empirical or observational proof of the existence of the TI (Maeder & Meynet 2005).

The stability problem of a system of toroidal fields and differential rotation has been studied in cylindric geometry (Michael 1954; Chandrasekhar 1961; Howard & Gupta 1962; Chanmugam 1979; Knobloch 1992: Dubrulle & Knobloch 1993; Kumar, Coleman & Kley 1994; Pessah & Psaltis 2005; Shalybkov 2006) but in all studies only axisymmetric perturbations are considered. Here as a continuation of the papers by Rüdiger et al. (2007a,b) and Rüdiger & Schultz (2010) the attention is focused to the nonaxisym-

⋆ Corresponding author: gruediger@aip.de

metric perturbation modes with m = 1 for real fluids. In particular, the possible realizations of the instabilities as an experiment laboratory in progress are discussed.

2 The Taylor-Couette geometry

A Taylor-Couette container is considered confining a toroidal magnetic field of given amplitudes at the cylinders which rotate with the common rotation rate Ω. We are here only interested in the hydrodynamically stable regime with rigid rotation. The gap between the cylinders is considered as so wide that also a column without any inner cylinder can be simulated. Formally, the inner radius is 100η̂ % of the outer radius. Extreme values of η̂ = 0.001 are used in the present paper contrary to the calculations by Rüdiger et al. (2007a) for a medium gap of η̂ = 0.5. The fluid between the cylinders is assumed to be incompressible with uniform density and dissipative with the kinematic viscosity ν and the magnetic diffusivity η.

The container possesses the inner and outer cylinder with radii R_{in} and R_{out} and with their ratio

η̂ =

R_{in} R_{out}

. (1)

The radial profiles of the magnetic background fields are restricted for real fluids. The solution of the stationary induction equation without shear reads

B_ϕ = AR + B R (2)

© 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim

in the cylinder geometry. A and B are the basic parameters; the term AR corresponds to uniform axial currents with I = 2A everywhere within R < R_{out}, and B/R corresponds to a uniform additional electric current only within R < R_{in}. In the present paper we generally put B = 0 (3) (see Roberts 1956; Pitts & Tayler 1985) with the consequence that the azimuthal magnetorotational instability (‘AMRI’, see Rüdiger 2007a) does not appear. The behavior of the toroidal field is thus only due to the TI for magnetic fields increasing outwards. It is useful to define the quantity

μ_B =

B_{out} B_{in}

, (4)

measuring the variation of B_ϕ across the gap. Vanishing B leads to μ_B = 1/η̂. In the following we fix μ_B = 1/η̂ but we shall vary the magnetic Prandtl number

Pm = ν η , (5)

and also the (small) values of η̂.

3 Equations and numerical model

The dimensionless MHD equations for incompressible fluids are Re ∂u ∂t + Re(u · ∇)u = −∇P + Δu + Ha^2 rot B × B, Rm ∂B ∂t = ΔB + Rm rot(u × B), (6)

with div u = div B = 0 and with the Hartmann number

Ha =

B_{in}D √ μ_0ρνη . (7)

Here D = √ R_{in}(R_{out} − R_{in}) is used as the unit of length, η/D as the unit of velocity and B_{in} as the unit of magnetic fields. Frequencies including the rotation rate Ω are normalized with the inner rotation rate Ω_{in}. The Reynolds number Re is defined as

Re =

ΩD^2 ν , (8)

and the magnetic Reynolds number is

Rm =

ΩD^2 η . (9)

Sometimes it appears as useful to work with the ‘mixed’ Reynolds number Rm^∗ = √ Re · Rm (10) which is symmetric in ν and η as it is also the Hartmann number. For Pm = 1 it is Re = Rm = Rm^∗. It is also useful to use the Lundquist number S = √ Pm Ha. The ratio of Rm^∗ and Ha,

Mm =

Rm^∗ Ha , (11)

is called the magnetic Mach number of rotation.

Applying the usual normal mode analysis, we look for solutions of the linearized equations of the form F = F (R) exp [ i(kz + mϕ + ωt) ] . (12) Using Eq. (12), linearizing the Eq. (6) and representing the result as a system of first order equations, one finds du_R dR + u_R R + i m R u_ϕ + iku_z = 0, dP dR + i m R ϕ_u + ikZ + ( k^2 + m^2 R^2 ) u_R +

+ iRe(ω + mΩ)u_R − 2ΩReu_ϕ − − iHa^2mAb_R + 2Ha^2Ab_ϕ = 0, dϕ_u dR − ( k^2 + m^2 R^2 ) u_ϕ − iRe(ω + mΩ)u_ϕ +

+ 2i m R^2 u_R − 2ReΩu_R +

+ 2Ha^2Ab_R + iHa^2mAb_ϕ − i m R P = 0, dZ dR + Z R − ( k^2 + m^2 R^2 ) u_z − iRe(ω + mΩ)u_z −

− ikP + iHa^2mAb_z = 0, db_R dR + b_R R + i m R b_ϕ + ikb_z = 0, db_z dR − i k ( k^2 + m^2 R^2 ) b_R + PmRe 1 k (ω + mΩ)b_R + + 1 k m R ϕ_B − 1 k mAu_R = 0, dϕ_B dR − ( k^2 + m^2 R^2 ) b_ϕ − iPmRe(ω + mΩ)b_ϕ + + i 2m R^2 b_R − Ru_R + imAu_ϕ = 0, (13)

where ϕ_u, Z and ϕ_B are defined as

ϕ_u = du_ϕ dR + u_ϕ R , Z = du_z dR , ϕ_B = db_ϕ dR + b_ϕ R , (14)

and A = 1/R_{in} (R_{in} in units of D).

An appropriate set of ten boundary conditions is needed to solve the system (13). For the velocity the boundary conditions are always no-slip while the cylinders are assumed to be perfect conductors. These boundary conditions are applied at both R_{in} and R_{out}. The wave number is varied as long as for given Hartmann number the Reynolds number takes its minimum. The procedure is described in detail by Shalybkov, Rüdiger & Schultz (2002). One immediately finds that the sign of the real wave number k is free so that with the solution for k also another one with −k exists. For insulating walls the boundary conditions are more complicated (see Rüdiger et al. 2007b).

Tayler (1973) found the necessary and sufficient condition d dR ( RB^2_ϕ ) < 0 (15)

for stability of an ideal nonrotating fluid against nonaxisymmetric disturbances. Our field profile B_ϕ = AR is thus stable against m = 0 and unstable for sufficiently large field

© 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim www.an-journal.org

Fig. 1 Top: the critical Hartmann number for very wide container gaps (η̂ → 0) between conducting and resting cylinders. The dotted line represents the profile (16) with H = 25. Bottom: note the high quality of the representation (16). Valid for all magnetic Prandtl numbers.

amplitudes, i.e. for Ha > Ha_{crit}. The same is true for the nearly uniform fields with μ_B ≃ 1. A general criterion for rotating flows does not exist.

The system (13) has been used to demonstrate that for resting cylinders the Ha_{crit} do not depend on the magnetic Prandtl number Pm (Rüdiger & Schultz 2010). Shalybkov (2006) has given a similar result for m = 0.

4 Resting container

In the present paper the radius of the inner cylinders is assumed as very small or even vanishing (η̂ ≪ 1). We have recently shown with similar models that indeed wide gaps are much more suitable for TI experiments with liquid metals like sodium or gallium than narrow gaps. The nonaxisymmetric modes which are excited by the Tayler instability in resting columnar containers do not rotate as their drift frequencies ℜ(ω) vanish.

4.1 Critical magnetic field amplitudes

The resulting Hartmann numbers Ha_{crit} for various η̂ are given in Fig. 1. They vary over many orders of magnitude and become very small for wide gaps (η̂ → 0). For small η̂ the critical Hartmann number vanishes like

Ha_{crit} = H η̂^{1.5}. (16)

Our calculations with the smallest R_{in} concern η̂ = 0.001 and provide Ha_{crit} = 0.00075 which leads to H ≃ 25 (see Fig. 1, bottom). For given H the relation (16) simply yields

B_{out} = H R_{out} √ ρμ_0νη. (17) for the critical magnetic field at the outer cylinder. Hence, the technical constraints to realize the TI in the laboratory working with liquid metals are the following. For a nonrotating container with R_{in} → 0 and R_{out} = 5 cm and for the gallium-tin alloy used in the experiment PROMISE ( √ ρμ_0νη = 25.7 in c.g.s.), Eq. (17) leads to B_{out} ≃ 128 G.

Now let I be the axial current inside the container, i.e.

B_{out} = I 5R_{out}

, (18)

where R, B and I are measured in cm, G, and A. Hence, for R_{in} → 0 the total current through the fluid conductor becomes 3.20 kA which is surprisingly small. We have thus shown that it should be possible to realize the nonaxisymmetric current-driven TI in the MHD laboratory also with conducting fluids of small magnetic Prandtl number such as sodium and gallium.

4.2 Growth rates

The other important parameter for the experiment is the growth rate of the instability. Contrary to the critical Hartmann numbers the growth rates for supercritical Hartmann numbers do depend on the magnetic Prandtl number. As it is not a mild dependence over many orders of magnitude of Pm a rather compact formulation is needed. We prefer a normalization of frequencies with the averaged diffusivity η^∗ = √ νη similar to the normalization of the magnetic field by the Hartmann number. Figure 2 shows the normalized growth rates

ω^∗ = ωD^2 η^∗ (19)

for various Ha and Pm. Note that even in this formulation the growth rates strongly vary over the range Pm = 1 . . . 10^{−6}. Fluids with equal values of ν and η are most unstable for fixed value of η^∗ (η^∗ = 2.9 cm^2/s for Gallistan, see below). The lower plot of Fig. 2 gives the values for various Pm but for fixed Ha. The curve takes its maximum for Pm = 1. Note that the growth rates for very small magnetic Prandtl numbers such as Pm = 10^{−6} are two orders of magnitudes smaller than they are for Pm = 1.

On the first view one takes from Fig. 2 that ω^∗ ≃ γHa which yields the relation ω_{gr} ≃ γ √ η̂Ω_A for the physical growth rate. Here the Alfvén frequency Ω_A is defined by

Ω_A =

B_{out} √ μ_0ρR_{out}

, (20)

and it is γ^<_∼ 4 for Pm = 1. Hence, for B_{out} = 1 kGauss and an outer radius of (say) R_{out} = 5 cm the growth rate is 20 s^{−1} so that the growth time is 0.05 s. For Pm = 10^{−6} (gallium) the value for γ is only 0.05 hence the growth time

www.an-journal.org © 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim

Fig. 2 Top: the growth rates of the instability for the resting container normalized with the diffusion time formed with the averaged diffusivity η^∗ = √ νη. Fluids (or simulations) with fixed η^∗ have maximum growth rates if Pm = 1. On the right vertical axis the curves are marked with their value of Pm. Bottom: the same but for the fixed Hartmann number Ha = 4. The ω^∗ for Pm = 10^{−6} is 0.2. It is η̂ = 0.05, μ_B = 20.

for B_{out} = 1 kG (!) with 4 s surprisingly long. Here and in the following the material quantities ρ = 6.4 g/cm^3 and η = 2428 cm^2/s for the gallium alloy GaInSn (“Gallistan”) are used.

However, the profiles in Fig. 2 are not linear. One finds that

ω^∗ = γ_ω (Ha − Ha_{crit})^2, (21)

gives a better representation where γ_ω depends on Pm rather than the value of Ha_{crit}. Neglecting the small values of the latter,

ω_{gr} = Γ_ω

B^2_{out} μ_0ρη (22)

Fig. 3 The parameter Γ_ω in Eq. (22) in its dependence on the inner radius η̂ and the magnetic Prandtl number Pm (marking numbers). The Pm-dependence disappears for small Pm. The values hold for all containers with small inner radius. For Pm = 1 it is Γ_ω = 0.0009.

is obtained for the physical growth rate. Here,

Γ_ω = η̂^2γ_ω √ Pm (23)

does no longer depend on the special (small) value of the geometry factor η̂. Even the limit η̂ → 0 is included.

A weak dependence on the magnetic Prandtl number remains. Figure 3 gives the numerical values of this quantity for various Pm. We find the limit Pm → 0 as possible. For fixed η we now find fluids with Pm = 1 as most stable while small or large viscosities are destabilizing.

For Pm = 10^{−6} we take from Fig. 3 the value Γ_ω = 0.041. Hence,

ω_{gr} = 2.0 ×10^{−3}B^2_{100} , (24)

which yields

τ_{gr} = 500 B^2_{100}

(25)

(with B_{100} = B_{out}/100 G) as the growth time in seconds for the TI in gallium experiments. The size of the container does no longer influence the growth rate. The growth time for B_{out} = 1 kG now results to 5 s – and to ∼2 min for, say, 200 G.

5 Rotating container

Figure 4 gives for the wide-gap container the rotational quenching of the TI for various values of the magnetic Prandtl number. The lines for marginal instability in the Rm^∗-Ha_{crit} plane are rather straight lines. The line for Pm = 1 gives the maximum stabilization by rigid rotation. In this representation a stronger stabilization does not exist.

© 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim www.an-journal.org

Fig. 4 The suppression of TI by uniform rotation for η̂ = 0.05. The curves are marked with their magnetic Prandtl numbers. In this representation fluids with Pm = 1 undergo the strongest stabilization by rotation. The critical Hartmann number for resting container is 0.31 for all Pm.

If Rm^{∗ <}_∼ 4 · Ha then all fluids are unstable even under the influence of rotation. Note that the rotational stabilization is much weaker for Pm ≠ 1. It is particularly weak for very small Pm.

We find from Fig. 4 that for fast rotation the magnetic Mach number (Eq. 11) is almost constant for given Pm (with minimum for Pm = 1) but still depends on the value of η̂. We then also find that the quantity M = √ η̂ Mm (26)

does no longer depend on η̂ but that it still slightly depends on Pm (Fig. 5). From Eq. (26) it results that

Ω = M Ω_A (27)

is the critical rotation rate which stabilizes the TI. Here, the Alfvén frequency (Eq. 20) of the outer magnetic field amplitude has been used.

The question is whether the rotational stabilization of the TI can be probed in the laboratory. The rigidly rotating wide-gap container with η̂ = 0.05 is thus considered also for the very small magnetic Prandtl numbers of fluid metals and for Reynolds numbers of order 10^3 where after Fig. 4 the bifurcation lines are no longer straight lines. The magnetic Prandtl number of sodium is about Pm = 10^{−5}, and for gallium it is about Pm = 10^{−6}. Without rotation the critical Hartmann number is 0.31 for this container (independent of Pm). With rotation the numerical results are given in Fig. 6. We find the rotational stabilization also existing for conducting fluids with their very small Pm. For not too fast rotation the differences of the resulting critical Ha are very small for both the fluid conductors so that experiments with gallium or sodium are possible. For the small Reynolds number of order 1000 the marginal-stable

Fig. 5 The same as in Fig. 4 but valid for η̂ → 0. Note that fluids with Pm = 1 can be stabilized with the smallest rotation rates.

Fig. 6 The suppression of the TI in a wide-gap container by rigid rotation for Pm = 10^{−5} and Pm = 10^{−6}. The standard Reynolds number (8) is given for experimental applications. The numerical values of the outer field strength and the critical rotation rates are given for experiments with Gallistan. η̂ = 0.05, μ_B = 20.

magnetic field is about two times higher than for Re = 0. With the density (ρ = 6.4 g/cm^3), viscosity (ν = 3.4×10^{−3} cm^2/s) and magnetic diffusivity (η = 2428 cm^2/s) for Gallistan the corresponding magnetic field amplitudes (at the outer cylinder) in Gauss and the rotation frequencies (in Hz) are also given in Fig. 6. The resulting values are moderate. It should thus not be too complicated to find the basic effect of the rotational suppression of TI also in the MHD laboratory.

Our linear code is also able to work with Pm = 0. The curves in Fig. 6 do not become more steep for Pm → 0. There is no visible difference between the curves for Pm = 10^{−6} and Pm = 0.

Figure 6 does not concern to a gallium column without inner cylinder. However, as demonstrated above the transi-

www.an-journal.org © 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim

Fig. 7 The parameter Γ_Ω for Pm = 10^{−5} (long line) and Pm = 10^{−6} (short line).

tion from η̂ = 0.05 to η̂ = 0 is easy. We take from Fig. 6 that close to the critical Hartmann number for resting container

Re = γ_Ω(Ha − Ha_{crit})^{2.5}. (28)

After the usual transformation to B_{out} one finds

Ω ≃ Γ_Ω (

B_{out} √ μ_0ρ

)^{5/2}

R^{1/2}_{out} Pm^{1/4}η^{3/2}

(29)

with Γ_Ω = η̂^{11/4} γ_ω. The result (29) also holds for η̂ → 0. Figure 7 shows the numerical values of Γ_Ω for the fluids with small magnetic Prandtl numbers.

Using the numerical result Γ_Ω ≃ 4 from Fig. 7 Eq. (29) yields

Ω ≃ 1.36 B^{2.5}_{100} [s^{−1}] (30)

for a container filled with Gallistan and with R_{out} = 5 cm or, what is the same, f = 0.22 B^{2.5}_{100} as the critical rotation frequency which marginally stabilizes the TI. Hence, for (say) 200 Gauss the limit frequency is 1.2 Hz. which is much faster in comparison to the container with η̂ = 0.05.

The influence of the rotation on the growth rates of the instability is only small. Figure 8 displays for Pm = 10^{−6} the normalized growth rates for Re = 0 (solid line) and Re = 1000 (dashed line). The stabilizing action of the basic rotation is obvious.

6 The magnetic field pattern

Without rotation the primary current-driven instability leads to a nondrifting steady-state solution. Isosurfaces of the pattern resulting from a 3D nonlinear simulation are shown in Fig. 9 for all the three field components. More details of the code which solves the incompressible MHD equations are given by Gellert et al. (2008). The boundary conditions at the walls are those for pseudovacuum. The container with η̂ = 0.05 is periodic in z-direction with a domain height of 2π(R_{out} −R_{in}). The Prandtl number Pm = 0.02 is the minimum value with which the code can operate. The Hartmann

Fig. 8 The normalized growth rates for Pm = 10^{−6} under the influence of rigid rotation with Re = 1000 (dashed). The solid line gives the growth rates for the resting container (see Fig. 2). Note the stabilizing action of global rotation. η̂ = 0.05, μ_B = 20.

number (Ha = 2) is supercritical with almost two times the critical value. The dominating modes with m = ±1 lead to a kidney-shaped pattern. Note the different azimuthal angles of the pattern of the azimuthal component compared to the others.

From linear calculations we know that for smaller Pm the axial wave numbers decrease and the pattern extensions in axial direction become larger.

The secondary bifurcation leads to axial oscillations around half the wavelength. To what extent this picture holds for Pm = 10^{−6} is open. Because of the Pmindependent critical Ha and the only slightly larger Hartmann number used in the simulations shown here, it is possible that liquid metal experiments behave nearly the same.

7 A short review

The interplay of toroidal magnetic fields and solid-body rotation for incompressible fluids of uniform density filling the gap between the cylinders of a Taylor-Couette container is considered. The toroidal field is the result of an electric axial current of homogeneous density. It is shown that for zero rotation the critical magnetic field amplitudes for marginal Tayler instability do not depend on the magnetic Prandtl number. The critical magnetic field at the inner cylinder strongly depends on the gap width. It is very high for small gaps and it this rather low for wide gaps. For small enough inner radius R_{in} the critical Hartmann number (of the inner field strength) runs as R^{1.5}_{in} . Note, however, that the critical magnetic field at the outer cylinder does hardly vary with the gap width (see Eq. 17). The resulting elec-

© 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim www.an-journal.org

Fig. 9 (online colour at: www.an-journal.org) Isosurface plots of all field components. The outermost visible surface represents 25 % of the maximum value. Re = 0, Ha = 2, η̂ = 0.05, μ_B = 20, Pm = 0.02.

tric currents necessary for TI with |m| = 1 slightly exceeds 3.2 kA if the material is the same gallium-tin alloy (GaInSn) as used in the experiment PROMISE. Such currents can easily be produced in the laboratory. The main difficulty for experiments is given by the long growth times of the instability for magnetic fields weaker than 1 kG.

Also the rotational quenching of the TI is studied. Figure 4 shows the rotational stabilization for various magnetic Prandtl numbers. To normalize the basic rotation a ‘mixed’ Reynolds number (Eq. 10) is used in which – as in the Hartmann number – the viscosities ν and η are symmetric. The ratio of this Reynolds number and the Hartmann number (i.e. the magnetic Mach number) is free of any diffusivity. This ratio describes the rotational quenching of TI for various Pm. It is shown that the most effective stabilization of TI happens for Pm = 1. It is weaker for both smaller Pm and higher Pm. Many numerical simulations with Pm ≃ 1, therefore, could overlook the nonaxisymmetric instability of strong toroidal fields.

Our calculations demonstrate that rigid rotation always stabilizes the magnetic field against the nonaxisymmetric TI. We have also shown that this rotational stabilization should be observable in the laboratory. Figure 6 provides the result that the critical Hartmann number in a wide-gap container of η̂ = 0.05 can be increased by a factor of two by a rigid rotation of only a few Hz.

Acknowledgements. Many discussion with Frank Stefani and Gunter Gerbeth (both FZD) are cordially acknowledged about the theory of the current-driven instability and its experimental realization.

References

Acheson, D.J.: 1978, Phil. Trans. R. Soc. London A 289, 459 Chandrasekhar, S.: 1961, Hydrodynamic and Hydromagnetic Stability, Clarendon Press, Oxford Chanmugam, G.: 1979, MNRAS 187, 769 Dubrulle, B., Knobloch, E.: 1993, A&A 274, 667 Howard, L.N., Gupta, A.S.: 1962, JFM 14, 463 Knobloch, E.: 1992, MNRAS 255, 25 Kumar, S., Coleman, C.S., Kley, W.: 1994, MNRAS 266, 379 Maeder, A., Meynet, G.: 2005, A&A 440, 1041 Michael, D.H.: 1954, Mathematika 1, 45 Pessah, M.E., Psaltis, D.: 2005, ApJ 628, 879 Pitts, E., Tayler, R.J.: 1985, MNRAS 216, 139 Roberts, P.H.: 1956, ApJ 124, 430 Rüdiger, G., Schultz, M.: 2010, AN 331, 121 Rüdiger, G., Hollerbach, R., Schultz, M., Elstner, D.: 2007a, MN- RAS 377, 1481 Rüdiger, G., Schultz, M., Shalybkov, D., Hollerbach, R.: 2007b, Phys. Rev. E 76, 056309 Shalybkov, D.: 2006, Phys. Rev. E 73, 016302 Shalybkov, D., Rüdiger, G., Schultz, M.: 2002, A&A 395, 339 Tayler, R.J.: 1957, Proc. Phys. Soc. B 70, 31 Tayler, R.J.: 1973, MNRAS 161, 365 Vandakurov, Yu.V.: 1972, SvA 16, 265

www.an-journal.org © 2011 WILEY-VCH Verlag GmbH & Co. KGaA, Weinheim