arXiv:1206.6918v1 [cs.IT] 29 Jun 2012

Source-Channel Coding for the Multiple-Access Relay Channel

Yonathan Murin, Ron Dabora Department of Electrical and Computer Engineering Ben-Gurion University, Israel Email: moriny@bgu.ac.il, ron@ee.bgu.ac.il

Deniz Gündüz Centre Tecnologic de Telecomunicacions de Catalunya (CTTC), Barcelona, Spain Email: deniz.gunduz@cttc.es

Abstract—This work considers reliable transmission of general correlated sources over the multiple-access relay channel (MARC) and the multiple-access broadcast relay channel (MABRC). In MARCs only the destination is interested in a reconstruction of the sources, while in MABRCs both the relay and the destination want to reconstruct the sources. We assume that both the relay and the destination have correlated side information. We find sufficient conditions for reliable communication based on operational separation, as well as necessary conditions on the achievable source-channel rate. For correlated sources transmitted over fading Gaussian MARCs and MABRCs we find conditions under which informational separation is optimal.

I. INTRODUCTION The multiple-access relay channel (MARC) is a network in which several users communicate with a single destination with the help of a relay [1]. Examples of such a network are sensor and ad-hoc networks in which an intermediate relay can be added to assist communication from the sources to the destination. Achievable regions for the MARC were derived in [2], [3] and [4]. In [2] Kramer et al. derived an achievable rate region for the MARC with independent sources. The coding scheme employed in [2] is based on decode-and-forward (DF) relaying, and uses regular encoding, successive decoding at the relay and backward decoding at the destination. In [3], another DF-based coding scheme for the MARC was presented. The work [3] also showed that, in contrast to DF for the classic relay channel, for the MARC different DF schemes yield different rate regions (backward decoding can yield larger rates than sliding window decoding). Outer bounds on the capacity of discrete memoryless (DM) MARCs were obtained in [4].

The previous work on MARCs considered independent messages at the terminals. In contrast, in the present work here we allow arbitrary correlation among the sources that should be transmitted to the destination in a lossless fashion.

In [5] Shannon showed that a source can be reliably transmitted over a memoryless point-to-point (PtP) channel, if and only if its entropy is less than the channel capacity. Hence, a simple comparison of the rates of the optimal source and channel codes for the respective source and channel suffices to conclude if reliable communication is feasible. This is called the separation theorem. The implication of the separation theorem is that independent design of the source and channel codes is optimal.

This work was supported by the European Commission’s Marie Curie IRG Fellowship PIRG05-GA-2009-246657 under the Seventh Framework Programme.

In [6] Shamai and Verdu considered the availability of correlated side information at the receiver in a PtP scenario, and showed that source-channel separation is optimal. The availability of receiver side information enables transmitting the source reliably over a channel with a smaller capacity compared to the capacity needed in the absence of receiver side information.

Unfortunately, optimality of source-channel separation in the Shannon sense does not generalize to multiuser networks [7], [8], [9]. Therefore, in general the source and channel codes must be jointly designed for every particular source and channel combination. Source-channel coding over the broadcast channel was considered by Tuncel in [10]. Tuncel distinguishes between two types of source-channel separation. Informational separation refers to classical separation in the Shannon sense. Operational separation refers to statistically independent source and channel codes that are not necessarily the optimal codes for the underlying source or the channel. In [10] Tuncel showed that for a broadcast channel in which each receiver has a different side information, operational separation is optimal, while informational separation is not.

Optimizing source coding along with multiuser channel coding in a general setting is a very complicated task. In [11] Tian et al. showed the optimality of operational separation for the following two scenarios: a) arbitrarily correlated sources over orthogonal links; b) independent sources over a general network with some restrictions on how many messages can be decoded at each destination. In [9] Gündüz et al. obtained necessary and sufficient conditions for the optimality of informational separation for the multiple-access channel with correlated sources and side information. Gündüz et al. also obtained necessary and sufficient conditions for the optimality of operational separation for the compound multiple-access channel with correlated sources and side information. In [12] Gündüz and Erkip showed that operational separation is optimal for the cooperative relay-broadcast channel. Necessary and sufficient conditions for reliable transmission of a source over a relay channel when side information is available either only at the receiver, or only at the relay or at both the relay and the receiver were established in [13].

In this paper we shall also consider MARCs and MABRCs subject to independent and identically distributed (i.i.d.) fading, for both phase and Rayleigh fading. Phase fading models apply to high-speed microwave communications where the oscillator’s phase noise and the system timing jitter are the key impairments. Phase fading is also the major impairment in communication systems that employ orthogonal frequency division multiplexing , as well as in some applications of naval communications. Rayleigh fading models are very common in wireless communications and apply to mobile communications in the presence of multiple scatterers without line-of-sight. The key similarity between the two models is the uniformly distributed phase of the fading process. The phase fading and Rayleigh fading models differ in the behaviour of the fading magnitude component, which is fixed for the former but varies following a Rayleigh distribution for the latter. Main Contributions

In this paper we establish a DF-based achievable sourcechannel rate for the MARC with correlated sources and with side information at the relay and the destination. The scheme uses irregular encoding, successive decoding at the relay and backward decoding at the destination. We show that for the MARC with correlated sources and side information, irregular encoding yields a higher achievable source-channel rate than the rate achieved by regular encoding. This rate also applies directly to the MABRC. We then derive necessary conditions on the achievable source-channel rate of MARCs (and MABRCs) with correlated sources and side information.

Next, we consider transmission of correlated sources over fading MARCs and MABRCs with side information at the relay and at the destination. Using the necessary conditions on the achievable source-channel rate of the MARC that we derive here, the capacity region of the MARC obtained in [2, Thm. 9], and the results presented in [14, Section III.C], we find conditions for correlated sources transmitted over phase fading MARCs with side information, under which informational separation is optimal. Optimality conditions are also obtained for Rayleigh fading MARCs with correlated sources and side information. Additionally, we find conditions for the optimality of separation for fading MABRCs. This is the first time the optimality of separation is shown for the MARC and the MABRC models. Note that these models are not degraded in the sense of [15], see also [2, Remark 33].

The rest of this paper is organized as follows: in Section II the model and notations are presented. In Section III the separation based achievable source-channel rate is presented as well as necessary conditions on the achievable source-channel rate. The optimality of separation for correlated sources transmitted over fading Gaussian MARCs is studied in Section IV. II. NOTATIONS AND MODEL In the following we use H(·) to denote the entropy of a discrete random variable and I(·; ·) to denote the mutual information between two random variables, as defined in [16, ch. 2, ch. 9]. We denote the set of real numbers with R, and we use C to denote the set of complex numbers. We denote random variables with upper case letters, e.g., X, Y , and their realizations with lower case letters x, y. A discrete random variable X takes values in a set X . We use p_X (x) to denote the probability mass function (p.m.f.) of a discrete RV X on X , and f_X (x) to denote the probability density function (p.d.f.) of a continuous RV X on C. For brevity we may omit the subscript X when it is the uppercase version of the sample symbol x. We use p_{X|Y} (x|y) to denote the conditional distribution of X given Y . We use X^j to denote the vector (X_1, X_2, . . . , X_j ). We denote the empty set with ϕ, and the complement of the set B by B^c. We use A^{∗(n)}ϵ (X) to denote the set of ϵ-strongly typical sequences with respect to distribution p_X (x) on X , CN (a, σ^2) to denote a proper, circularly symmetric, complex Normal distribution with mean a and variance σ^2, and E{·} to denote stochastic expectation.

The MARC consists of two transmitters (sources), a receiver (destination) and a relay. Transmitter i has access to the source sequence S^m_i , for i = 1, 2. The receiver is interested in the lossless reconstruction of the source sequences observed by the two transmitters. The objective of the relay is to help the receiver decode the source sequences. It is also assumed that the relay and the receiver have side information correlated with the source sequences. For the MABRC both the receiver and the relay are interested in a lossless reconstruction of the source sequences. Figure 1 depicts the MABRC with side information setup.

Fig. 1. Multiple-access broadcast relay channel with correlated side information. (Ŝ^m_{1,3}, Ŝ^m_{2,3}) are the reconstructions of (S^m_1 , S^m_2 ) at the relay, and (Ŝ^m_1 , Ŝ^m_2 ) are the reconstructions at the destination .

The sources and the side information sequences, {S_{1,k}, S_{2,k}, W_k, W_{3,k}}^m_{k=1}, are arbitrarily correlated according to a joint distribution p(s_1, s_2, w, w_3) over a finite alphabet S_1 × S_2 × W × W_3, and independent across different sample indexes k. All nodes know this joint distribution.

For transmission, a discrete memoryless channel with inputs X_1, X_2, X_3 over finite input alphabets X_1, X_2, X_3, and outputs Y, Y_3 over finite output alphabets Y, Y_3, is available. The channel is memoryless in the sense p(y_k, y_{3,k}|y^{k−1}, y^{k−1}_3 , x^k_1 , x^k_2 , x^k_3 ) = p(y_k, y_{3,k}|x_{1,k}, x_{2,k}, x_{3,k}). An (m, n) source-channel code for the MABRC with correlated side information consists of two encoding functions at the transmitters: f^{(m,n)}_i : S^m_i → X^n_i , i = 1, 2, and two decoding functions at the destination and the relay: g^{(m,n)} : Y^n × W^m → S^m_1 × S^m_2 , g^{(m,n)}_3 : Y^n_3 × W^m_3 → S^m_1 × S^m_2 . Finally, there is a causal encoding function at the relay, x_{3,k} = f^{(m,n)}_{3,k} (y^{k−1}_{3,1} , w^m_{3,1}), 1 ≤ k ≤ n. Note that in the MARC scenario the decoding function g^{(m,n)}_3 does not exist. Let Ŝ^m_i denote the reconstruction of S^m_i , i = 1, 2, respectively, at the receiver. Let Ŝ^m_{i,3} denote the reconstruction of S^m_i , i = 1, 2, respectively, at the relay. The average probability of error, P^{(m,n)}e , of an (m, n) code for the MABRC is defined as P^{(m,n)}_e ≜ Pr ( (Ŝ^m_1 , Ŝ^m_2 ) ≠ (S^m_1 , S^m_2 ) or (Ŝ^m_{1,3}, Ŝ^m_{2,3}) ≠ (S^m_1 , S^m_2 ) ) , while for the MARC the average probability of error is defined as P^{(m,n)}_e ≜ Pr ( (Ŝ^m_1 , Ŝ^m_2 ) ≠ (S^m_1 , S^m_2 ) ) . A source-channel rate κ is said to be achievable for the MABRC, if for every ϵ > 0 there exist positive integers n_0, m_0 such that for all n > n_0, m > m_0, n/m = κ, there exists an (m, n) code for which P^{(m,n)}e < ϵ. The same definition applies to the MARC.

For fading Gaussian MARCs and MABRCs, the received signals at time k at the receiver and at the relay are given by (see Figure 2)

Y_k = H_{11,k}X_{1,k} + H_{21,k}X_{2,k} + H_{31,k}X_{3,k} + Z_k (1a) Y_{3,k} = H_{13,k}X_{1,k} + H_{23,k}X_{2,k} + Z_{3,k}, (1b)

Fig. 2. Transmission of correlated sources over the fading Gaussian MARC with side information at the relay and at the destination (additive noises are not depicted).

k = 1, 2, . . . , n, where Z and Z_3 are independent of each other, i.i.d., circularly symmetric, complex Normal RVs, CN (0, 1). The channel input signals are subject to per-symbol average power constraints: E{|X_i|^2} ≤ P_i, i = 1, 2, 3. In the following it is assumed that the destination knows the instantaneous channel coefficients from Transmitter i, i = 1, 2, and from the relay to itself, and the relay knows the instantaneous channel coefficients from both transmitters to itself. This is referred to as receiver channel state information (Rx- CSI). For phase fading channels the channel coefficients are given by H_{li,k} = a_{li}e^{jΘli,k} , where a_{li} ∈ R are constants representing the attenuation and Θ_{li,k} are uniformly distributed over [0, 2π), i.i.d., and independent of each other and of the additive noises Z_3 and Z. For Rayleigh fading channels the channel coefficients are given by H_{li,k} = a_{li}U_{li,k} , a_{li} ∈ R are constants representing the attenuation, and U_{li,k} are circularly symmetric, complex Normal RVs, U_{li,k} ∼ CN (0, 1), i.i.d., and independent of each other and of the additive noises Z_3 and Z.

III. SOURCE-CHANNEL CODING FOR DISCRETE MEMORYLESS MARCS AND MABRCS A. Operational Separation-Based Achievable Rate In this subsection we present an achievable rate for MARCs and MABRCs with correlated sources and side information, based on operational separation.

Theorem 1. For DM MARCs and DM MABRCs with relay and receiver side information as defined in Section II, sourcechannel rate κ is achievable if,

H(S_1|S_2, W_3) < κI(X_1; Y_3|X_2, V_1, X_3) (2a) H(S_2|S_1, W_3) < κI(X_2; Y_3|X_1, V_2, X_3) (2b) H(S_1, S_2|W_3) < κI(X_1, X_2; Y_3|V_1, V_2, X_3) (2c) H(S_1|S_2, W ) < κI(X_1, X_3; Y |X_2, V_2) (2d) H(S_2|S_1, W ) < κI(X_2, X_3; Y |X_1, V_1) (2e) H(S_1, S_2|W ) < κI(X_1, X_2, X_3; Y ), (2f) for an input distribution that factors as

p(s_1, s_2, w_3, w)p(v_1)p(x_1|v_1)p(v_2)p(x_2|v_2)p(x_3|v_1, v_2). Proof outline: The achievability is established by using two independent Slepian-Wolf source coding schemes [16, Section 14.4], and a channel coding scheme similar to the one detailed in [3, Sections II, III]. The channel coding scheme employs a DF code with irregular block Markov encoding, successive decoding at the relay, and backward decoding at the destination. Detailed proof is provided in [17]. B. Discussion

In Thm. 1, bounds (2a)–(2c) are constraints for decoding at the relay, while bounds (2d)–(2f) are constraints for decoding at the destination. The source-channel achievable rate of Thm. 1 is established by using two different Slepian-Wolf coding schemes: one for the relay and one for the destination. This requires an irregular encoding scheme for the channel code. In regular encoding, the codebooks at the source and the relay have the same size, see for example [3]. Applying regular encoding to MABRCs with correlated sources and side information leads to merging some of the constraints in (2). In particular (2a) and (2d) will be combined into the constraint max { H(S_1|S_2, W_3), H(S_1|S_2, W ) } < κ min { I(X_1; Y_3|X_2, V_1, X_3), I(X_1, X_3; Y |X_2, V_2) } . For irregular encoding, bounds (2a) and (2d) need not be combined, since the transmission rates to the relay and to the destination can be different due to different quality of the side information. We conclude that for MABRCs with correlated sources and side information, irregular encoding yields a higher source-channel achievable rate than the one achieved by regular encoding. When the relay and destination have the same side information (W =W_3) then the irregular and regular schemes obtain the same achievable source-channel rates.

We note that when using regular encoding for MARCs, there is a single Slepian-Wolf code, hence, in the scheme used in Thm. 1 it is not required to recover the source sequences at the relay and the right-hand side (RHS) of the constraints (2a)–(2f) can be combined. For example, (2a) and (2d) will be combined into the constraint

H(S_1|S_2, W ) < κ min { I(X_1; Y_3|X_2, V_1, X_3), I(X_1, X_3; Y |X_2, V_2) } . C. Necessary Conditions on the Achievable Source-Channel Rate

In this subsection we present necessary conditions on the achievable source-channel rate for MARCs and for MABRCs with correlated sources and side information at the relay and at the destination.

Proposition 1. Consider the transmission of arbitrarily correlated sources S_1 and S_2 over the DM MARC with relay side information W_3 and receiver side information W . Any achievable source-channel rate κ must satisfy the constraints: H(S_1|S_2, W ) ≤ κI(X_1, X_3; Y |X_2) (3a) H(S_2|S_1, W ) ≤ κI(X_2, X_3; Y |X_1) (3b) H(S_1, S_2|W ) ≤ κI(X_1, X_2, X_3; Y ), (3c) for some input distribution p(x_1, x_2, x_3). Proof: A detailed proof is provided in [17].

Remark 1. Setting X_2 = S_2 = ϕ, Proposition 1 specializes to the converse of [12, Thm. 3.1] for the relay channel. Proposition 2. Consider the transmission of arbitrarily correlated sources S_1 and S_2 over the DM MABRC with relay side information W_3 and receiver side information W . Any achievable source-channel rate κ must the satisfy the constraints in (3) as well as the following constraints:

H(S_1|S_2, W_3) ≤ κI(X_1; Y_3|X_2, X_3) (4a) H(S_2|S_1, W_3) ≤ κI(X_2; Y_3|X_1, X_3) (4b) H(S_1, S_2|W_3) ≤ κI(X_1, X_2; Y_3|X_3), (4c) for some input distribution p(x_1, x_2, x_3). Proof: A detailed proof is provided in [17].

IV. OPTIMALITY OF SOURCE-CHANNEL SEPARATION FOR FADING GAUSSIAN MARCS AND MABRCS We begin by considering source-channel separation for phase fading Gaussian MARCs (1). The result is stated in the following theorem.

Theorem 2. Consider the transmission of arbitrarily correlated sources S_1 and S_2 over a phase fading Gaussian MARC with receiver side information W and relay side information W_3. Let the channel inputs be subject to per-symbol power constraints E{|X_i|^2} ≤ P_i, i = 1, 2, 3, and let the channel coefficients and the channel input powers satisfy a^2_{11}P_1 + a^2_{31}P_3 ≤ a^2_{13}P_1 (5a) a^2_1P_2 + a^2_{31}P_3 ≤ a^2_3P_2 (5b) a^2_{11}P_1 + a^2_1P_2 + a^2_{31}P_3 ≤ a^2_{13}P_1 + a^2_3P_2. (5c) A source-channel rate κ is achievable if

H(S_1|S_2, W ) < κ log_2(1 + a^2_{11}P_1 + a^2_{31}P_3) (6a) H(S_2|S_1, W ) < κ log_2(1 + a^2_1P_2 + a^2_{31}P_3) (6b) H(S_1, S_2|W ) < κ log_2(1 + a^2_{11}P_1 + a^2_1P_2 + a^2_{31}P_3).(6c)

Conversely, if source-channel rate κ is achievable, then conditions (6) are satisfied with < replaced by ≤. Proof: See subsections IV-A, IV-B.

Remark 2. The source-channel rate κ in Thm. 2 is achieved by using X_i ∼ CN (0, P_i), i ∈ {1, 2, 3}, all i.i.d. and independent of each other, and applying DF at the relay.

Remark 3. The achievability scheme of Thm. 2 uses the channel code construction and decoding rules detailed in [14, Section III.C]. The decoding rules detailed in [14, Section III.C] imply that the destination channel decoder does not use any information provided by the destination source decoder. The only interaction between the source code and channel code is through the bin indices of the transmitted sequences. Hence, Thm. 2 implies that informational separation is optimal.

Next, we consider sources transmission over Rayleigh fading MARCs.

Theorem 3. Consider the transmission of arbitrarily correlated sources S_1 and S_2 over a Rayleigh fading Gaussian MARC with receiver side information W and relay side information W_3. Let the channel inputs be subject to per-symbol power constraints E{|X_i|^2} ≤ P_i, i = 1, 2, 3, and let the channel coefficients and the channel input powers satisfy

1 + a^2_{11}P_1 + a^2_{31}P_3 ≤ a^2_{13}P_1

e^{1a2}13^{P1} E_1

(_1

a^2_{13}P_1

) (7a)

1 + a^2_1P_2 + a^2_{31}P_3 ≤ a^2_3P_2

e^{1a2}3^{P2} E_1

(_1

a^2_3P_2

) (7b)

1 + a^2_{11}P_1 + a^2_1P_2 + a^2_{31}P_3 ≤

a^2_3P_2 − a^2_{13}P_1 ( e^{1a2}3^{P2} E_1

(_1

a^2_3P_2 ) − e^{1a2}13^{P1} E_1

(_1

a^2_{13} P_1 )) , (7c)

where E_1(x) ≜ ∫_∞ q=x 1 q e^{−q}dq. A source-channel rate κ is achievable if

H(S_1|S_2, W ) < κE_Ũ { log_2(1 + a^2_{11}|U_{11}|^2P_1

+ a^2_{31}|U_{31}|^2P_3) } (8a) H(S_2|S_1, W ) < κE_Ũ { log_2(1 + a^2_1|U_{21}|^2P_2

+ a^2_{31}|U_{31}|^2P_3) } (8b) H(S_1, S_2|W ) < κE_Ũ { log_2(1 + a^2_{11}|U_{11}|^2P_1+ a^2_1|U_{21}|^2P_2 + a^2_{31}|U_{31}|^2P_3) } , (8c)

where Ũ = ( U_{11}, U_{13}, U_{21}, U_{23}, U_{31} ) . Conversely, if sourcechannel rate κ is achievable, then conditions (8) are satisfied with < replaced by ≤.

Proof: The proof uses [14, Corollary B.1] and follows similar arguments to those in the proof of Thm. 2.

Remark 4. The source-channel rate κ in Thm. 3 is achieved by using X_i ∼ CN (0, P_i), i ∈ {1, 2, 3}, all i.i.d. and independent of each other, and applying DF at the relay.

A. Achievability Proof of Thm. 2

1) Code construction: For i=1, 2, assign every s_i ∈ S^m_i to one of 2^{mRi} bins independently according to a uniform distribution on {1, 2, . . . , 2^{mRi} }. Denote these assignments by f_i. A channel code based on DF with rates R̂_1 and R̂_2, and a blocklength n, is constructed as detailed in [14, Section III.C]. Transmitter i has 2^{nR̂i} messages, thus we require κR̂_i = R_i.

2) Encoding: Consider a source sequence of length Bm, s^{Bm}_i ∈ S^{Bm}_i , i = 1, 2. Partition this sequence into B lengthm subsequences, s_{i,b}, b = 1, 2, . . . , B. Similarly partition the side information sequence w^{Bm} ∈ W^{Bm}, into B length-m subsequences. We transmit a total of Bm source samples over B + 1 blocks of n channel uses each. If we set n = κm, by increasing B we obtain a source-channel rate (B+1)n/Bm → n/m = κ as B → ∞.

In block b, b = 1, 2, . . . , B, source terminal i, i = 1, 2, observes s_{i,b} and finds its corresponding bin index u_{i,b} ∈ {1, 2, . . . , 2^{mRi} }. Each transmitter sends its corresponding bin index using the channel code described in [14, Section III.C].

Encoding at the relay: Assume that at time b the relay knows (u_{1,b−1}, u_{2,b−1}). The relay sends these bin indices using the channel code described in [14, Section III.C].

3) Decoding and error probability: Conditions (5) imply that the achievable channel rate region for decoding at the relay contains the achievable channel rate region for decoding at the destination. Hence, reliable decoding of the channel code at the destination implies reliable decoding of the channel code at the relay. When the channel coefficients and the channel input powers satisfy conditions (5), the RHS of constraints (6) is the capacity region of the phase fading Gaussian MARC, (see [2, Thm. 9]). Hence, the transmitted bin indices {u_{1,b}, u_{2,b}}^B_{b=1} can be reliably decoded at the destination if R_1 ≤ κ log_2(1 + a^2_{11}P_1 + a^2_{31}P_3) (9a) R_2 ≤ κ log_2(1 + a^2_1P_2 + a^2_{31}P_3) (9b) R_1 + R_2 ≤ κ log_2(1 + a^2_{11}P_1 + a^2_1P_2 + a^2_{31}P_3). (9c) Decoding the sources at the destination: The decoded bin indices, denoted ũ_{i,b}, i=1, 2, b=1, 2, . . . , B, are then given to the source decoder at the destination. Using the bin indices and the side information w_b, the source decoder at the destination estimates s_{1,b}, s_{2,b}. More precisely, given the bin indices ũ_{1,b}, ũ_{2,b}, it declares (s̃_{1,b}, s̃_{2,b}) to be the decoded sequences if it is the unique pair of sequences that satisfies f_1(s̃_{1,b}) = ũ_{1,b}, f_2(s̃_{2,b}) = ũ_{2,b} and (s̃_{1,b}, s̃_{2,b}, w_b) ∈ A^{∗(m)}ϵ (S_1, S_2, W ). From the Slepian-Wolf theorem [16, Thm 14.4.1], (s_{1,b}, s_{2,b}) can be reliably decoded at the destination if H(S_1|S_2, W ) < R_1 (10a) H(S_2|S_1, W ) < R_2 (10b) H(S_1, S_2|W ) < R_1 + R_2. (10c) Combining conditions (9) and (10) yields (6) and completes the achievability proof. B. Converse Proof of Thm. 2

Consider the necessary conditions of Proposition 1. From [2, Thm. 8] it follows that for phase fading with Rx-CSI, the mutual information expressions on the RHS of (3) are simultaneously maximized by X_1, X_2, X_3 independent, zeromean complex Normal, X_i ∼ CN (0, P_i), i = 1, 2, 3 yielding the same expressions as in (6). Therefore, for phase fading MARCs, when conditions (5) hold, the conditions in (6) coincide with the necessary conditions of Proposition 1, and the conditions in (6) are satisfied with ≤ instead of <. C. Fading MABRCs

The optimality of informational separation can be established for MABRCs using the results for the MARC with additional constraints, as indicated in the following theorem: Theorem 4. For phase fading MABRCs for which the conditions in (5) hold together with H(S_1|S_2, W_3) ≤ H(S_1|S_2, W ) (11a) H(S_2|S_1, W_3) ≤ H(S_2|S_1, W ) (11b) H(S_1, S_2|W_3) ≤ H(S_1, S_2|W ), (11c) the maximum achievable source-channel rate κ satisfies (6). The same statement holds for Rayleigh fading MABRCs with (7) replacing (5) and (8) replacing (6).

Remark 5. Conditions (11) imply that for the scenario described in Thm. 2 regular encoding and irregular encoding yield the same source-channel achievable rates (see discussion in Section III-B), hence the channel code construction of [14, Section III.C] can be used.

Remark 6. The proof for MABRCs differs from the achievability proof of section IV-A only due to decoding the source sequences at the relay. This decoding follows similar arguments to the decoding of the sources at the destination. Conditions (11) imply that reliable decoding of the sources at the destination guarantees reliable decoding of the sources at the relay, since the relay achievable source rate region contains the destination achievable source rate region. REFERENCES

[1] G. Kramer and A. J. Wijnngaarden. “On the white Gaussian multipleaccess relay channel”. Proc. IEEE Int. Symp. Inform. Theory, Sorrento, Italy, Jun. 2000, p. 40.

[2] G. Kramer, M. Gastpar, and P. Gupta. “Cooperative strategies and capacity theorems for relay networks”. IEEE Trans. Inform. Theory, vol. 51, no. 9, pp. 3037–3063, Sep. 2005.

[3] L. Sankar, G. Kramer, and N. B. Mandayam. “Offset encoding for multiaccess relay channels”. IEEE Trans. Inform. Theory, vol. 53, no. 10, pp. 3814–3821, Oct. 2007.

[4] L. Sankaranarayanan, G. Kramer, and N. B. Mandayam. “Capacity theorems for the multiple-access relay channel”. Proc. 42nd Annu. Allerton Conf. Communications, Control, and Computing, Monticello, IL, Sep. 2004, pp. 1782–1791.

[5] C. E. Shannon. “A mathematical theory of communication”. Bell Syst.

Tech. J., vol. 27, pp. 379–423 and pp. 623–656, 1948.

[6] S. Shamai and S. Verdu. “Capacity of channels with side information”.

European Transactions on Telecommunications and Related Technologies, vol. 6, no. 5, pp. 587–600, Sep. 1995.

[7] C. E. Shannon. “Two-way communication channels”. Proc. 4th Berkeley Symp. Math. Statist. and Prob., vol. 1, pp. 611–644, 1961.

[8] T. M. Cover, A. El Gamal, and M. Salehi. “Multiple access channels with arbitrarily correlated sources”. IEEE Trans. Inform. Theory, vol. 26, no. 6, pp. 648–657, Nov. 1980.

[9] D. Gündüz, E. Erkip, A. Goldsmith, and H. V. Poor. “Source and channel coding for correlated sources over multiuser channels”. IEEE Trans. Inform. Theory, vol. 55, no. 9, pp. 3927–3944, Sep. 2009.

[10] E. Tuncel. “Slepian-Wolf coding over broadcast channels”. IEEE Trans.

Inform. Theory, vol. 52, no. 4, pp. 1469–1482, Apr. 2006. [11] C. Tian, J. Chen, S. N. Diggavi, and S. Shamai. “Optimality and approximate optimality of source-channel separation in networks”. Submitted to the IEEE Trans. Inform. Theory, 2010.

[12] D. Gündüz and E. Erkip, “Reliable cooperative source transmission with side information”. Proc. IEEE Inform. Theory Workshop, Bergen, Norway, Jul. 2007, pp. 22–26.

[13] R. Kwak, W. Lee, A. El Gamal, and J. Cioffi. “Relay with side information”. Proc. IEEE Int. Symp. Inform. Theory, Nice, France, Jun. 2007, pp. 606–610.

[14] R. Dabora. “The capacity region of the fading interference channel with a relay in the strong interference regime”. Submitted to the IEEE Trans. Information Theory, June 2010. Available at http://www.bgu.ac.il/∼daborona/.

[15] L. Sankar, N. B. Mandayam, and H. V. Poor, “On the sum-capacity of the degraded Gaussian multiaccess relay channel”. IEEE Trans. Inform. Theory, vol. 55, no. 12, pp. 5394–5411, Dec. 2009.

[16] T. M. Cover and J. Thomas. Elements of Information Theory. John Wiley and Sons Inc., 1991.

[17] Y. Murin, R. Dabora and D. Gündüz, “Source-channel coding theorems for the multiple-access relay channel”. Submitted to the IEEE Trans. Information Theory, May 2011. Available at http://arxiv.org/abs/1106.3713v2.