arXiv:1503.01435v2 [cond-mat.soft] 9 Jun 2017

Under consideration for publication in J. Fluid Mech. 1

Viscous-poroelastic interaction as mechanism to create adhesion in frogs’ toe pads

A. Tulchinsky and A. D. Gat

Faculty of Mechanical Engineering, Technion - Israel Institute of Technology, Haifa 32000, Israel

(Received 2014)

The toe pads of frogs consist of soft hexagonal structures and a viscous liquid contained between and within the hexagonal structures. It has been hypothesized that this configuration creates adhesion by allowing for long range capillary forces, or alternatively, by allowing for exit of the liquid and thus improving contact of the toe pad. In this work we suggest interaction between viscosity and elasticity as a mechanism to create temporary adhesion, even in the absence of capillary effects or van der Waals forces. We initially illustrate this concept experimentally by a simplified configuration consisting of two surfaces connected by a liquid bridge and elastic springs. We then utilize poroelastic mixture theory and model frog’s toe pads as an elastic porous medium, immersed within a viscous liquid and pressed against a rigid rough surface. The flow between the surface and the toe pad is modeled by the lubrication approximation. Inertia is neglected and analysis of the elastic-viscous dynamics yields a governing partial differential equation describing the flow and stress within the porous medium. Several solutions of the governing equation are presented and show a temporary adhesion due to stress created at the contact surface between the solids. This work thus may explain how some frogs (such as the torrent frog) maintain adhesion underwater and the reason for the periodic repositioning of frogs’ toe pads during adhesion to surfaces.

1. Introduction The toe pads of frogs consist of soft thin hexagonal structures and a viscous fluid between and within the soft structures (Ernst 1973a,b; Green 1979). It has been hypothesized that such configuration enables attachment to surfaces by capillary forces (Emerson & Diehl 1980; Hanna et al. 1991; Federle 2006), or alternatively that the channel network allows for exit of the viscous liquid and thus improves contact of the toe pad with the surface (Federle et al. 2006; Persson 2007; Tsipenyuk & Varenberg 2014). Analytical works include Federle et al. (2006) who modeled the contribution of capillary forces to shear stress on the surface and Persson (2007), who studied the effect of elasticity on capillary forces.

In this work we suggest a mechanism for creating temporary adhesion based on interaction between viscous flow and elastic deformation. We model the toe pads of frogs as an elastic porous medium (similarly to Battiato et al. 2010; Battiato 2012), immersed within a viscous liquid, and pressed against a solid surface with known roughness. The dynamics of the elastic porous material are studied via the poroelastic theory (Biot 1972; Bowen 1980; Ambrosi & Preziosi 2000). The flow between the frogs’ toe pads and the solid surface is modeled by the lubrication approximation. Forces and kinematic constraints acting on the liquid-saturated toe pad deform the material. The deformation of the porous material creates a viscous flow within the toe pads while modifying its stress field. The viscous fluid, flowing from the lubrication region into the porous material, yields a pressure-field and thus effectively creates a force acting between the porous material and the surface, perpendicular to the surface. This force creates tangential friction between the porous material and the solid surface, thus preventing slip on the surface. Such a mechanism will allow for adhesion even in the absence of capillary forces and thus may explain how some frogs can maintain adhesion in the presence of rain or while being submerged (such as river frogs, see Endlein et al. 2013b; Barnes et al. 2002). In addition, the time-varying nature of the suggested mechanism may explain why frogs periodically reposition their toes when connected to a surface (Endlein et al. 2013a,b).

The structure of this paper is as follows: In the next section we illustrate the concept experimentally by a simplified configuration consisting of two surfaces connected by a liquid bridge and elastic springs. In section 3.1 we define the poroelastic problem. In section 3.2 we analyze the flow-field and deformation field within the poroelastic medium. In section 3.3 we analyze the flow in the lubrication region between the toe pad and the solid surface and in section 3.4 we obtain a governing equation for the dynamics of the toe pad, present several solutions and estimate viscous-poroelastic adhesion in frogs. In section 4 we summarize the results.

2. Experimental illustration of viscous-elastic friction creation We initially focus on a simplified case in order to illustrate the effects of viscous-elastic interaction on friction. We examine the dynamics of two parallel surfaces connected by a liquid bridge and linearly elastic springs (see Fig. 1a). While in this case there are no poroelastic dynamics, it includes both viscous forces and elastic forces due to the liquid bridge and the linear springs, respectively. The springs are located outside of the liquid bridge and do not affect the flow-field. Friction is created by the normal force applied by the springs on the contact area with the surface. The configuration is axisymmetric. We denote the gap between the two surfaces h, the viscosity μ, the surface tension γ, the density ρ, the liquid drop volume v_d, the liquid radius r_d, the total springs stiffness k, the relaxed spring length h_r (thus the normal force applied by the springs is k(h − h_r)) and the external normal force f_e (see Fig. 1a). Hereafter, characteristic values are denoted by asterisk superscripts. We define u^∗ as the characteristic speed, p^∗ as the characteristic pressure and h^∗ as the characteristic gap. Following Gat et al. (2011), under the assumptions of shallow liquid bridge, h^∗/r_d ≪ 1, negligible inertia of the liquid, h^{∗2}ρu^∗/μ ≪ 1, negligible gravity gρh^∗/p^∗ ≪ 1 and negligible capillary forces γv_d/(h^∗)^2 ≪ 1, the force balance equation is f_e − μ 3v^2_d 2πh^5 dh dt + k(h_r − h) = 0. (2.1)

The tangential friction acting at the solid interface is f_t = μ_s(h_r −h)k, where μ_s is the friction coefficient. For cases in which both the springs and viscosity terms are non-negligible, order of magnitude yields the characteristic time scale t^∗ = μv^2_d/π^2kh^{∗5}. During this time scale the springs will apply a normal force on the surface of the order of ≈ kh^∗, which will in turn create a tangential friction force.

We conducted experiments with a circular flat plate connected to 10 extended beams acting as linear elastic springs (see Fig. 1b). The solid was printed by Objet Eden250, and the material is Objet FullCure720. In all cases the configuration was tested immediately after printing and used only once. The liquid is silicon oil droplet with volume v_d = 5 · 10^{−6}m^3, density ρ = 750kg/m^3, surface tension 0.021Nm^{−1} and viscosity μ = 60P as.

Figure 1. (a) An illustrative front view of the mathematical model. (b) An upper view photo of the experimental model attached to a horizontal surface with a liquid bridge between and (c) experimental results presenting time vs. slip for plates with springs (squares) and without springs (circles). Bars presents standard deviation.

The plate was pressed against a rigid surface (positioned parallel to gravity, see Fig. 1b) and released at t = 0. The properties of the examined configuration are k ≈ 4.5·10^4N/m, h_r = 1.3mm. The order of magnitude of capillary forces is 2γv_d/(h^∗)^2 ≈ 0.2N and is negligible compared with the order of magnitude of the elastic force kh^∗ ≈ 50N (where h^∗ = 1mm). For such a configuration the characteristic time scale of is t^∗ = μv^2_d/π^2kh^{∗5} = O(10^3s). We examined 6 identical plates and 6 control plates without springs. In all cases the initial gap was determined by spacers (see Fig. 1a) as h(t = 0) = 0.8mm. The results are presented in Fig 1c and clearly show enhancement of friction due to viscouselastic interaction. While the control plates without springs immediately slipped, the configurations with springs slipped only at ≈ 250s.

3. Adhesion due to viscous-poroelastic interaction We now turn to analyze a more complex case of viscous-elastic interaction involving viscous flow within an elastic porous material as a mechanism to create adhesion.

3.1. Problem Definition We model the interaction between an elastic porous material and a Newtonian fluid via the poroelastic mixture theory (Preziosi et al. 1996; Bowen 1980; Atkin & Craine 1976; Rajagopal & Tao 1995). We focus on axi-symmetric configurations with negligible inertial and capillary effects. The relevant regions are the poroelastic region and a thin liquid-filled gap between the poroelastic region and the rough surface (marked by red dotted line, see Fig. 2). The relevant variables are the radius of the poroelastic material r_o, the poroelastic material height h, the poroelastic material relaxed height h_r (height

Figure 2. Illustrative description of the model consisting of a poroelastic material (dotted area) connecting a rigid body and a lubrication region (red dashed). The poroelastic material is axi-symmeteric with radius ro, height h and external axial force fe acting on the rigid body.

when no stress is applied on the solid), the external force f_e, the solid fraction (i.e. ratio of solid volume to total volume of liquid and solid) Φ, the relaxed solid fraction Φ_r, the time t, the radial and axial coordinates r = (r, z), the solid velocity v_s = (u_s, v_s, w_s), the liquid velocity v_l = (u_l, v_l, w_l), the liquid viscosity μ, the solid density ρ_s, the liquid density ρ_l, the permeability k, and the excess stress tensor σ (defined as the stress tensor of the mixture minus the liquid pressure, see Preziosi et al. 1996).

3.2. Analysis of the poroelastic medium The dynamics of a poroelastic medium saturated with Newtonian incompressible liquid is governed by the conservation of mass of the solid ∂Φ ∂t + ∇ · (Φv_s) = 0, (3.1)

the conservation of mass of the liquid − ∂Φ ∂t + ∇ · [(1 − Φ)v_l] = 0, (3.2)

Darcy’s law for the flow within the porous material

v_l − v_s = − k (1 − Φ)μ

(∇p − ρ_lg) (3.3)

and equation of the mixed momentum ρ_c ( ∂v_m ∂t + v_m · ∇v_m ) = −∇p + ∇ · σ + [ρ_sΦ + ρ_l(1 − Φ)]g (3.4)

where ρ_c = Φρ_s + (1 − Φ)ρ_l is the density of the mixture considered as a whole and v_m = [Φρ_sv_s + (1 − Φ)ρ_lv_l]/ρ_c is the mass average velocity (see Preziosi et al. 1996) .

The relevant boundary conditions are no solid velocity at z = 0 and external velocity function v_e(t) at z = h(t), v_s(z = 0) = 0, v_s(z = h(t)) = v_l(z = h(t)) = v_e(t). (3.5) The initial conditions are Φ(t = 0) = Φ_i, h(t = 0) = h_i. (3.6) Hereafter all normalized parameters are denoted by capital letters and characteristic values are denoted by asterisk superscripts. We define normalized coordinates R, Z and time T R = r r_o , Z = z h^∗ , T = t h^∗/w^∗ , (3.7)

normalized liquid velocity V_l and pressure P

V_l = v_l w^∗ , P = p p^∗ , (3.8)

normalized solid velocity V_s, solid stress Σ, permeability K

V_s = v_s w^∗ , Σ = σ σ^∗ , K = k k^∗ , (3.9)

and poroelastic height H H = h(t) h^∗ , (3.10) where h^∗ is the characteristic height, w^∗ is the characteristic speed, p^∗ is the characteristic pressure, σ^∗ is the characteristic axial stress and k^∗ is the characteristic permeability.

Our analysis will focus on a thin geometry, defined as

ε_1 = h^∗ r_o ≪ 1. (3.11)

Substituting the normalized variables yield the leading order form of (3.1-3.4) as ∂Φ ∂T + ∂ ∂Z (ΦW_s) + O(ε_1) = 0, (3.12) − ∂Φ ∂T + ∂ ∂Z [(1 − Φ)W_l] + O(ε_1) = 0, (3.13)

W_l − W_s = − k^∗p^∗ μw^∗h^∗ K_{zz} (1 − Φ) ∂P ∂Z + O ( ε_1, ρ_lgk_0 μw^∗ ) (3.14) and ∂P ∂Z = σ^∗ p^∗ ∂Σ_{zz} ∂Z + O ( ε_1, ρ_j (w^∗)^2 p^∗ , [ρ_sΦ + ρ_l(1 − Φ)]g p^∗ ) , (3.15)

where Σ_{zz} and K_{zz} are the axial terms of Σ and K, respectively, and W_s and W_l are the axial solid and liquid speeds, respectively.

The constitutive relationships for the permeability, k, and stress σ are approximated as (following previous works of Anderson 2005; Siddique 2009; Siddique et al. 2009) k_{zz} = k_0 Φ , σ = m(Φ_r − Φ) (3.16)

where k_0 > 0 and m > 0 are known constants defining the poroelastic material permeability and stiffness, respectively. Order of magnitude of (3.15) and (3.16) yields p^∗ = σ^∗ = m and k^∗ = k_0.

We define the scaled coordinate Ψ = z/h(t) and formulate the problem according to Preziosi et al. (1996). Adding (3.13), (3.12), integrating over Z and using (3.5) we obtain

W_l(1 − Φ) + ΦW_s = ∂H ∂T . (3.17)

From (3.14) and (3.17),

W_s = ∂H ∂T − mk_0 μw^∗h^∗ 1 ΦH(T ) ∂Φ ∂Ψ (3.18) and W_l = ∂H ∂T + mk_0 μw^∗h^∗ 1 (1 − Φ)H(T ) ∂Φ ∂Ψ . (3.19)

Combining (3.19) and (3.12) together with (3.15) yields ∂Φ ∂T + (1 − Ψ) ∂H ∂T 1 H(T ) ∂Φ ∂Ψ = mk_0 μw^∗h^∗ 1 H^2(T )

∂^2Φ ∂Ψ^2

. (3.20)

We express the boundary conditions (3.5) in terms of solid fraction Φ as mk_0 μw^∗h^∗ ∂Φ ∂Ψ = 0, Ψ = 1 (3.21) and mk_0 μw^∗h^∗ ∂Φ ∂Ψ − H(T ) ∂H ∂T Φ = 0, Ψ = 0, (3.22)

where μw^∗h^∗/mk_0 can be interpreted as the ratio between the characteristic speed of the poroelastic problem, w^∗, and the characteristic speed of the viscous flow, mk_0/μh^∗.

3.3. Analysis of lubrication region We denote by tildes the liquid velocity ṽ_l = (ũ_l, w̃_l) in the lubrication region, where ũ_l is the radial speed and w̃_l is the axial speed. The governing equations in the lubrication region are the axi-symmetric Stokes equations for Newtonian incompressible liquid

∇p = μ∇^2ṽ_l (3.23)

and conservation of mass ∇ · ṽ_l = 0. (3.24) The relevant boundary conditions are gauge pressure p = 0 at r = r_o, symmetry ∂p/∂r = 0 at r = 0, no-slip and no-penetration ṽ_l = 0 at the solid interface and mass-flux and pressure matching to the poroelastic region w̃_l = (1 − Φ)w_l at z = 0. The liquid slip at the boundary of the porous material, z = 0, is proportional to ∝ √ k_0∂ũ_l/∂z, where √ k_0 is the characteristic length scale of the permeable material (Beavers & Joseph 1967). We relate the characteristic roughness h̃ to average viscous resistance by defining

h̃^{−3} = 1 A ∫ A h^{−3}_s dA, (3.25)

where h_s is the local gap between the solid surface and the poroelastic surface and A is a sufficiently large surface area on the z plane. The normalized velocity Ũ_l, W̃_l and Z̃ coordinate for the lubrication region are defined as

Ũ_l = u u^∗ , W̃_l = W̃_l w^∗ , Z̃ = z h̃ . (3.26) We require sufficiently small k_0 so that

ε_2 = k_0h^∗ h̃3/12 ≪ 1, ε^3 = u_l(Z = 0) u^∗ = √ k_0 h^∗ ≪ 1 (3.27)

representing the scaled pore size and the slip at the boundary of the poroelastic surface. For ε_3 ≪ 1 we require Ũ_l = 0 at Z̃ = 0. (The lubrication region may also be modeled as a porous region of depth h_p and the radial permeability k_p, where h̃^3/12 = k_ph_p, see Battiato et al. 2010; Battiato 2012).

Substituting (3.26) into (3.23,3.24), order of magnitude analysis yields

u^∗ = w^∗r_o h̃ , w^∗ = mh̃^3/12 μr^2_0

, (3.28)

and normalized (3.23) is thus ∂P ∂R ∼ 1 H^3_s

∫_0 −H_s Ũ_ldZ̃, ∂P ∂Z̃ ∼ 0, (3.29)

where H_s = h_s/h̃ is the local normalized gap. We substitute (3.29) into (3.24) and apply the boundary conditions W̃_l = (1−Φ)W_l at Z̃ = 0 (flux matching between the lubrication region and the poroelastic region) and Ũ_l = W̃_l = 0 at the solid surface. Thus we obtain the pressure distribution in the lubrication region. Substituting into the variables of the poroelastic region and utilizing (3.25) yields

P (Ψ = 0) ∼ −(1 − Φ(Ψ = 0))W_l(Ψ = 0)

1 − R^2 4 . (3.30)

3.4. Results 3.4.1. Governing equations

Substituting (3.28) into (3.20-3.22) yields mk_0 μw^∗h^∗ = k_0h^∗ h̃3/12 r^2_o (h^∗)^2 = ε_2 ε^2_1

, (3.31)

and the governing equation 1 H^2

∂^2Φ ∂Ψ^2 − ε^2_1 ε_2 [ ∂Φ ∂T + (1 − Ψ) ∂H ∂T 1 H ∂Φ ∂Ψ ] = 0, (3.32)

with the boundary conditions ∂Φ ∂Ψ − ε^2_1 ε_2 H ∂H ∂T Φ = 0, Ψ = 0, (3.33) ∂Φ ∂Ψ = 0, Ψ = 1 (3.34) and initial condition Φ = Φ_i, T = 0. (3.35) The liquid speed W_l and solid speed W_s are thus

W_s = ∂H ∂T − ε_2 ε^2_1 1 ΦH(T ) ∂Φ ∂Ψ , W_l = ∂H ∂T + ε_2 ε^2_1 1 (1 − Φ)H(T ) ∂Φ ∂Ψ . (3.36)

Substituting (3.36) into (3.30) yields the gauge pressure at Z = 0

P (Z = 0) = − (1 − Φ(0)) ( ∂H ∂T + ε_2 ε^2_1 1 (1 − Φ(0))H

∂Φ(0) ∂Ψ ) 1 − R^2 4 . (3.37)

Integration over P (Z = 0) will yield the total normal force applied by the liquid. The external force applied on the poroelastic material F_e = f_e/mr^2_o (see Fig. 2), is balanced by the force applied by the solid surface (denoted hereafter as F_s = π(Φ_r − Φ(Ψ = 0)) and normalized by mr^2_o ) and the force applied by the liquid gauge pressure at Ψ = 0. The force balance equation, F_e =

∫_1 0 (Σ_{zz} − P )2πRdR, yields the expression for the external force

F_e = π(Φ_r − Φ(Ψ = 0)) + π 8 (1 − Φ(0)) ( ∂H ∂T + ε_2 ε^2_1 1 (1 − Φ(0))H

∂Φ(0) ∂Ψ ) . (3.38)

For the limit ε^2_1/ε_2 ≪ 1 we define the asymptotic expansion

Φ = Φ_0 + ( ε^2_1 ε_2 ) Φ_1 + ( ε^2_1 ε_2

)_2

Φ_2 + O [( ε^2_1 ε_2

)_3]

. (3.39)

(We focus on the limit ε^2_1/ε_2 ≪ 1 since it agrees with the characteristic physical parameters of frogs’ toe pads, see Section 3.4.4.) We substitute (3.39) into (3.32-3.35). The leading order problem yields Φ_0(T ) is a function of time only. The first order terms of (3.32) and (3.34) yields

Φ_1 = H^2

∂Φ_0 ∂T ( Ψ^2 2 − Ψ ) + C_1(T ). (3.40)

Substituting Φ_0 and Φ_1 into the O(ε^2_1/ε_2) order boundary condition at Ψ = 0 (3.33) yields an ordinary differential equation with regard to time ∂Φ_0 ∂T + ∂H ∂T Φ_0 H = 0. (3.41)

Solving (3.41) with (3.35) yields Φ_0 = Φ_iH(0)/H(T ). We determine C_1(T ) from the O[(ε^2_1/ε_2)^2] order (3.32),

∂^2Φ_2 ∂Ψ^2

= H^2

∂Φ_1 ∂T + (1 − Ψ) ∂H ∂T H ∂Φ_1 ∂Ψ (3.42)

and the O[(ε^2_1/ε_2)^2] boundary and initial conditions. Substituting (3.40) into (3.42) and applying (3.34) we obtain an ordinary differential equation from the boundary condition at Ψ = 0, similarly to (3.41), for the O(ε^2_1/ε_2) order, ∂C_1 ∂T + ∂H ∂T 1 H C_1 = − 1 3 Φ_iH(0) H ∂ ∂T ( H ∂H ∂T ) . (3.43)

Applying (3.35) we solve (3.43) and obtain,

C_1 = −

H(0) 3 Φ_i ∂H ∂T . (3.44)

Thus Φ to order O(ε^2_1/ε_2) is Φ Φ_i ∼ H(0) H + ε^2_1 ε_2

H(0) ∂H ∂T ( Ψ − Ψ^2 2 − 1 3 ) , (3.45)

and from (3.35) we obtain the requirement ∂H(0)/∂T = 0 in order to satisfy spatially uniform initial condition.

3.4.2. Externally controlled H for ε^2_1/ε_2 ≪ 1

Based on (3.45) and (3.38) we can calculate F_e required to achieve an arbitrary H(T ). After calculating H(T ), exact solutions of the solid fraction Φ, fluid velocity W_l, solid velocity W_s and internal stress Σ can be obtained from (3.45, 3.36-3.38). Figure 3 presents a case of ∂H/∂T = tanh(CT ), where C = 100 and thus ∂H/∂T ≈ 1 for T > 0.02. The initial uniform solid fraction of the poroelastic medium is Φ_i = 0.6, relaxed solid fraction is Φ_r = 0.4, and ε^2_1/ε_2 = 0.1. Part (a) presents change in poroelastic layer height H − 1

(dash-dotted), external force F_e (solid), total force by the liquid pressure F_p (dashed) and force applied by the solid surface F_s (dotted). The total force by the liquid pressure F_p becomes nearly constant from T ≈ 0.03 (as the ∂H/∂T → 1), while the F_s decreases in time. The external force is initially negative and prevents the compressed poroelastic material to expand more rapidly than the required ∂H/∂T = 1. From T ≈ 0.1 F_e is positive and acts to increase ∂H/∂T . In parts (b-d) blue, purple, red, yellow and green lines mark normalized time T = 0.2, 0.4, 0.6, 0.8, and 1, respectively. Part (b) presents solid fraction Φ vs. Z for various times, showing decrease of Φ with time and as Z → 0. Part (c) presents liquid speed W_l (solid) and solid speed W_s (dashed) vs. Z for various times. Both speeds are approximately linear with Z with gradients decreasing with time. Part (d) presents pressure P (solid) and axial stress Σ_{zz} vs. Z for various times. The average pressure P is approximately constant, due to the uniform liquid mass-flux into the poroelastic material. The axial stress increases with time due to the forced deformation of the poroelastic material. Due to the initial compression, the axial stress is negative until T ≈ 0.4 and then becomes positive due to stretching by the external force.

3.4.3. Externally controlled F_e for ε^2_1/ε_2 ≪ 1

We apply (3.45) with (3.38) to obtain H as a function of the external force acting on poroelastic material for ε^2_1/ε_2 ≪ 1,

F_e = π ( Φ_r − Φ_i

H(0) H ) + π 8 ∂H ∂T . (3.46)

For constant F_e separation of variables yields an implicit solution of H(T ), T = π 8 [ H − H(0) F_e − πΦ_r − πΦ_iH(0) (F_e − πΦ_r)^2 ln ( H(F_e − πΦ_r) − πΦ_iH(0) H(0)(F_e − πΦ_r) − πΦ_iH(0) )] . (3.47)

Figure 4 presents the case of initial compression of the poroelastic material, with sudden release F_e = 0, solved by (3.47). For F_e = 0, exact solutions of the solid fraction Φ, fluid velocity W_l, solid velocity W_s and internal stress Σ_{zz} are calculated from (3.45, 3.36-3.38). Initial uniform solid fraction of the poroelastic medium is Φ_i = 0.6, relaxed solid fraction is Φ_r = 0.4, initial height is H(0) = 1 and ε^2_1/ε_2 = 0.1. Part (a) presents change in poroelastic layer height H − 1 (dash-dotted), external required force F_e (solid), total force by the liquid pressure F_p (dashed) and force applied by the solid surface F_s (dotted). The absolute value of the force applied by the liquid pressure F_p decreases while the sign F_p is negative for all T . The force applied by the solid surface F_s decreases in time and is positive for all T . The speed ∂H/∂T is maximal at T = 0 and decreases with time as the configuration reaches a steady balance. In parts (b-d) blue, purple, red, yellow and green lines mark normalized time T = 0.2, 0.4, 0.6, 0.8, and 1, respectively. Part (b) presents solid fraction Φ vs. Z for various times, showing decrease of Φ with time and nearly constant values with Z. Part (c) presents liquid speed W_l (solid) and solid speed W_s (dashed) vs. Z for various times. Both speeds are approximately linear with Z with gradients decreasing with time. Part (d) presents pressure P (solid) and axial stress Σ_{zz} vs. Z for various times. Since no external forces act on the system, the dominant balance is between pressure P and axial stress and thus P ≈ Σ_{zz}. The magnitude of both parameters decreases with time as the system approach steady balance.

3.4.4. Characteristic values of frogs’ toe pads and adhesion time estimation We estimate, based on existing works, the order-of-magnitude of the relevant physical properties of frog’s toe pads. We focus on torrent frogs due to their ability to keep adhesion underwater and thus without capillary forces. Based on Federle et al. (2006)

Figure 3. Configuration with speed ∂H/∂T = tanh(100T ) (effectively ∂H/∂T ≈ 1 for T > 0.02), initial uniform solid fraction of the poroelastic medium Φi = 0.6, relaxed solid fraction Φr = 0.4, and ε^2_1/ε2 = 0.1. Part (a) presents change in gap H − 1 (dash-dotted), external required force Fe (solid), total force by the liquid pressure Fp (dashed) and force applied by the solid surface Fs (dotted). In parts (b-d) blue, purple, red, yellow and green lines mark normalized time T = 0.2, 0.4, 0.6, 0.8, and 1, respectively. Part (b) presents solid fraction Φ vs. Z for various times. Part (c) presents liquid speed W_l (solid) and solid speed Ws (dashed) vs. Z for various times. Part (d) presents pressure P (solid) and axial stress Σzz vs. Z for various times.

and Endlein et al. (2013a) we obtain the total toe pad area 10^{−4}m^2, number of toes 18, yielding individual toe pad radius of r_o = 1.3 · 10^{−3}m (assuming circular toe pads), frog mass is 2.7 · 10^{−3}kg, the viscosity of the mucus is μ ≈ 10^{−3}P a · s, toe pad height is h_r = 10^{−5}m, the permeability of the frog’s toe pad is calculated via k_0 ≈ d^2_p/4, where d_p = 10^{−7}m is the characteristic length scale of the pores. We examine various values of the characteristic gap in the lubrication region h̃ and the stiffness parameter m. For h̃ = 10−6m, we obtain ε_1 = h∗/r_o ≈ 6.3 · 10−3, we and ε_2 = k_0h∗/12h̃3 = 0.1, thus ε^2_1/ε_2 ≈ 4 · 10^{−4}.

Slip will occur when f_t ⩾ f_sμ_s, where f_s is the dimensional normal force acting on the surface, μ_s is the friction coefficient and f_t is a tangential force (see Fig. 1). Utilizing F_s = π(Φ_r − Φ(Ψ = 0)), we can obtain Φ_s, the solid fraction at Ψ = 0 for which slip will occur

Φ_s = Φ_r − 1 μ_s f_t mπr^2_o . (3.48)

Figure 4. Configuration with initial compression and a sudden release at T = 0 with Fe = 0. The initial uniform solid fraction of the poroelastic medium is Φi = 0.6, relaxed solid fraction Φr = 0.4, and ε^2_1/ε2 = 0.1. Part (a) presents change in poroelastic layer height H − 1 (dash-dot-ted), external required force Fe (solid), total force by the liquid pressure Fp (dashed) and force applied by the solid surface Fs (dotted). In parts (b-d) blue, purple, red, yellow and green lines mark normalized time T = 0.2, 0.4, 0.6, 8, and 1, respectively. Part (b) presents solid fraction Φ vs. Z for various times. Part (c) presents liquid speed W_l (solid) and solid speed Ws (dashed) vs. Z for various times. Part (d) presents pressure P (solid) and stress Σzz vs. Z for various times.

Substituting (3.45) into (3.48) yields H_s, the height of poroelastic medium when slip occurs

H_s =

Φ_i Φ_s

, (3.49)

and substituting (3.49) into (3.47) yields the adhesion time t_a.

Fig. 5 presents dimensional adhesion time t_a for various configurations and parameters. Part (a) presents the slope angle θ and the normal forces. The normal force is f_e = − cos(θ)m_f g/n_t and the tangential force is f_t = | sin(θ)m_f g/n_t|, where m_f is the mass of the frog, g is gravity and n_t is the number of frog toes. Parts b-c present adhesion time t_a for different frog mass of 10^{−3}Kg (dashed), 2 · 10^{−3}Kg (dashed) and 3 · 10^{−3}Kg (dotted) at θ = 60^0. Part b presents adhesion time t_a vs. stiffness parameter m for Φ_i = 0.85 and θ = 60^0. For stiffness parameter under a critical value (m ≈ 10^3P a) no adhesion is created. With increasing m a maxima of adhesion time is presented as well as a monotonic decrease in adhesion time as m → ∞. Part (c) presents adhesion time

Figure 5. Adhesion time (time until tangential slip occur) ta for various physical parameters, Part (a) presents the slope angle θ and the normal fe and tangential ft forces. Part (b) presents adhesion ta time vs. the stiffness of the poroelastic material m for θ = 60^0 and Φi = 0.85. Part (c) presents adhesion ta time vs. the initial solid fraction Φi (initial compression) for θ = 60^0 and m = 5 · 10^5 [P a]. Part (d) presents adhesion ta time vs. slope angle θ for Φi = 0.85 and m = 5 · 10^5[P a]. Frog mass of 10^{−3}Kg (dashed) 2 · 10^{−3}Kg (dashed) and 3 · 10^{−3}Kg (dotted) are presented. In all cases Φr = 0.7.

t_a vs. characteristic gap in the lubrication region h̃ (defined by (3.25)), for θ = 60^0 and m = 5 · 10^5P a. A monotonic increase in adhesion time with decreasing h̃ is observed. Part (d) presents adhesion time vs. slope angle θ for Φ_i = 0.85 and m = 5 · 10^5P a. Under a critical minimal value of θ steady adhesion is achieved. With increasing θ there is a decrease in adhesion time until a minimum value and then a moderate maxima at θ = 180^0. In all cases we observe a monotonic increase in adhesion time with reduction of frog mass.

4. Concluding Remarks In this work we suggested viscous-elastic interaction as a mechanism to explain adhesion of frogs’ toe pads. We applied a poroelastic model for the toe pad and a lubrication approximation for the flow between the toe pad and the solid surface. We obtained a governing equation for the solid fraction, which can be solved and then applied to obtain the solid stress, solid velocity, liquid pressure and liquid velocity. The viscous-elastic interaction was shown to be able to create temporary adhesion, even in the absence of capillary forces, and the adhesion time was estimated for physical parameters chosen from orderof-magnitude estimation of frogs’ toe pads. A maxima for adhesion time was observed with regard to m, the stiffness parameter of the poroelastic medium, and a minima with regard to the slope angle of the surface. The time-dependent nature of viscous-elastic adhesion is in agreement with the periodic repositioning of frogs’ toe pads during adhesion to surfaces. This analysis focused on a single toe pad, however, the dynamics of a complete frog includes multiple toe pads which are repositioned at different times. Thus the computed adhesion time t_a represents the time a single toe pad is connected to a surface may differ significantly from adhesion time of the entire frog.

This research was supported by the ISRAEL SCIENCE FOUNDATION (Grant 818/13).

Appendix A. Dimensional equations and boundary conditions The dimensional governing equation for Φ, the solid fraction, is ∂Φ ∂t + ∂ ∂z [ Φ ( ∂h ∂t − mk_0 μ ∂Φ ∂z )] = 0 (A 1)

with the dimensional boundary conditions ∂Φ ∂z − μ mk_0 ∂h ∂t Φ = 0, z = 0 (A 2) ∂Φ ∂z = 0, z = h(t) (A 3) and initial condition Φ = Φ_i, t = 0, (A 4) where the parameters k_0, m and Φ_r represent permeability, stiffness parameter and relaxed solid fraction, respectively, are known constants defining the properties of the poroelastic medium by the relations (following Anderson 2005; Siddique 2009; Siddique et al. 2009) k_{zz} = k_0 Φ , σ = m(Φ_r − Φ). (A 5) The dimensional liquid speed w_l and solid speed w_s are

w_s = ∂h ∂t − mk_0 μ(1 − Φ) ∂Φ ∂z (A 6) and w_l = ∂h ∂t + mk_0 μΦ ∂Φ ∂z . (A 7)

The dimensional gauge pressure at z = 0 is

p(z = 0) = −3 μr^2_o h̃3 (1 − Φ(0)) ( ∂h ∂t + mk_0 μ(1 − Φ(0))

∂Φ(0) ∂z ) ( 1 − r^2 r^2_o ) . (A 8)

The dimensional force balance equation of the poroelastic medium is

f_e = 3π 2 μr^2_o h̃3 (1 − Φ(0)) ( ∂h ∂t + mk_0 μ(1 − Φ(0))

∂Φ(0) ∂z ) − mπr^2_o (Φ(z = 0) − Φ_r). (A 9)

where f_e is the external force. Slip occurs when f_t > μ_sf_s, where f_s = mπr^2_o (Φ(z = 0) − Φ_r) is the normal force applied by the solid fraction of the poroelastic material and and μ_s is the friction coefficient.

14 A. Tulchinsky and A. D. Gat

For ε^2_1/ε_2 → 0 we obtain the relation between Φ and h Φ Φ_i ∼ h(0) h + μh(0) mk_0 ∂h ∂t ( z h − 1 2 z^2 h^2 − 1 3 ) . (A 10)

REFERENCES

Ambrosi, D. & Preziosi, L. 2000 Modeling injection molding processes with deformable porous preforms. SIAM J. Appl. Math. 61 (1), 22–42.

Anderson, D.M. 2005 Imbibition of a liquid droplet on a deformable porous substrate. Physics of Fluids 17 (8), 087104–087104–22.

Atkin, R.J. & Craine, R.E. 1976 Continuum theories of mixtures: basic theory and historical development. Quarterly J. Mech. and Appl. Math. 29 (2), 209–244.

Barnes, J, Smith, J, Oines, C & Mundl, R 2002 Bionics and wet grip. Tire Technology International 2002 (Dec), 56–60.

Battiato, Ilenia 2012 Self-similarity in coupled brinkman/navier–stokes flows. Journal of Fluid Mechanics 699, 94–114.

Battiato, Ilenia, Bandaru, Prabhakar R & Tartakovsky, Daniel M 2010 Elastic response of carbon nanotube forests to aerodynamic stresses. Physical review letters 105 (14), 144504.

Beavers, G.S. & Joseph, D.D. 1967 Boundary conditions at a naturally permeable wall. J.

Fluid Mech. 30, 197–207.

Biot, M.A. 1972 Theory of finite deformations of porous solids. Indiana University Math. J.

21 (7), 597–620.

Bowen, R.M. 1980 Incompressible porous media models by use of the theory of mixtures. Int.

J. Eng. Sci. 18 (9), 1129–1148.

Emerson, S.B. & Diehl, D. 1980 Toe pad morphology and mechanisms of sticking in frogs.

Biological J. Linnean Society 13 (3), 199–216.

Endlein, T., Barnes, W. J. P., Samuel, D. S., Crawford, N. A., Biaw, A. B. & Grafe, U. 2013a Sticking under wet conditions: The remarkable attachment abilities of the torrent frog, staurois guttatus. PLOS ONE 8 (9), e73810.

Endlein, T., Ji, A., Samuel, D., Yao, N., Wang, Z., Barnes, W. J. P., Federle, W., Kappl, M. & Dai, Z. 2013b Sticking like sticky tape: tree frogs use friction forces to enhance attachment on overhanging surfaces. J. Royal Society Interface 10 (80), 20120838.

Ernst, V.V. 1973a The digital pads of the tree frog, hyla cinerea. i. the epidermis. Tissue and Cell 5 (1), 83–96.

Ernst, V.V 1973b The digital pads of the tree frog, hyla cinerea. ii. the mucous glands. Tissue and Cell 5 (1), 97–104.

Federle, W. 2006 Why are so many adhesive pads hairy? J. Exp. Biology 209 (Pt 14), 2611– 2621, lR: 20131121; JID: 0243705; ppublish.

Federle, W., Barnes, W.J., Baumgartner, W., Drechsler, P. & Smith, J.M. 2006 Wet but not slippery: Boundary friction in tree frog adhesive toe pads. J. Royal Society, Interface 3 (10), 689–697, lR: 20130904; GR: Wellcome Trust/United Kingdom; JID: 101217269; OID: NLM: PMC1664653; ppublish.

Gat, A.D., Navaz, H. & Gharib, M. 2011 Dynamics of freely moving plates connected by a shallow liquid bridge. Physics of Fluids (1994-present) 23 (9), 097101.

Green, D.M. 1979 Treefrog toe pads: comparative surface morphology using scanning electron microscopy. Canadian J. Zoology 57 (10), 2033–2046.

Hanna, G., Jon, W. & Barnes, W.J. 1991 Adhesion and detachment of the toe pads of tree frogs. J. Exp. Biology 155 (1), 103–125.

Persson, BNJ 2007 Wet adhesion with application to tree frog adhesive toe pads and tires.

Journal of Physics: Condensed Matter 19 (37), 376110.

Preziosi, L., Joseph, D.D. & Beavers, G.S. 1996 Infiltration of initially dry, deformable porous media. Int. J. Multiphase Flow 22 (6), 1205–1222.

Rajagopal, K.R. & Tao, L. 1995 Mechanics of mixtures. World Sci., Singapore .

Viscous-elastic adhesion 15

Siddique, J.I. 2009 Newtonian and non-newtonian flows into deformable porous materials. PhD thesis, George Mason University.

Siddique, J.I., Anderson, D.M. & Bondarev, A. 2009 Capillary rise of a liquid into a deformable porous material. Physics of Fluids 21 (1), 013106.

Tsipenyuk, A. & Varenberg, M. 2014 Use of biomimetic hexagonal surface texture in friction against lubricated skin. J. Royal Soc. Interface 11, 20140113.