arXiv:1712.06129v1 [physics.optics] 17 Dec 2017

Electromagnetic energy and negative asymmetry parameter in coated magneto-optical cylinders: Applications to tunable light transport in disordered systems

Tiago J. Arruda,^{1, ∗} Alexandre S. Martinez,^{1, 2} and Felipe A. Pinheiro^3 1Faculdade de Filosofia, Ciências e Letras de Ribeirão Preto, Universidade de São Paulo, 14040-901 Ribeirão Preto, São Paulo, Brazil 2National Institute of Science and Technology in Complex Systems, 22290-180 Rio de Janeiro, Rio de Janeiro, Brazil 3Instituto de Física, Universidade Federal do Rio de Janeiro, 21941-972 Rio de Janeiro, Rio de Janeiro, Brazil

We investigate electromagnetic scattering of normally irradiated gyrotropic, magneto-optical coreshell cylinders using Lorenz-Mie theory. A general expression for time-averaged electromagnetic energy inside a coated gyroelectric and gyromagnetic scatterer is derived. Using realistic material parameters for a silica core and InSb shell, we calculate the stored electromagnetic energy and the scattering anisotropy. We show that the application of an external magnetic field along the cylinder axis induces a drastic decrease in electromagnetic absorption in a frequency range in the terahertz, where absorption is maximal in the absence of the magnetic field. We demonstrate not only that the scattering anisotropy can be externally tuned by applying a magnetic field, but also that it reaches negative values in the terahertz range even in the dipolar regime. We also show that this preferential backscattering response results in an anomalous regime of multiple light scattering from a collection of magneto-optical core-shell cylinders, in which the extinction mean free path is longer than the transport mean free path. By additionally calculating the energy-transport velocity and diffusion coefficient, we demonstrate an unprecedented degree of external control of multiple light scattering, which can be achieved by either applying an external magnetic field or varying the temperature.

PACS numbers: 42.25.Fx, 42.79.Wc, 41.20.Jb, 78.20.Ci

I. INTRODUCTION

Electromagnetic (EM) scattering by small particles with sizes of the order of the wavelength has many applications not only in different areas of physics, such as meteorology, optical communications, sensing, and astrophysics [1], but also in interdisciplinary fields, such as biophysics [2]. The advent of plasmonics and metamaterials has allowed for the discovery of novel scattering phenomena, which do not exist in naturally occurring materials such as plasmonic cloaking [3–5], unconventional Fano resonances [6–9], artificial magnetism [10, 11], superscattering [12], and the unprecedented control of the scattering directionality [13, 14].

In particular, controlling the scattering direction crucially depends on the design optimization of the electric and magnetic responses of small particles. Most approaches to controlling the scattering direction rely on tailoring the electric structures of nanoparticles, as typically the electric response is dominant in natural media at optical frequencies [1, 15]. However, efforts have been made to propose and design metamaterials that support both electric and magnetic dipolar resonances, such as spheres [13, 16] and high permittivity cylinders [14]. These efforts have allowed the achievement of zero-backward scattering and near-zero-forward scattering conditions (known as Kerker conditions), first

∗ tiagoarruda@pg.ffclrp.usp.br

theoretically predicted for hypothetical particles exhibiting both electric and magnetic dipolar resonances [17], and highly directional EM scattering [18–23]. The observation of Kerker conditions relies on the interference of electric and magnetic dipoles in nanostructures [24, 25]. Alternative theoretical approaches for Kerker conditions, involving electric dipoles and quadrupoles, also exist [26]. Recently, both broadband zero backward and near-zero forward scattering have been obtained even beyond the dipole limit, relaxing design constraints in practical experiments [27]. Other mechanisms for achieving directional light scattering have also been proposed using magneto-optical materials [28, 29].

In addition, achieving preferential backward scattering remains a challenge and has many applications in multiple light scattering. Preferential backscattering, which hardly occurs in natural media, is characterized by negative values of the asymmetry parameter, the average of the cosine of the scattering angle ⟨cos θ⟩. Indeed, for small particles in the Rayleigh regime, scattering is dipolar so that ⟨cos θ⟩ ≈ 0. In contrast, Mie particles scatter strongly in the forward direction, ⟨cos θ⟩ ≈ 1. Negative ⟨cos θ⟩ has been reported in ferromagnetic particles [30] and lossless dielectric nanospheres made of moderate permittivity materials, such as silicon or germanium nanospheres in the infrared region [31]. In these cases, negative asymmetry parameters have been show to lead to an unusual regime in multiple light scattering, in which the scattering mean free path is larger than the transport mean free path [31]. This peculiar transport regime has also been demonstrated for multiple scattering systems with correlated disorder under certain conditions [32].

In this paper we propose an alternative, versatile strategy not only to achieve preferential backscattering (negative ⟨cos θ⟩) but also to control the scattering direction with an external parameter, which can be either an applied magnetic field or the temperature. We demonstrate that these effects can be obtained by investigating light scattering in dielectric cylinders coated with a gyroelectric, magneto-optical shell. For concreteness, we consider realistic material parameters: a silica (SiO_2) core and an indium antimonide (InSb) shell, which has a strong magneto-optical and temperature dependence of the dielectric function on the response in the far-infrared [33– 35]. Specifically, in the framework of the Lorenz-Mie theory we show that the asymmetry scattering factor for this system can be tuned from negative to positive values by applying moderate magnetic fields B at the Voigt configuration. We derive a closed analytical expression for the time-averaged EM energy stored inside the core-shell cylinder for both TE and TM polarizations to show that the application of an external magnetic field induces a gap in EM absorption in the terahertz (THz) regime. We also consider multiple light scattering by an assembly of coated-cylinders and calculate the transport meanfree path, energy-transport velocity and light diffusion coefficient. This analysis reveals that the unusual light transport regime where the scattering mean free path is longer than the transport mean free path can be reached by varying either the temperature or the external magnetic field.

This paper is organized as follows. In Sec. II, we present the system and fundamental quantities regarding the Lorenz-Mie theory in a consistent notation. Our expressions are general and can be applied to arbitrary core-shell cylinders containing gyroelectric and gyromagnetic materials normally irradiated with plane waves in TE or TM polarizations. The main analytical result is presented in Sec. III, in which we calculate the timeaveraged internal energy and its relation to the absorption cross section, generalizing previous results obtained for isotropic cylinders. In Sec. IV, we study both single scattering and diffusion of EM waves in two-dimensional (2D) disordered media consisting of (SiO_2) core-shell (InSb) cylinders and discuss some applications. Finally, in Sec. V, we summarize our results and conclude.

II. THE LORENZ-MIE THEORY FOR GYROTROPIC COATED CYLINDERS

To investigate magneto-optical effects in 2D media, we consider a center-symmetric, infinitely long, gyrotropic core-shell cylinder, with inner radius a and outer radius b, normally irradiated with monochromatic plane waves. This scatterer is embedded in an isotropic lossless medium (ε_0, μ_0), where ε and μ are the dielectric permittivity and magnetic permeability, respectively. The material parameters of the coated cylinder are (←→ε_1 , ←→μ_1 ) for the core (0 < r ≤ a) and (←→ε_2 , ←→μ_2 ) for the shell (a < r ≤ b), where the gyroelectric and gyromagnetic tensors are, respectively,

←→ε_q = � � ε_{xx} ε_{xy} 0 ε_{yx} ε_{yy} 0 0 0 ε_{zz} � � = � � ε^⊥_q ıγ_q 0 −ıγ_q ε^⊥_q 0 0 0 ε^{||}q

� � , (1)

←→μ_q = � � μ_{xx} μ_{xy} 0 μ_{yx} μ_{yy} 0 0 0 μ_{zz} � � = � � μ^⊥_q ıη_q 0 −ıη_q μ^⊥_q 0 0 0 μ^{||}_q

� � . (2)

Considering the time harmonic dependence e^{−ıωt}, where ω is the angular frequency, one has the curl Maxwell equations ∇ × (E, H) = ıω(←→μ · H, −←→ε · E). In cylindrical coordinates (r, ϕ, z), there are two irradiation schemes with analytical solutions, as depicted in Fig. 1: the TM polarization or p wave (H||ẑ), which provides the field components E_r and E_ϕ in terms of partial derivatives of H_z ; and the TE polarization or s wave (E||ẑ), which leads to H_r and H_ϕ in terms of partial derivatives of E_z .

Figure 1. A center-symmetric core-shell, infinitely long circular cylinder normally irradiated with plane waves in the Voigt configuration (B ⊥ k). The core has optical properties (ε1, μ_1) and radius a, whereas the shell has (ε2, μ_2) and radius b. The surrounding medium is the vacuum (ε0, μ0). The incident EM fields (E^p_i , H^p_i ) and (E^s_i , H^s_i ) are on p or s polarizations, respectively. The applied external magnetic field satisfies |B| ≫ |μ0Hi|.

For both polarizations, we define the following quantities, used throughout this text:

TM (p) ⇒ � � � ε^p_q ≡ ε^⊥_q [1 − (β^p_q )^2] , μ^p_q ≡ μ^{||}q , β^p_q ≡ γ_q/ε^⊥_q ; (3)

TE (s) ⇒ � � � ε^s_q ≡ ε^{||}_q , μ^s_q ≡ μ^⊥_q [1 − (β^s_q )^2] , β^s_q ≡ η_q /μ^⊥_q . (4)

With this simplified notation, for both p and s waves, β_q = 0 (also known as the Voigt parameter) describes an isotropic 2D medium with (ε_q , μ_q ). In the following, we focus on p-polarized waves and cylinders composed of gyroelectric materials, Eq. (1). The discussion for s polarization is analogous.

A. Electric and magnetic fields for p waves

The EM wave impinging on the cylinder is set as a monochromatic wave propagating with wave vector k = −kx̂ and time harmonic dependence e^{−ıωt}. The scatterer geometry is depicted in Fig. 1. For p-polarized waves in cylindrical coordinate system (r, ϕ, z), we have the ansatz [E^p_i (r, ϕ), H^p_i (r, ϕ)] = (−E_0ŷ, H_0ẑ)e^{−ıkr cos ϕ}, where the electric and magnetic amplitudes are related by E_0 = H_0 � ε_0/μ_0.

Expanding the incident EM field in vector cylindrical harmonics, we obtain for r > b the nonvanishing components

E^p_{ir} = − ∞� n=−∞

E_nn

J_n(kr) kr e^{ınϕ} , (5)

E^p_{iϕ} = −ı ∞� n=−∞

E_nJ^′_n(kr)e^{ınϕ} , (6)

H^p_{iz} = k ωμ_0 ∞� n=−∞

E_nJ_n(kr)e^{ınϕ} , (7)

where E_n = E_0(−ı)^n, k^2 = ω^2ϵ_0μ_0, and J_n is the cylindrical Bessel function. As a consequence, the nonvanishing components of the EM field scattered by the cylinder are, for r > b [1],

E^p_{sr} = − ∞� n=−∞

E_na^p_nn

H^{(1)}_n (kr) kr e^{ınϕ} , (8)

E^p_{sϕ} = −ı ∞� n=−∞

E_na^p_nH^{′(1)}_n (kr)e^{ınϕ} , (9)

H^p_{sz} = k ωμ_0 ∞� n=−∞

E_na^p_nH^{(1)}_n (kr)e^{ınϕ} , (10)

where a_n is the scattering coefficient and H^{(1)}n is the cylindrical Hankel function of the first kind. The form of the scattering coefficient depends on the material properties of the scatterer.

From Maxwell’s equations, one can show that the magnetic field H_q = H_{qz}ẑ within the scatterer must satisfy the following Helmholtz equation [28, 36]: (∇^2 + k^p_q )H_{qz} = 0, where (k^p_q )^2 = ω^2ϵ^p_q μ^p_q . The remaining EM field components are calculated from (k^p_q )^2E_{qr} = ıωμ^p_q [ıβ^p_q ∂/∂r + (1/r)∂/∂ϕ]H_{qz} and (k^p_q )^2E_{qϕ} = −ıωμ^p_q [∂/∂r − (ıβ^p_q /r)∂/∂ϕ]H_{qz} . Explicitly, we have for the core region, q = 1 (0 < r ≤ a),

E^p_{1r} = − ∞� n=−∞

E_nb^p_n ~J_n(k^p_1 r, β^p_1 )e^{ınϕ} , (11)

E^p_{1ϕ} = −ı ∞� n=−∞

E_nb^p_nJ_n(k^p_1 r, β^p_1 )e^{ınϕ} , (12)

H^p_{1z} = k^p_1 ωμ^p_1 ∞� n=−∞

E_nb^p_nJ_n(k^p_1 r)e^{ınϕ} , (13)

where, for the sake of simplicity, we define J_n(ρ, β) ≡ J^′_n(ρ) + βnJ_n(ρ)/ρ and ~J_n(ρ, β) ≡ βJ^′_n(ρ) + nJ_n(ρ)/ρ; and, for the shell region, q = 2 (a ≤ r ≤ b),

E^p_{2r} = − ∞� n=−∞

E_n � c^p_n ~J_n(k^p_2 r, β^p_2 ) + d^p_n ~Y_n(k^p_2 r, β^p_2 ) � e^{ınϕ} ,

(14)

E^p_{2ϕ} = − ı ∞� n=−∞

E_n [c^p_nJ_n(k^p_2 r, β^p_2 ) + d^p_nY_n(k^p_2 r, β^p_2 )] e^{ınϕ} ,

(15)

H^p_{2z} = k^p_2 ωμ^p_2 ∞� n=−∞

E_n [c^p_nJ_n(k^p_2 r) + d^p_nY_n(k^p_2 r)] e^{ınϕ} ,

(16)

where Y_n(ρ, β) ≡ Y^′_n(ρ) + βnY_n(ρ)/ρ and ~Y_n(ρ, β) ≡ βY^′_n(ρ) + nY_n(ρ)/ρ, with Y_n being the cylindrical Neumann function.

The Lorenz-Mie coefficients a^p_n, b^p_n, c^p_n and d^p_n are obtained by imposing the boundary conditions at r = a and r = b, reading:

a^p_n =

~m^p_2 J^′_n(y) [J_n(m^p_2 y) − A^p_nY_n(m^p_2 y)] − J_n(y)α^p_n ~m^p_2 H^{′(1)}n (y) [J_n(m^p_2 y) − A^pnY_n(m^p_2 y)] − H^{(1)}n (y)α^pn , (17)

b^p_n =

~m^p_2 c^p_n [J_n(m^p_2 x) − A^p_nY_n(m^p_2 x)]

~m^p_1 J_n(m^p_1 x)

, (18)

c^p_n =

2ı/(πy) ~m^p_2 H^{′(1)}_n (y) [J_n(m^p_2 y) − A^p_nY_n(m^p_2 y)] − H^{(1)}_n (y)α^p_n , (19) d^p_n = −A^p_nc^p_n , (20) where the auxiliary functions are α^p_n = J_n(m^p_2 y, β^p_2 ) − A^p_nY_n(m^p_2 y, β^p_2 ) ,

A^p_n =

~m^p_1 J_n(m^p_1 x)J_n(m^p_2 x, β^p_2 ) − ~m^p_2 J_n(m^p_1 x, β^p_1 )J_n(m^p_2 x) ~m^p_1 J_n(m^p_1 x)Y_n(m^p_2 x, β^p_2 ) − ~m^p_2 J_n(m^p_1 x, β^p_1 )Y_n(m^p_2 x) , with size parameters x = ka and y = kb. The relative refractive and impedance indices are m^p_q = k^p_q /k = � ε^p_q μ^p_q /(ε_0μ_0) and ~m^p_q = � ε^p_q μ_0/(ε_0μ^p_q ), respectively (m_q = ~m_q if μ_q = μ_0 [30]). Notice that parity symmetry a_{−n} = a_n, b_{−n} = b_n, c_{−n} = c_n and d_{−n} = d_n only holds if β_1 = β_2 = 0, which retrieves the isotropic result for the TM mode [37–39].

The corresponding expressions for s-polarized waves are analogous to the ones above. For the sake of completeness, the multipole expansions and the Lorenz-Mie coefficients (a^s_n, b^s_n, c^s_n, d^s_n) are presented in Appendix A. These expressions are necessary to study cylinders composed of gyromagnetic materials, Eq. (2).

B. Lorenz-Mie efficiencies and multiple scattering

The extinction and scattering efficiencies for cylindrical scatterers at normal incidence are directly calculated via Q_{sca} = (2/y)

�_∞

n=−∞ |an|

2 and Q_{ext} = (2/y)

�_∞

n=−∞ Re(an), respectively, where y = kb is the

size parameter of the outer cylinder. They are defined as the respective cross section of a segment L ≫ b of the infinite cylinder in units of the geometrical cross section 2bL. Rewriting these efficiencies to consider sums for n ≥ 1, one has

Q_{sca} = 2 y � |a_0|^2 + ∞� n=1 � |a_{−n}|^2 + |a_n|^2 � � , (21)

Q_{ext} = 2 y Re � a_0 + ∞� n=1 (a_{−n} + a_n) � , (22)

with Q_{abs} = Q_{ext} − Q_{sca} being the absorption efficiency. The differential scattering efficiency reads

∂Q(ϕ) ∂ϕ = 2 πy � � � �a0 + ∞� n=1 � a_{−n}e^{ınθ} + a_ne^{−ınθ} � � � � � 2 , (23)

where θ = π − ϕ is the scattering angle, so that θ = 0^o corresponds to forward scattering and θ = 180^o corresponds to backscattering. Here we consider the same convention as in Refs. [40] and [28], so that one obtains Q_{sca} by integrating Eq. (23) in the range [0, π] instead of [0, 2π] [41]. The efficiencies for p and s polarizations are obtained by considering a^p_n and a^s_n, respectively, where one must define the quantities (ε_q , μ_q, β_q ) according to relations (3) or (4).

Some quantities calculated in the single scattering approach can be used to study multiple-scattering properties in the diffusive regime and for low concentrations of scatterers [42, 43]. In this regime, the scattering mean free path ℓ_{sca} is comparable to the size of the system and suffices kℓ_{sca} ≫ 1. This situation is depicted in Fig. 2.

The asymmetry parameter ⟨cos θ⟩, which is related to the transferred linear momentum in the forward direc-

Figure 2. A two-dimensional disordered medium composed of identical parallel core-shell cylinders, embedded in the medium (ε0, μ0), normally irradiated with plane waves in the Voigt configuration (B ⊥ k). We consider the distance among the cylinders much greater than their radius and kℓsca ≫ 1 (ℓsca being the scattering mean free path), so that the weak disorder approximation holds. The incident polarization schemes, TM and TE modes, are indicated by (E^p_i , H^p_i ) and (E^s_i , H^s_i ), respectively.

tion [1], is calculated from the relationship

Q_{sca}⟨cos θ⟩ =

�_π 0 dθ ∂Q(ϕ) ∂ϕ cos θ , (24)

where Q_{sca} and ∂Q(ϕ)/∂ϕ are defined in Eqs. (21) and (23), respectively, for a single-scattering process.

The transport mean free path is ℓ^⋆ = 1/(ρσ^⋆), where ρ is the density of particles in the host medium, and σ^⋆ = σ_{ext} − σ_{sca}⟨cos θ⟩ is the transport cross section [44], with σ_{ext} and σ_{sca} being the extinction and scattering cross sections, respectively. Notice that here we take into account unavoidable losses to calculate ℓ^⋆, as in Refs. [44– 46]. For lossless scatterers σ_{ext} = σ_{sca}, so that ℓ^⋆ = ℓ_{sca}/(1 − ⟨cos θ⟩), where ℓ_{sca} = 1/(ρσ_{sca}) is the scattering mean free path. For a disordered 2D medium consisting of parallel cylindrical particles, as depicted in Fig. 2, we obtain

ℓ^⋆ b = π/2 f_{pack} (Q_{ext} − Q_{sca}⟨cos θ⟩)

, (25)

where f_{pack} is the filling fraction. It is convenient to define the extinction mean free path: ℓ_{ext} = πb/(2f_{pack}Q_{ext}). In this 2D case in the Voigt configuration, the effective diffusion coefficient is D = v_Eℓ^⋆/2, where v_E is the energy-transport velocity. Note that D does not depend explicitly on B, which does not apply to the Faraday configuration (B||k) [47]. From the weak disorder approximation of the Bethe-Salpeter equation [42, 43], it follows that

v_E c ≈ 1 f_{pack}(W/W_0 − 1) + 1

, (26)

where c = 1/ √ ε_0μ_0 is the velocity of light in the host medium and W/W_0 is the energy-enhancement factor in a single scatterer, with W being the time-averaged internal EM energy [37–39, 48]. Equation (26), originally calculated for spheres, is not restricted to low densities of scatterers [42] and can successfully be applied to cylinders [49]. In the following, we analytically calculate W/W_0 for a gyrotropic coated cylinder for both p and s waves.

III. THE EXACT ANALYTIC TIME-AVERAGED ENERGY WITHIN GYROTROPIC COATED CYLINDERS

The time-averaged EM energy density within a gyroelectric and gyromagnetic medium (←→ε_q , ←→μ_q ), given by Eqs. (1) and (2), is

⟨u_q⟩_t = 1 4 � ε^{(eff)}_{q⊥} � |E_{qr}|^2 + |E_{qϕ}|^2 � + ε^{(eff)}_{q||} |E_{qz} |^2

+ μ^{(eff)}_{q⊥} � |H_{qr} |^2 + |H_{qϕ}|^2 � + μ^{(eff)}_{q||} |H_{qz} |^2

+ 2Im � γ^{(eff)}_q E_{qr} E^∗_{qϕ} + η^{(eff)}_q H_{qr}H^∗_{qϕ} � � , (27)

where the effective energy coefficients, if the medium is weakly absorbing [50], are ε^{(eff)}_{q⊥} = ∂[ωRe(ε^⊥_q )]/∂ω,

ε^{(eff)}_{q||} = ∂[ωRe(ε^{||}_q )]/∂ω, γ^{(eff)}_q = ∂[ωRe(γ_q )]/∂ω, and so forth. Equation (27) is simplified whether we consider p waves (E_{qz} = H_{qr} = H_{qϕ} = 0) or s waves (H_{qz} = E_{qr} = E_{qϕ} = 0).

From Eq. (27), the corresponding time-averaged EM energy in a segment L of a cylindrical shell l_1 ≤ r ≤ l_2 is, therefore [39],

W_q =

�_{L/2}

−L/2 dz �_{2π} 0 dϕ �_{l2}

l_1

dr r⟨u_q ⟩_t . (28)

If the cylindrical shell l_1 ≤ r ≤ l_2 has the same optical properties as the surrounding medium (ε_0, μ_0), it follows that

W_{0q} = ε_0 2 |E_0|^2π(l^2 − l^2_1)L , (29)

where E_0 is the electric amplitude of the incident wave.

The technical details involved in the analytical derivation of W_q , with q = 1 for (l_1, l_2) = (0, a) and q = 2 for (l_1, l_2) = (a, b), are given in Appendix B. Using the results in Appendix B, let us consider the partial contributions to the internal energy: W^+_{q⊥} = � d^3rε^{(eff)}_{q⊥} (|E_r|^2 + |E_φ|^2)/4, W_{q||} = � d^3rε^{(eff)}_{q||} |E_z |^2/4,

W^−_{q⊥} = � d^3rIm(γ^{(eff)}q E_r E^∗_φ)/2, and so on. For both p or s polarizations, the partial contributions to the EM energy in the cylinder have the same analytical expression, but with the corresponding Lorenz-Mie coefficients and material parameters in the equations.

From Eq. (28), we obtain for the core region (q = 1, l_1 = 0, and l_2 = a)

W^±_{1⊥} W_{01}

= ζ^±_{1⊥} ∞� n=−∞

|b_n|^2F^{±(JJ)}

1,n , (30)

W_{1||} W_{01}

= ζ_{1||} ∞� n=−∞

|b_n|^2I^{(JJ)}_{1,n} , (31)

where we have considered (A, B) = (b_n, 0) into Eqs. (B1) and (B2) in Appendix B to obtain W^+_{1⊥} and W^−_{1⊥}, respectively. The auxiliary functions I^{(JJ)}_{1,n} and F^{±(JJ)}_{1,n} are obtained from Eqs. (B3) [or (B4)] and (B5), respectively, and depend on the product of the Bessel functions. The EM energy within the core (←→ε_1 , ←→μ_1 ) is, therefore,

W_1 = W^+_{1⊥} + W^−_{1⊥} + W_{1||} . (32)

For the cylindrical shell (q = 2, l_1 = a, and l_2 = b), we obtain

W^±_{2⊥} W_{02}

= ζ^±_{2⊥} ∞� n=−∞ � |c_n|^2F^{±(JJ)} 2,n + 2Re � c_nd^∗_nF^{±(JY )} 2,n � + |d_n|^2F^{±(Y Y )} 2,n � , (33)

W_{2||} W_{02}

= ζ_{2||} ∞� n=−∞ � |c_n|^2I^{(JJ)}_{2,n}

+ 2Re � c_nd^∗_nI^{(JY )}_{2,n} � + |d_n|^2I^{(Y Y )}_{2,n} � , (34)

where we have considered (A, B) = (c_n, d_n) into Eqs. (B1) and (B2) in Appendix B to achieve W^+_{2⊥} and W^−_{2⊥}, respectively. The auxiliary functions F^{±(ZZ̄)}_{2,n} and

I^{(ZZ̄)}_{2,n} are defined in Appendix B, where Z and Z̄ are any Bessel (J_n) or Neumann (Y_n) function. The EM energy within the shell (←→ε_2 , ←→μ_2 ) is

W_2 = W^+_{2⊥} + W^−_{2⊥} + W_{2||} . (35)

To obtain the internal energy associated with p or s polarization schemes one must consider Eqs. (3) and (b^p_n, c^p_n, d^p_n) or Eqs. (4) and (b^s_n, c^s_n, d^s_n), respectively, and apply the relations:

TM (p) ⇒ � � � ζ^{p+}_{q⊥} ≡ ε^{(eff)}_{q⊥} /ε_0, ζ^{p−}_{q⊥} ≡ γ^{(eff)}_q /ε_0 , ζ^p_{q||} ≡ | ~m^p_q |^2μ^{(eff)}_{q||} /μ_0 ;

(36)

TE (s) ⇒ � � � ζ^{s+}_{q⊥} ≡ | ~m^s_q |^2μ^{(eff)}_{q⊥} /μ_0, ζ^{s−}_{q⊥} ≡ | ~m^s_q |^2η^{(eff)}_q /μ_0 , ζ^s_{q||} ≡ ε^{(eff)}_{q||} /ε_0 .

(37)

The energy-enhancement factor W_{1,2}/W_0 within the scatterer, where W_{1,2} = W_1 + W_2 is the total internal energy and W_0 = W_{01} + W_{02}, is

W_{1,2} W_0

= S^2

W_1 W_{01} + � 1 − S^2

� W_2

W_{02}

, (38)

with S = a/b being the aspect ratio.

In addition, since the internal field intensities are proportional to the power loss, we can write the absorption efficiency Q^p_{abs} in terms of the partial energy contributions:

Q^p_{abs} πy = Im � S^2 � � ε^{⊥1} ε^{(eff)}_{1⊥}

W^{p+}_{1⊥} W_{01} + γ_1

γ^{(eff)}_1

W^{p−}_{1⊥} W_{01} + μ^{||}_1

μ^{(eff)}_{1||}

W^p_{1||}

W_{01} � �

+ (1 − S^2) � � ε^{⊥2}

ε^{(eff)}_{2⊥}

W^{p+}_{2⊥} W_{02} + γ_2

γ^{(eff)}_2

W^{p−}_{2⊥} W_{02} + μ^{||}_2

μ^{(eff)}_{2||}

W^p_{2||}

W_{02} � � � . (39)

For s waves, Q^s_{abs} is obtained from Eq. (39) by replacing the symbols (ε, γ, μ) with (μ, η, ε) and the label p with s. It is worth mentioning that Eq. (39) provides an explicit connection between the internal energy and a measurable quantity, Q_{abs} [39, 48].

IV. DIELECTRIC MICROCYLINDERS WITH MAGNETO-OPTICAL COATINGS

So far our results are general and can be applied, e.g., to the study of coated gyromagnetic materials and nanowires. Here we focus on a particular case: infinite coated gyroelectric cylinders irradiated with THz p waves. Finite-size effects are known to weakly affect the scattering properties of cylinders provided their length is much larger than both their diameter and the incident wavelength [1, 41, 51]. Provided these conditions are met, light is mostly scattered in the plane perpendicular to the cylinder axis [1]. Some technical details regarding the calculations are provided in Appendix C.

The cylinder is embedded in vacuum (ε_0, μ_0) and consists of a dielectric core made of silica (SiO_2) (ε_1 = 2.25ε_0 and μ_1 = μ_0 in the far-infrared) coated with a cylindrical shell of indium antimonide (InSb), whose dielectric tensor [Eq. (1) for q = 2] reads [52, 53]:

ε^⊥_2 (ω, B, T ) ε_0

= ε_∞ − ω^2_p (ω + Γı) ω � (ω + Γı)^2 − ω^2_c

� , (40)

ε^{||}_2 (ω, B, T ) ε_0

= ε_∞ − ω^2_p ω (ω + Γı)

, (41)

γ_2(ω, B, T ) ε_0 = ω^2_pω_c ω � (ω + Γı)^2 − ω^2_c

� , (42)

where ε_∞ = 15.7 is the high-frequency permittivity. The cyclotron frequency is ω_c = eB/m^⋆, where e is the electron charge, B is the external dc magnetic field, and m^⋆ = 0.015m_e is the effective mass of free carriers, with m_e being the bare mass of the electron. The plasma frequency and the collision frequency of carriers are, respectively, ω_p = � N e^2/(ε_0m^⋆) and Γ = e/(μ_em^⋆), where N is the intrinsic carrier density and μ_e is the electron mobility. The intrinsic carrier density (in cm^{−3}) in undoped InSb is strongly dependent on the temperature and reads [54]:

N (T ) ≈ 5.76 × 10^{14}T^{3/2} exp [−0.129/ (k_BT )] , (43)

where k_B is the Boltzmann constant (in eV K^{−1}). This expression, derived from the temperature variation of the Hall coefficient, agrees well with experimental data for 150 K ≤ T ≤ 300 K [33–35]; for this reason we restrict our analysis to this temperature range. In addition, we employ a realistic empirical expression for the electron Hall mobility (in cm^2V^{−1}s^{−1}) [33]

μ_e(T ) ≈ 7.7 × 10^4 (T/300)^{−5/3} , (44)

which has been experimentally validated in the temperature range 150 K ≤ T ≤ 300 K [35], which we consider here.

For the corresponding energy coefficients in Eq. (27), we consider the Loudon approach [55] to deal with lossy Drude-Lorentz models [56]:

ε^{(eff)}_{2⊥} (ω) = Re � ε^⊥_2 (ω) � + 2ω Γ Im � ε^⊥_2 (ω) � , (45)

γ^{(eff)}_2 (ω) = Re [γ_2(ω)] + 2ω Γ Im [γ_2(ω)] . (46)

We recall that ε^{||}_2 (ω) does not contribute to the scattering by p waves. The remaining energy coefficients are calculated by the usual Landau’s formula for lossless or weakly absorbing media [50]. For non-dispersive media, it is simply the real part.

From Eqs. (40) and (41), note that ε^{||}_2 (ω, T, B) = ε^⊥_2 (ω, T, 0). Using relations (4), i.e., ε^s_2 = ε^{||}_2 and μ^s_2 = μ_0 (with β^s_2 = 0), one can readily verify that scattering for s waves is insensitive to B. Indeed in the Rayleigh limit (kb ≪ 1) for s waves one has |a^s_0| ≫ |a^s_{±1}| for nonmagnetic scatterers [1], and hence the overall scattering response depends on the bulk resonances of the InSb associated with ε^{||}_2 . For this reason, we do not consider s waves in our discussion. In addition, it is worth mentioning that oblique incidence would lead to cross-polarization coupling for higher-order modes, i.e. s or p waves would be scattered in a combination of both s and p polarization states [51]. Since the magneto-optical response is maximal for p waves and vanishes for s waves, oblique incidence would weaken the net magneto-optical effect due to radiation polarization conversion. For this reason, together with the fact that for normal incidence an analytical solution exists, we prefer to focus on the normal incidence case [39, 51].

In Figs. 3(a)–3(c), we show the asymmetry parameter ⟨cos θ⟩, the energy-enhancement factor W_{1,2}/W_0, and

Figure 3. Single scattering by a dielectric SiO2 microcylinder (ε1 = 2.25ε0 ) coated with undoped InSb [ε2 = ε2(ω, B, T ), Eqs. (40)–(44)]. The left panel (a)–(c) corresponds to room temperature (T = 295 K), with the scatterer radius being b = 2.5 μm (kb ≪ 1), and the aspect ratio S = a/b = 0.35. The right panel (d)–(f) corresponds to T = 250 K, with the scatterer radius being b = 25 μm (kb ≈ 1), and the aspect ratio S = a/b = 0.5. The system is normally irradiated with p waves and is subjected to an external magnetic field B = Bẑ. (a) The asymmetry parameter ⟨cos θ⟩ as a function of the frequency f = ω/2π, for various magnetic field amplitudes B. The insets show the extinction efficiency Qext for B = 0.0 T (a^p_1 = a^p_{−1}) and B = 0.5 T (a^p_1 ≠ a^p_{−1}) and the corresponding scattering pattern for B = 0.5 T and f = 2.0 THz. (b) The energy-enhancement factor W1,2/W0 within the core-shell cylinder. (c) The ratio between the transport and the extinction mean free paths ℓ^⋆/ℓext, Eq. (25). The inset shows the ratio between the scattering and the extinction efficiencies Q^p_{sca}/Q^p_{ext}. For the other configuration (kb ≈ 1), one has (d) ⟨cos θ⟩, (e) W1,2/W0 and (f) ℓ^⋆/ℓext as a function of f and B.

the transport mean free path ℓ^⋆, respectively, in a (SiO_2) core-shell (InSb) cylinder for p waves as a function of the frequency and external magnetic field. We set b = 2.5 μm (with aspect ratio S = a/b = 0.35), and room temperature (T = 295 K). The range of size parameters in Figs. 3(a)–3(c) is 0.089 < kb < 0.17, so that dipole contributions to the scattering (n = 0 and n = ±1) are dominant; in particular, the magnetic dipole contribution (n = 0) is negligible since μ_1 = μ_2 = μ_0. Figure 3(a) shows that the application of an external magnetic field B strongly affects the scattering directionality. Indeed, the presence of B breaks the scattering isotropy of dipolar scattering, in contrast to what occurs for non-Faraday-active materials in the Rayleigh regime (kb ≪ 1). In these materials ⟨cos θ⟩ ≈ 0 [1] as a consequence of the typical isotropic dipolar scattering pattern, for which Q^p_{sca} ∝ |a^p_1 |^2. For magneto-optical materials a^p_1 ≠ a^p_{−1} for B ≠ 0 [see the inset of Fig. 3(a)], leading to a strongly asymmetric, magnetic-field-dependent scattering pattern, as shown in Fig. 3(a). In particular, the two peaks related to the dipole resonance for B = 0.0 T are essentially due to the presence of the dielectric core SiO_2. We have verified that as a → 0, only one peak remains for a^p_1 = a^p_{−1} around f = 2.4 THz . Here, the dielectric core broadens the dipole resonance for B = 0.0 T.

Figure 4. Normalized differential scattering efficiency ∂Q(ϕ)/∂ϕ, Eq. (23), for a (SiO2) core-shell (InSb) cylinder with outer radius b = 25 μm and aspect ratio S = a/b = 0.5, for a fixed frequency f = 1.6 THz (kb ≈ 0.84). The system is normally irradiated with p waves and is subjected to an external magnetic field B = Bẑ and temperature T = 250 K. (a) B = 0.0 T, showing preferential forward scattering (⟨cos θ⟩ ≈ 0.63). (b) B = 1.3 T, showing preferential backscattering (⟨cos θ⟩ ≈ −0.32).

Figure 3(a) reveals not only that the presence of B leads to anisotropic scattering (⟨cos θ⟩ ≠ 0), but also that B induces preferential backscattering (⟨cos θ⟩ < 0), which hardly occurs in light-scattering [1]. In particular, the conditions ⟨cos θ⟩ = ±1/2 are known as the first (+) and second (−) Kerker conditions, respectively [17, 31]. Figure 3(a) shows that both Kerker conditions are almost met for certain frequencies and magnetic fields due to the fact that a^p_1 ≠ a^p_{−1}. The appearance of ⟨cos θ⟩ < 0 in the dipole approximation is explained, for p waves, by the far-field interference between the coefficients a^p_1 and a^p_{−1}. This breaking of the degeneracy results in a rotation of the dipolar scattering pattern [see the inset in Fig. 3(a)], whose rotation angle in our notation is [28]

θ_{rot} ≈ 1 2 arctan � Im � a^p_1 a^{p∗}_{−1} � Re � a^p_1 a^{p∗}_{−1} � � . (47)

Conversely, for the stored EM energy, we have nonvanishing interference between the electric-field components (E_{2r}E^∗_{2ϕ}) in the xy plane, as can be seen from the EM energy density expression [see Eq. (27)]. It is worth emphasizing that, in contrast to previous studies on directional scattering [13, 14, 31], our approach does not rely on magnetic resonances since a^p_0 = 0. Rather, it is based on the magnetic-field dependence of electric dipolar resonances a^p_1 and a^p_{−1}.

The breaking of the degeneracy in the scattering coefficients a^p_1 ≠ a^p_{−1} in a magnetic field also shows up in the internal EM energy stored in the cylinder, W_{1,2}, as shown in Fig. 3(b). In fact, by increasing B the internal resonances at a^p_1 and a^p_{−1} become farther apart in frequency, leading to an increasing spectral gap in W_{1,2}. As the internal energy is proportional to the absorption cross section, Q^p_{abs}, for kb ≪ 1 and weak absorption [37, 48], Fig. 3(b) demonstrates a novel way to externally tune EM absorption by applying an external magnetic field. It is worth mentioning that this effect can be achieved for moderate magnetic fields (B ≈ 0.5 T) and that B > 0 shifts a^p_{−1} and a^p_1 to low and high frequencies, respectively; B < 0 does the opposite. In Fig. 3(c), the ratio ℓ^⋆/ℓ_{ext} is shown to demonstrate that a frequency band exists below approximately 2.4 THz in which the anomalous transport regime ℓ^⋆ < ℓ_{ext} occurs. This band can be shifted to lower frequencies by varying B and results from the negative asymmetry parameters in the same frequency range, as shown in Fig. 3(a).

Figueres 3(d)–3(f) demonstrate that it is possible to achieve directional scattering, which can be tuned by applying an external magnetic field, beyond the Rayleigh limit. Indeed, in Figs. 3(d)–3(f) ⟨cos θ⟩, W_{1,2}, and ℓ^⋆ are calculated, respectively, for the same system but now with b = 25 μm (S = a/b = 0.5), and T = 250 K. For the frequency range 0.6 THz to 2.6 THz, size parameters are 0.31 < kb < 1.4, i.e. beyond the Rayleigh limit. In addition, by decreasing the temperature from 295 K to 250 K, absorption of the InSb coating also decreases significantly [see Eqs. (43) and (44)]. The overall result is that for this new set of parameters absorption is small beyond the Rayleigh limit, so that Q_{sca} is comparable to Q_{ext} for B = 0.0 T. In Fig. 3(d), we demonstrate that ⟨cos θ⟩ becomes negative by applying B even for kb ≈ 1. Figure 3(e) shows that the presence of B increases the magnetic dipole contribution a^p_0 for low frequencies (1.2 THz) at the same time that it increases the electric dipole contribution a^p_{±1} for high frequencies (2.4 THz). The interference between electric and magnetic dipole contributions leads to a minimum in the internal energy around f ≈ 1.6 THz as B increases. As shown in Fig. 3(f), this interference induces a band (1.3 THz to 2.0 THz)

Figure 5. Multiple scattering by parallel identical SiO2 microcylinders (ε1 = 2.25ε0 ) coated with undoped InSb [ε2 = ε2(ω, B, T ), Eqs. (40)–(44)], with packing fraction f_{pack} = 35%. The radius of each scatterer is b = 2.5 μm, with corresponding aspect ratio S = a/b = 0.35. The system is normally irradiated with p waves and is subjected to an external magnetic field B = Bẑ and temperature T . (a) The energy-transport velocity v_E (in units of c), Eq. (26), through the disorder medium as a function of the frequency f = ω/2π, for various magnetic field amplitudes B. (b) The corresponding diffusion coefficient D = v_Eℓ^⋆/2 (in units of bc). (c) v_E and (d) D for B = 0.0 T as a function of f and temperature T .

of anomalous scattering in which ℓ^⋆ < ℓ_{ext}. Moreover, for B = 1.3 T, ℓ^⋆ ≈ ℓ_{sca}/(1 − ⟨cos θ⟩) since absorption becomes very small in this frequency range, as can be verified by the inset in Fig. 3(f). This implies that there exists a transport regime in which ℓ^⋆ < ℓ_{sca}, with ℓ^⋆ ≈ 0.8ℓ_{sca}. It is worth mentioning that the application of the external magnetic field can suppress absorption in this frequency range, resulting in Q_{sca}/Q_{ext} ≈ 1, as shown in the inset in Fig. 3(f). It is worth emphasizing that this anomalous scattering regime, induced by the external magnetic field, occurs with the inclusion of unavoidable losses and without consideration of any positional correlation among scatterers, in contrast to Refs. [31] and [32], respectively. In addition, for fixed frequency and material parameters, Fig. 4 shows that we can effectively tune the directional scattering pattern by applying B.

In Fig. 5, we investigate the impact of tunable scattering anisotropy in light transport in planes composed of identical, infinitely long magneto-optical core-shell cylinders, as depicted in Fig. 2. The parameters are the same as in Figs. 3(a)–3(b): b = 2.5 μm, S = a/b = 0.35, and T = 295 K. For a fixed packing fraction f_{pack} = 35% we calculate the energy-transport velocity v_E and the diffusion coefficient D = v_Eℓ^⋆/2. For fixed (room) temperature, Figs. 5(a) and 5(b) show that one can effectively tune light transport with an external magnetic field. Indeed, Figs. 5(a) and 5(b) reveal that the application of an external magnetic field up to B ≈ 1.0 T leads to an increase in v_E and D, increasing diffusion in the plane. In particular, as the magnetic field is increased the diffusion coefficient D becomes maximal at a frequency band where a minimum at ℓ^⋆ and v_E (≈ 0.15c), and hence D, exists for B = 0.0 T. Indeed, at B = 1.1 T, the diffusion coefficient is two orders of magnitude greater than at B = 0.0 T.

In Figs. 5(c) and 5(d), we calculate v_E and D as a function of the frequency fixing all the aforementioned parameters, for B = 0.0 T and for different temperatures. The analysis of these figures reveals that tuning the light scattering and light propagation in-plane with the temperature is also possible. In fact, note that by increasing the temperature from T = 270 K to 300 K one broadens and shifts the band of minimum v_E to high frequencies, and hence the diffusion coefficient D. Also, as the temperature decreases (typically for T > 220 K), smaller magnetic fields are required to achieve a strong magneto-optical response in InSb at high frequencies, in the THz range [53]. This implies that, for T < 295 K, smaller magnetic fields (e.g., B ≈ 0.5 T instead of 1.0 T) could be applied to obtain the same energy-transport velocity enhancement exhibited in Figs. 5(a) and 5(b). This strong dependence on the temperature facilitates the modulation of the EM energy transport, which can be enhanced or attenuated by B and shifted in frequency by varying temperature.

Although we have focused on InSb magneto-optical coatings, there are other materials that could possibly be used to achieve similar results. As alternatives to InSb, one could use, e.g., materials that are known to exhibit a low electron effective mass m^⋆, and hence a high cyclotron frequency ω_c, such as InAs, HgTe, Hg_{1−x}Cd_xTe, PbTe, PbSe, PbS, and GaAs [57, 58]. In cylindrical geometry, all these materials are expected to exhibit a strong magneto-optical effect under a normal incidence of p waves at high frequencies.

V. CONCLUSIONS

Using the Lorenz-Mie theory, we have calculated a set of analytical expressions to completely describe the EM scattering by gyrotropic core-shell magneto-optical cylinders. A closed analytic expression has been derived for the EM energy stored inside the cylinder. For concreteness, using realistic material parameters for the silica core and InSb shell, we have calculated the stored EM energy and the scattering anisotropy. We have shown that the application of an external magnetic field induces a drastic decrease in EM absorption in a frequency window in the THz, where absorption is maximal in the absence of the magnetic field. We have demonstrated not only that the scattering anisotropy can be externally tuned by applying a magnetic field, but also that it can reach negative values in the THz even in the dipolar regime. This is due to the fact that the external magnetic field breaks the degeneracy between the first two electric Mie scattering coefficients, which, without the magnetic field, lead to isotropic scattering. We have shown that this also leads to an anomalous regime of multiple light scattering in a collection of magneto-optical core-shell cylinders, in which the scattering mean free path is longer than the transport mean free path in specific ranges in the THz. In our approach, we have demonstrated an unprecedented degree of external control of multiple light scattering, which can be tuned by either applying an external magnetic field or varying the temperature.

ACKNOWLEDGMENTS

The authors thank W. J. M. Kort-Kamp for fruitful discussions at an early stage of this work and an anonymous referee for valuable comments and suggestions. The authors acknowledge the Brazilian agencies for support. T.J.A. holds grants from FAPESP

(Grant No. 2010/10052-0) and CAPES/PNPD (Grant No. 1564300), and A.S.M. holds grants from CNPq (Grant Nos. 307948/2014-5 and 485155/2013). F.A.P. acknowledges The Royal Society-Newton Advanced Fellowship (Grant No. NA150208), CAPES (Grant No. BEX 1497/14-6), and CNPq (Grant No. 303286/2013- 0) for financial support.

Appendix A: Electric and magnetic fields for s waves

Let us briefly discuss the multipole expansions for TE mode or s polarization. According to Fig. 1, we have: [E^s_i (r, ϕ), H^s_i (r, ϕ)] = (E_0ẑ, H_0ŷ)e^{−ıkr cos ϕ}, with k = −kx̂. By duality relations between electric and magnetic quantities, the EM fields for TE polarization (H^s_i ⊥ ẑ) are readily obtained from Eqs (5)- (16). First, we must redefine the material parameters according to Eq. (4), substituting (ε^p_q , μ^p_q , β^p_q ) with (ε^s_q, μ^s_q , β^s_q ). The field components are then obtained by replacing (E^p_r , E^p_ϕ, H^p_z ) with (−pH^s_r, −pH^s_ϕ, p^{−1}E^s_z ) and (a^p_n, b^p_n, c^p_n, d^p_n) with (a^s_n, b^s_n, c^s_n, d^s_n), where p = ωμ_0/k for the incident and scattered EM fields [Eqs. (5)–(10)] and p = ωμ^s_q /k^s_q for the internal fields [q = 1 for Eqs. (11)– (13) and q = 2 for Eqs. (14)–(16)]. The TE coefficients are a^s_n =

J^′_n(y) [J_n(m^s_2y) − A^s_nY_n(m^s_2y)] − ~m^s_2J_n(y)α^s_n

H^{′(1)}_n (y) [J_n(m^s_2y) − A^s_nY_n(m^s_2y)] − ~m^s_2H^{(1)}_n (y)α^s_n , (A1)

b^s_n = c^s_n [J_n(m^s_2x) − A^s_nY_n(m^s_2x)]

J_n(m^s_1x)

, (A2)

c^s_n =

2ı/(πy)

H^{′(1)}_n (y) [J_n(m^s_2y) − A^s_nY_n(m^s_2y)] − ~m^s_2H^{(1)}_n (y)α^s_n , (A3) d^s_n = −A^s_nc^s_n , (A4)

where the new auxiliary functions are

α^s_n = J_n(m^s_2y, β^s_2) − A^s_nY_n(m^s_2y, β^s_2) ,

A^s_n =

~m^s_2J_n(m^s_1x)J_n(m^s_2x, β^s_2) − ~m^s_1J_n(m^s_1x, β^s_1)J_n(m^s_2x) ~m^s_2J_n(m^s_1x)Y_n(m^s_2x, β^s_2) − ~m^s_1J_n(m^s_1x, β^s_1)Y_n(m^s_2x) ,

and m^s_q = � ε^s_q μ^s_q /(ε_0μ_0) and ~m^s_q = � ε^s_q μ_0/(ε_0μ^s_q).

Appendix B: Integrals of Bessel and Neumann functions

To calculate the stored EM energy W_q defined in Eq. (28), we perform volume integrations involving the product of Bessel and/or Neumann functions. By the recurrence relations nZ_n(ρ) = ρZ_{n−1}(ρ) − ρZ^′_n(ρ) and ρZ^′_n(ρ) = nZ_n(ρ) − ρZ_{n+1}(ρ), for any cylindrical Bessel or Neumann functions Z_n [59], we obtain 2 � �AJ_n(ρ, β) + BY_n(ρ, β) � �^2 + � �A ~J_n(ρ, β) + B ~Y_n(ρ, β) � �^2 � = |1 + β|^2 |AJ_{n−1}(ρ) + BY_{n−1}(ρ)|^2

+ |1 − β|^2 |AJ_{n+1}(ρ) + BY_{n+1}(ρ)|^2 , (B1) 4Re � [AJ_n(ρ, β) + BY_n(ρ, β)]^∗ � A ~J_n(ρ, β) + B ~Y_n(ρ, β) � = |1 + β|^2 |AJ_{n−1}(ρ) + BY_{n−1}(ρ)|^2

− |1 − β|^2 |AJ_{n+1}(ρ) + BY_{n+1}(ρ)|^2 . (B2)

Equations (B1) and (B2) are suitable for simplifying the radial integrals of the field components. Indeed, according to Refs. [39], we define, for m_q ≠ m^∗_q (q = {1, 2}), the auxiliary function

I^{(ZZ̄)}_{q,n} = 1 (l^2 − l^2_1)

�_{l2}

l_1

dr rZ_n(ρ_q )Z̄_n(ρ^∗_q )

= r^2 � ρ^∗_q Z_n(ρ_q)Z̄^′_n(ρ^∗_q ) − ρ_qZ^′_n(ρ_q )Z̄_n(ρ^∗_q ) � (l^2 − l^2_1) � ρ^2_q − ρ^{∗2}_q � � � � � r=l_2

r=l_1 , (B3)

where Z_n and Z̄_n are any cylindrical Bessel or Neumann functions, and l_1, l_2 ∈ R are the integration limits. Using the L’Hospital rule, if m_q = m^∗_q [i.e., Im(m_q ) = 0], Eq. (B3) can be rewritten as

I^{(ZZ̄)}_{q,n} = r^2 4(l^2 − l^2_1) � 2Z_n(ρ_q )Z̄_n(ρ_q )

− Z_{n−1}(ρ_q )Z̄_{n+1}(ρ_q ) − Z_{n+1}(ρ_q )Z̄_{n−1}(ρ_q) � � � � � r=l_2

r=l_1 . (B4)

The case m_q = −m^∗_q [i.e., Re(m_q ) = 0] is discussed in Ref. [39] and plays no role in our analysis. For the sake of simplicity, we define

F^{±(ZZ̄)} q,n = ± 1 2 � |1 + β_q|^2 I^{(ZZ̄)}_{q,n−1} ± |1 − β_q |^2 I^{(ZZ̄)}_{q,n+1} � . (B5)

Appendix C: Numerical calculation of the internal energy

Our numerical results are based on a computer code written for Scilab 5.5.2. For calculations, the infinite sums are truncated in n_{max} = max(N_{Mie}, |m_1|y, |m_2|y) + (101 + y)^{1/2}, where N_{Mie} = y + 4.05y^{1/3} + 2 [60]. This value guarantees the convergence of the scattering quantities [1]. In particular, it is convenient to define the internal energy for n ≥ 1 to perform numerical calculations. To this end, we define the functions

S^±_{1⊥} = 1 2 ∞� n=1 � � |b_{−n}|^2|1 + β_1|^2 ± |b_n|^2|1 − β_1|^2 � I^{(JJ)}_{1,n+1} + � |b_n|^2|1 + β_1|^2 ± |b_{−n}|^2|1 − β_1|^2 � I^{(JJ)}_{1,n−1} � ,

S_{1||} = ∞� n=1 � |b_{−n}|^2 + |b_n|^2 � I^{(JJ)}_{1,n} ,

S^±_{2⊥} = 1 2 ∞� n=1 � � |c_{−n}|^2|1 + β_2|^2 ± |c_n|^2|1 − β_2|^2 � I^{(JJ)}_{2,n+1} + � |c_n|^2|1 + β_2|^2 ± |c_{−n}|^2|1 − β_2|^2 � I^{(JJ)}_{2,n−1} + � |d_{−n}|^2|1 + β_2|^2 ± |d_n|^2|1 − β_2|^2 � I^{(Y Y )}

2,n+1 + � |d_n|^2|1 + β_2|^2 ± |d_{−n}|^2|1 − β_2|^2 � I^{(Y Y )}

2,n−1

+ 2Re � � c_{−n}d^∗_{−n}|1 + β_2|^2 ± c_nd^∗_n|1 − β_2|^2 � I^{(JY )}_{2,n+1} + � c_nd^∗_n|1 + β_2|^2 ± c_{−n}d^∗_{−n}|1 − β_2|^2 � I^{(JY )}_{2,n−1} � , S_{2||} = ∞� n=1 � � |c_{−n}|^2 + |c_n|^2 � I^{(JJ)}_{2,n} + � |d_{−n}|^2 + |d_n|^2 � I^{(Y Y )}

2,n + 2Re � c_{−n}d^∗_{−n} + c_nd^∗_n � I^{(JY )}_{2,n} � � .

With this set of expressions, Eqs. (30)–(35) can be rewrit- ten for both p and s waves, reading

W^+_{1⊥} W_{01}

= ζ^+_{1⊥} � |b_0|^2 � 1 + |β_1|^2 � I^{(JJ)}_{1,1} + S^+_{1⊥} � , (C1)

W^−_{1⊥} W_{01}

= −ζ^−_{1⊥} � 2|b_0|^2Re(β_1)I^{(JJ)}_{1,1} + S^−_{1⊥} � , (C2)

W_{1||} W_{01}

= ζ_{1||} � |b_0|^2I^{(JJ)}_{1,0} + S_{1||} � , (C3)

W^+_{2⊥} W_{02}

= ζ^+_{2⊥} � |c_0|^2 � 1 + |β_2|^2 � I^{(JJ)}_{2,1} + 2Re � c_0d^∗_0 � 1 + |β_2|^2 � I^{(JY )}_{2,1} � + |d_0|^2 � 1 + |β_2|^2 � I^{(Y Y )}

2,1 + S^+_{2⊥} � , (C4)

W^−_{2⊥} W_{02}

= −ζ^−_{2⊥} � 2|c_0|^2Re(β_2)I^{(JJ)}_{2,1} + 4Re � c_0d^∗_0Re(β_2)I^{(JY )}_{2,1} � + 2|d_0|^2Re(β_2)I^{(Y Y )}_{2,1} + S^−_{2⊥} � , (C5)

W_{2||} W_{02}

= ζ_{2||} � |c_0|^2I^{(JJ)}_{2,0} + 2Re � c_0d^∗_0I^{(JY )}_{2,0} � + |d_0|^2I^{(Y Y )}_{2,0} + S_{2||} � . (C6)

[1] C. F. Bohren and D. R. Huffman, Absorption and Scattering of Light by Small Particles (Wiley, New York, 1983).

[2] R. Huschka, J. Zuloaga, M. W. Knight, L. V. Brown, P.

Nordlander, and N. J. Halas, J. Am. Chem. Soc. 133, 12247 (2011).

[3] A. Alù and N. Engheta, Phys. Rev. Lett. 100, 113901 (2008).

[4] B. Edwards, A. Alù, M. G. Silveirinha, and N. Engheta, Phys. Rev. Lett. 103, 153901 (2009).

[5] W. J. M. Kort-Kamp, F. S. S. Rosa, F. A. Pinheiro, and C. Farina, Phys. Rev. Lett. 111, 215504 (2013).

[6] M. I. Tribelsky, A. E. Miroshnichenko, and Y. S. Kivshar, Europhys. Lett. 97, 44005 (2012).

[7] T. J. Arruda, A. S. Martinez, and F. A. Pinheiro, Phys.

Rev. A 87, 043841 (2013); 92, 023835 (2015) [8] H. L. Chen and L. Gao, Opt. Express 21, 23619 (2013). [9] J. Sancho-Parramon and D. Jelovina, Nanoscale 6, 13555 (2014).

[10] A. E. Miroshnichenko, B. Luk’yanchuk, S. A. Maier, and Y. S. Kivshar ACS Nano 6, 837 (2012).

[11] A. I. Kuznetsov, A. E. Miroshnichenko, Y. H. Fu, J.

Zhang, and B. Luk’yanchuk, Sci. Rep. 2, 492 (2012). [12] Z. Ruan and S. Fan, Phys. Rev. Lett., 105, 013901 (2010).

[13] W. Liu, A. E. Miroshnichenko, D. N. Neshev, and Y. S.

Kivshar, ACS Nano 6, 5489 (2012).

[14] W. Liu, A. E. Miroshnichenko, R. F. Oulton, D. N. Neshev, O. Hess, and Y. S. Kivshar, Opt. Lett. 38, 2621 (2013).

[15] B. S. Luk’yanchuk and V. Ternovsky, Phys. Rev. B 73, 235432 (2006).

[16] A. Garcia-Etxarri, R. Gomez-Medina, L. S. Froufe-Perez, C. Lopez, L. Chantada, F. Scheffold, J. Aizpurua, M. Nieto-Vesperinas, and J. J. Saenz, Opt. Express 19, 4815 (2011).

[17] M. Kerker, D. S. Wang, and L. Giles J. Opt. Soc. Am.

73, 765 (1983).

[18] I. Staude, A. E. Miroshnichenko, M. Decker, N. T. Fofang, S. Liu, E. Gonzales, J. Dominguez, T. S. Luk, D.

N. Neshev, I. Brener, and Y. Kivshar, ACS Nano 7, 7824 (2013).

[19] M. Nieto-Vesperinas, R. Gomez-Medina, and J. J. Saenz, J. Opt. Soc. Am. A 18, 54 (2011).

[20] T. Coenen, F. Bernal Arango, A. Femius Koenderink, and A. Polman, Nat. Commun. 5, 3250 (2014).

[21] Y. H. Fu, A. I. Kuznetsov, A. E. Miroshnichenko, Y. F.

Yu, and B. Luk’yanchuk, Nat. Commun. 4, 1527 (2013). [22] X. Zambrana-Puyalto, I. Fernandez-Corbaton, M. L.

Juan, X. Vidal, and G. Molina-Terriza, Opt. Lett. 38, 1857 (2013).

[23] I. M. Hancu, A. G. Curto, M. Castro-Lopez, M. Kuttge, and N. F. Van Hulst, Nano Lett. 14, 166 (2014).

[24] S. Person, M. Jain, Z. Lapin, J. J. Saenz, G. Wicks, and L. Novotny Nano Letters 13, 1806 (2013).

[25] J. M. Geffrin, B. Garcia-Camara, R. Gomez-Medina, P.

Albella, L.S. Froufe-Perez, C. Eyraud, A. Litman, R. Vaillon, F. Gonzalez, M. Nieto-Vesperinas, J. J. Saenz, and F. Moreno Nat. Comm. 3, 1171 (2012).

[26] R. Alaee, R. Filter, D. Lehr, F. Lederer, and C. Rockstuhl, Opt. Lett. 40, 2645 (2015).

[27] Y. Li, M. Wan, W. Wu, Z. Chen, P. Zhan, and Z. Wang, Sci. Rep. 5 12491 (2015).

[28] W. J. M. Kort-Kamp, F. S. S. Rosa, F. A. Pinheiro, and C. Farina, J. Opt. Soc. Am. A 31, 1969 (2014); W. J. M. Kort-Kamp, arXiv:1505.02333.

[29] D. Lacoste, B. A. van Tiggelen, G. L. J. A. Rikken, and A. Sparenberg, J. Opt. Soc. Am. A 15, 1636 (1998).

[30] F. A. Pinheiro, A. S. Martinez, and L. C. Sampaio, Phys.

Rev. Lett. 84, 1435 (2000); 85, 5563 (2000).

[31] R. Gomez-Medina, L. S. Froufe-Perez, M. Yepez, F.

Scheffold, M. Nieto-Vesperinas, and J. J. Saenz, Phys. Rev. A 85, 035802 (2012).

[32] G. M. Conley, M. Burresi, F. Pratesi, K. Vynck, and D.

S. Wiersma, Phys. Rev. Lett. 112, 143901 (2014). [33] O. Madelung, Physics of III-V Compounds, (Wiley, New York, 1964).

[34] M. Oszwalldowski and M. Zimpel, J. Phys. Chem. Solids 49, 1179 (1988).

[35] S. C. Howells and L. A. Schlie, Appl. Phys. Lett. 69, 550 (1996).

[36] J. C. Monzon and N. J. Damaskos, IEEE Trans. Antennas Propag. AP-34, 1243 (1986).

[37] T. J. Arruda and A. S. Martinez, J. Opt. Soc. Am. A 27, 992 (2010); 27, 1679 (2010).

[38] T. J. Arruda, F. A. Pinheiro, and A. S. Martinez, J. Opt.

14, 065101 (2012).

[39] T. J. Arruda, A. S. Martinez, and F. A. Pinheiro, J. Opt.

Soc. Am. A 31, 1811 (2013); 30, 1205 (2013); 32, 943 (2015).

[40] B. S. Luk’yanchuk, A. E. Miroshnichenko, and Y. S.

Kivshar, J. Opt. 15, 073001 (2013).

[41] H. C. van de Hulst, Light Scattering by Small Particles (Dover, New York, 1981).

[42] M. P. van Albada, B. A. van Tiggelen, A. Lagendijk, and A. Tip, Phys. Rev. Lett. 66, 3132 (1991).

[43] B. A. van Tiggelen, A. Lagendijk, M. P. van Albada, and A. Tip, Phys. Rev. B 45, 12233 (1992).

[44] A. Ishimaru, Wave Propagation and Scattering in Random Media (Academic Press, New York, 1978).

[45] A. Ishimaru, Y. Kuga, R. L.-T. Cheung, and K. Shimizu, J. Op. Soc. Am. 73, 131 (1983).

[46] R. Aronson and N. Corngold, J. Opt. Soc. Am. A 16, 1066 (1999).

[47] A. S. Martinez and R. Maynard, Phys. Rev. B 50, 3714 (1994).

[48] A. Bott and W. Zdunkowski, J. Opt. Soc. Am. A 4, 1361 (1987).

[49] R. Ruppin, J. Opt. Soc. Am. A 15, 1891 (1998). [50] L. D. Landau and E. M. Lifshits, Electrodynamics of Continuous Media (Pergamon Press, Oxford, 1984).

[51] A. Alù, D. Rainwater, and A. Kerkhoff, New J. Phys. 12, 103028 (2010).

[52] X. Dai, Y. Xiang, S. Wen, and H. He, J. Appl. Phys.

109, 053104 (2011).

[53] S. Chen, F. Fan, X. He, M. Chen, and S. Chang, App.

Opt. 54, 9177 (2015).

[54] R. W. Cunningham and J. B. Gruber, J. Appl. Phys. 41, 1804 (1970).

[55] R. Loudon, J. Phys. A: Gen. Phys. 3, 233 (1970). [56] R. Ruppin, Phys. Lett. A. 299, 309 (2002). [57] W. Zawadzki, Adv. Phys. 23, 435 (1974). [58] A. Raymond, J. L. Robert, and C. Bernard, J. Phys. C:

Solid State Phys. 12, 2289 (1979).

[59] G. N. Watson, A Treatise on the Theory of Bessel Functions (Cambridge Univ. Press, Cambridge, 1958).

[60] P. W. Barber and S. C. Hill, Light Scattering by Particles: Computational Methods (World Scientific, Singapore, 1990).