arXiv:1802.00263v1 [cs.IT] 1 Feb 2018

Robust Sequential Detection in Distributed Sensor Networks

Mark R. Leonard, Student Member, IEEE, and Abdelhak M. Zoubir, Fellow, IEEE

Abstract—We consider the problem of sequential binary hypothesis testing with a distributed sensor network in a non- Gaussian noise environment. To this end, we present a general formulation of the Consensus + Innovations Sequential Probability Ratio Test (CISPRT). Furthermore, we introduce two different concepts for robustifying the CISPRT and propose four different algorithms, namely, the Least-Favorable-Density- CISPRT, the Median-CISPRT, the M-CISPRT, and the Myriad- CISPRT. Subsequently, we analyze their suitability for different binary hypothesis tests before verifying and evaluating their performance in a shift-in-mean and a shift-in-variance scenario.

Index Terms—sequential hypothesis testing, sequential detection, robustness, distributed sensor networks, distributed detection

I. INTRODUCTION

The paradigm of sequential hypothesis testing is to make a reliable decision for one out of two or more hypotheses based on as few measurements as possible. This work is concerned with robust sequential binary hypothesis tests of the shift-in-mean and shift-in-variance type in distributed sensor networks. These kinds of tests play an important role in modern realtime applications such as intelligent traffic control, smart homes, or video surveillance [1]. We consider sequential tests to make a decision as soon as enough data has been collected to guarantee a certain level of confidence [2]. In addition, the tests are performed in a distributed fashion to avoid having a single point of failure and exploit the inherent scalability and fault-tolerance a sensor network provides [3]. Furthermore, we are interested in tests that are robust against distributional uncertainties such as outliers encountered in realworld scenarios where the assumption of Gaussianity is often violated [4].

The concepts of sequential detection [1], [2], [5]–[7], distributed signal processing in wireless sensor networks [8]– [13], and robustness [4], [14]–[19] are well-established fields of research. Also the combinations of either two of them, i.e., distributed sequential detection [20]–[23], robust sequential detection [19], [24]–[26], and robust hypothesis testing in distributed sensor networks [21], [27]–[30], have received considerable attention in recent years. To the best of our knowledge, the union of sequential hypothesis testing, a distributed network architecture, and robustness is an important niche area that has not been treated in the literature, yet.

M. R. Leonard and A. M. Zoubir are with the Signal Processing Group, Institute of Telecommunications, Technische Universität Darmstadt, Darmstadt 64283, Germany (e-mail: leonard@spg.tu-darmstadt.de, zoubir@spg.tudarmstadt.de)

Manuscript submitted

This work contains the following contributions: We develop a general formulation for the Consensus + Innovations Sequential Probability Ratio Test (CISPRT) from [23] that (a) is applicable to arbitrary binary hypothesis tests, and (b) works with right-stochastic weighting matrices, which makes it suitable for common distributed detection problems. Furthermore, we propose a robust version of the CISPRT, dubbed LFD-CISPRT, based on the concept of least-favorable densities (LFDs). To this end, we derive the probability density function of the robust log-likelihood ratio of the LFDs and show how to calculate its mean and variance. Subsequently, we present an alternative method to robustify the CISPRT, which introduces robust estimators into the test statistic update. With the Median-CISPRT, the M-CISPRT, and the Myriad- CISPRT we propose three robust distributed sequential detectors based on this concept and analyze their suitability for Gaussian shift-in-mean and shift-in-variance tests. These results generalize and extend our first approaches from [31] and [32] and provide a unified framework for robust sequential detection in distributed sensor networks. An extension of some of the presented concepts to multiple hypothesis tests can be found in [33].

The paper is structured as follows: In Section II we formulate the problem of distributed sequential shift-in-mean and shift-in-variance tests in the face of distributional uncentainties. Section III is dedicated to the reformulation of the CISPRT with the decision thresholds being derived in Section IV. The robustification of the CISPRT based on LFDs is presented in Section V, the concept based on robust estimators in Section VI. In Section VII we present simulation results, which verify and evaluate the performance of our proposed algorithms in a shift-in-mean and a shift-in-variance test. Conclusions are drawn in Section VIII.

II. PROBLEM FORMULATION Let Y (t) ∈ R^N , t = 1, 2, . . . be a sequence of random vectors with entries Y_k(t), k = 1, . . . , N. For all k and t the random variables Y_k(t) are assumed to be independent and identically distributed according to distribution P , which admits a density p. Furthermore, consider a network of N agents, which can be modeled as a simple, connected, and undirected graph G = (V, E) with V denoting the set of agents and E being the set of edges between these agents. The open neighborhood of agent k is given by N_k = {l ∈ V | (k, l) ∈ E}, i.e., the set of all agents to which k is connected by an edge.

In distributed sequential detection, each agent k, k = 1, . . . , N, sequentially performs a binary statistical hypothesis test to decide between the null hypothesis H_0 and the alternative H_1 given by

H_0 : P = P_0 H_1 : P = P_1.

To this end, each node k takes a measurement y_k(t) at time instant t from which a test statistic is computed. Considering a Gaussian environment, the hypotheses can be rewritten in terms of the corresponding random variable Y_k(t) as

H_0 : Y_k(t) ∼ N (μ_0, σ^2_0 ) H_1 : Y_k(t) ∼ N (μ_1, σ^2_1 ), (1) where μ_i, i ∈ {0, 1} is the known mean and σ^2_i the variance of a zero-mean Gaussian noise process. While all of our results can be applied to any binary hypothesis test of this type, we will focus on the following two test scenarios:

1) Scenario 1: Shift-in-Mean Test

We test for the mean of the distribution under the true hypothesis assuming equal variance σ^2 under both H_0 and H_1. The hypotheses become

H_0 : Y_k(t) ∼ N (μ_0, σ^2), H_1 : Y_k(t) ∼ N (μ_1, σ^2). (2) 2) Scenario 2: Shift-in-Variance Test

We test for the variance of the distribution under the true hypothesis assuming two zero-mean Gaussian distributions. An example for this is a test for the presence or absence of a signal with known variance σ^2_x in noise with power σ^2_n, i.e.,

H_0 : Y_k(t) ∼ N (0, σ^2_n), H_1 : Y_k(t) ∼ N (0, σ^2_x + σ^2_n). (3) In many practical applications there is an uncertainty about the distribution of the data such that the assumption of Gaussian measurement noise might be violated. Taking these uncertainties into account transforms the test into one between two disjoint probability sets P_0 and P_1 with

H_0 : P ∈ P_0, H_1 : P ∈ P_1.

In Sections V and VI we present two different methods to robustify distributed sequential detectors based on the CISPRT against distributional uncertainties. We do this by limiting the influence of outliers on the test such that the required probabilities of false alarm and misdetection are still fulfilled. As the simulation results in Section VII show, this comes at no or minimal cost in terms of the average run length of the test.

III. A GENERAL FORMULATION OF THE CISPRT

In [22], [23], the authors propose the CISPRT as a distributed sequential detector based on the consensus+innovations approach [34]. In analogy to the centralized SPRT introduced by Wald [2], each agent k in the CISPRT compares its test statistic S_k(t) at time instant t with an upper and a lower threshold to either decide for one of the two hypotheses if the respective threshold is crossed, or continue the test. S_k(t) is recursively calculated as [22], [23]

S_k(t) = ∑ l∈N_k ∪{k} w_{kl} (S_l(t − 1) + η_l(t)) , (4)

with w_{kl} denoting appropriate combination weights that sum to one. Furthermore, η_l(t) is the log-likelihood ratio of node l at time instant t, which is calculated as

η_l(t) = log ( p_1(y_l(t)) p_0(y_l(t)) )

= log ( σ_0 σ_1 e^− (yl(t)−μ1 )2 2σ2 1 e (yl (t)−μ0 )2 2σ2 0 )

= σ^2_1 (y_l(t) − μ_0)^2 − σ^2_0 (y_l(t) − μ_1)^2 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

(5) assuming the general formulation from Eq. (1). By collecting the combination weights into an N × N combination matrix, Eq. (4) can be rewritten as

S_k(t) = t∑ j=1 e^⊤_k W^{t+1−l}η(j), (6) with e_k denoting the kth column of identity matrix I of size N. Furthermore, vector η(j) = [η_1(j), . . . , η_N (j)]^⊤ collects the log-likelihood ratios of all agents at time instant j. In the sequel, we discuss how to choose the combination matrix W .

A. The Choice of Weighting Matrix W

In [23], the authors assume a weighting matrix that is nonnegative, symmetric, irreducible, and stochastic by design. However, the design process relies on a method originally introduced in [35], which can and most of the time does produce a matrix with negative weights as explicitly stated by the authors. In the context of distributed detection, such a matrix is not practical since it will cause the information of some of the collaborating nodes to be given a negative weight. This operation has no meaning in distributed sensor networks.

Instead of requiring the weighting matrix to be non-negative, symmetric, irreducible, and stochastic, we consider a rightstochastic matrix, the rows of which sum up to one. Matrices of this kind are common, e.g., in the context of diffusion adaptation [10]. An example for a right-stochastic matrix is one that puts equal weight on the information of the closed neighborhood of a node, i.e., the entries of W are given by w_{k,l} = {_1 |N_k ∪{k}| , l ∈ Nk ∪ {k} 0 , otherwise .

IV. DECISION THRESHOLDS FOR THE CISP RT The decision thresholds derived in [23] suffer from two disadvantages. First, they only hold for the specific case of symmetric Gaussian shift-in-mean hypothesis tests. In [31] and [32], we generalized these thresholds for use in arbitrary binary hypothesis tests. Second, the derivation of the thresholds relies on the symmetry of W , an assumption that is usually not valid in distributed sensor networks. In the sequel, we improve the generalized thresholds from [31] and [32] by requiring only the right-stochasticity of W in the derivation. First, however, expressions for the mean and the variance of the test statistic under H_0 and H_1 are derived, which will be needed in the subsequent steps.

A. Mean and Variance of the Test Statistic

The expected value of the test statistic in Eq. (4) under hypothesis H_i, i ∈ {0, 1} is given by E_i{S_k(t)} = t∑ j=1 e^⊤_k W^{t+1−j} E_i{η(j)}

= μ_{η,i} t∑ j=1 e^⊤_k W^{t+1−j} 1 = μ_{η,i}t,

(7)

where E_i{·} denotes taking the expectation under hypothesis H_i, μ_{η,i} = E_i{η(j)} is the expected value of the loglikelihood ratio under H_i, and 1 is the one-vector of length N. The variance of the test statistic in Eq. (4) under hypothesis H_i can be calculated as Var_i{S_k(t)} = E_i{(S_k(t) − μ_{η,i}t)^2} = E_i{S_k(t)^2} − 2μ_{η,i}tE_i{S_k(t)^2} + μ^2_{η,i}t^2 = E_i{S_k(t)^2} − μ^2_{η,i}t^2 = E_i t∑ j=1 e^⊤_k W^{t+1−j} η(j) 2 − μ^2_{η,i}t^2

= t∑ j=1 t∑ l=1 e^⊤_k W^{t+1−j} E_i {η(j)η(l)} ( W^{t+1−l} )_⊤ e_k − μ^2_{η,i}t^2. Since E_i {η(j)η(l)} = { μ^2_{η,i}11^⊤ , j ≠ l σ^2_{η,i}I + μ^2_{η,i}11^⊤ , j = l , where σ^2_{η,i} denotes the variance of the log-likelihood ratio under H_i. By rearranging the two sums, we obtain

Var_i{S_k(t)} = σ^2_{η,i} t∑ j=1 e^⊤_k W^j ( W^j )_⊤ e_k

+ μ^2_{η,i} t∑ j=1 t∑ l=1 W^j 11^⊤ ( W^l )_⊤ e_k − μ^2_{η,i}t^2

= σ^2_{η,i} t∑ j=1 e^⊤_k W^j ( W^j )_⊤ e_k + μ^2_{η,i}t^2 − μ^2_{η,i}t^2

= σ^2_{η,i} t∑ j=1 e^⊤_k W^j ( W^j )_⊤ e_k

= σ^2_{η,i} t∑ j=1 e^⊤_k W^{j−m}W^m ( W^⊤ )_m ( W^⊤ )_{j−m} e_k, with 1 ≤ m ≤ j. By upper-bounding the (k, k)th entry of W^m ( W^⊤ )_m with a scalar ξ according to e_kW^m ( W^⊤ )_m e^⊤_k ≤ ξ11^⊤ and using the properties

W 11^⊤ = 11^⊤ 11^⊤W^⊤ = 11^⊤ W 11^⊤W^⊤ = 11^⊤

an upper bound on the variance of the test statistic can be found as Var_i{S_k(t)} ≤ σ^2_{η,i}ξt. (8) A suitable choice for ξ is the maximum value of the matrix W^m ( W^⊤ )_m , i.e., ξ = ‖ ‖W^m ( W^⊤ )_m‖ ‖_{max} , (9)

where ‖ · ‖_{max} is the max norm of a matrix. Another choice for ξ is the largest eigenvalue of W^m ( W^⊤ )_m divided by the number of nodes N, i.e., ξ = 1 N λ_{max} ( W^m ( W^⊤ )_m) . (10)

Note that the accuracy of this approximation can be tuned by the choice of m and thus traded off against computational load. In most distributed sensor networks, computational power at the individual nodes is a scarce resource, which is why it makes sense to choose m = 1. However, if more computational power is available, a higher accuracy can be achieved by choosing a larger value for m.

The resulting expressions for the mean and the variance of the test statistic depend on the mean and the variance of the log-likelihood ratio η_k(t) of node k at time instant t. For a general binary hypothesis test as defined in Eq. (1) it can be shown that these quantities are given by μ_{η,0} = − μ^2_0 + μ^2_1 − 2μ_0μ_1 + σ^2_0 − σ^2_1 2σ^2_1

+ log ( σ_0 σ_1 )

μ_{η,1} = μ^2_0 + μ^2_1 − 2μ_0μ_1 + σ^2_1 − σ^2_0 2σ^2_0

+ log ( σ_0 σ_1

) (11)

σ^2_{η,0} = 1 2 ( 1 + σ^4_0 σ^4_1 ) + (μ_0 − μ_1)^2 σ^2_0 σ^4_1 − σ^2_0 σ^2_1

σ^2_{η,1} = 1 2 ( 1 + σ^4_1 σ^4_0 ) + (μ_0 − μ_1)^2 σ^2_1 σ^4_0 − σ^2_1 σ^2_0 . (12)

The derivation of Eqs. (11) and (12) is detailed in Appendix A. B. Derivation of the Decision Thresholds

The test can easily be shown to terminate almost surely at a finite stopping time T_k with T_k = inf {t|S_k(t) /∈ [λ, υ]} ,

SUBMITTED FOR PUBLICATION 4

PSfrag replacements

(a)

PSfrag replacements

(b) Fig. 1: Shift-in-variance test: (a) probability density function of the log-likelihood ratio and (b) evolution over time of the probability density function of the test statistic S_k(t) of an agent with 3 neighbors

where λ and υ denote the lower and upper decision threshold, respectively. A decision is then made at each node k according to if S_k(T_k) ≤ λ : decide for H_0, if S_k(T_k) ≥ λ : decide for H_1.

Since S_k(T ) is well-defined, the probability of false alarm can be written as [23]

P_{FA} = P_0(S_k(T ) ≥ υ) ≤ ∞∑ t=1 P_0(S_k(t) ≥ υ)

≈ ∞∑ t=1 Q ( υ − μ_{η,0}t σ_{η,0} √ ξt ) , (13)

where Q(x) denotes the tail probability of the standard normal distribution. Inequality (13) holds true as long as the test statistic follows a Gaussian distribution. This is always the case in a shift-in-mean setup since the log-likelihood ratio is also Gaussian distributed. For shift-in-variance tests, the log-likelihood ratio follows a chi-squared distribution with 1 degree of freedom as shown in Fig. 1(a). Hence, we can use the central limit theorem to state that Eq. (13) is approximately true after just a few time steps as depicted in Fig. 1(b). For more details on this, see Section VI-D.

Using the property Q(x) ≤^1_2 e^{− x22} and taking a similar approach as the authors in [23], we obtain

P_{FA} ≤ 2e υμη,0 4σ2 η,0 ξ 1 − e^− μ2 η,0 2σ2 η,0 ξ .

Requiring P_{FA} ≤ α and solving for υ yields the upper threshold

υ ≥ 4σ^2_{η,0}ξ μ_{η,0} log ( α 2 ) + log 1 − e^− μ2η,0 2σ2 η,0 ξ . (14)

Repeating the same procedure for the probability of misdetection and requiring P_{MD} ≤ β yields the lower threshold λ ≤ 4σ^2_{η,1}ξ μ_{η,1} log ( β 2 ) + log 1 − e^− μ2η,1 2σ2 η,1 ξ . (15)

As mentioned in [23], tighter thresholds can be obtained by numerically solving 1 2 ∞∑ t=1 e −λ2−μ2η,1 t2 +2λμη,1 t 2σ2 η,1 ξt = β 1 2 ∞∑ t=1 e −υ2 −μ2η,0 t2+2υμη,0 t 2σ2 η,0 ξt = α. (16)

The complete derivation is given in Appendix B.

V. ROBUST DISTRIBUTED SEQUENTIAL DETECTION

USING THE LFD-CISP RT

In this section we use to the concept of least-favorable densities (LFDs) to modify the CISPRT such that it can deal with composite hypotheses arising from distributional uncertainties.

A. Least-favorable Densities (LFDs)

The set of possible distributions P_i under hypothesis H_i can be characterized with the help of Kassam’s band model [26], [36] as

P_i = { P_i | | | p^′_i ≤ pi ≤ p^{′′}_i } , i.e., the true density p_i is assumed to lie within a band specified by p^′_i and p^{′′}_i . A pair of densities (q_0, q_1) within the respective bands is said to be least favorable if they characterize the worst case of a centralized fixed-sample-size test between H_0 and H_1. Using the algorithm in [26, Table 1], we can iteratively calculate the LFDs as

q_0 = min {p^{′′}_0 , max {c_0(νq_0 + q_1), p^′_0}} q_1 = min {p^{′′}_1 , max {c_1(q_0 + νq_1), p^′_1}}

(17) for some ν ≥ 0 and some c_0, c_1 ∈ (0,^1_ν ]. We assume uncertainties of the ε-contamination type [4], i.e., p_i = (1 − ε)p^0_i + εh_i = p^′_i + εh_i,

(18)

with contamination factor ε, and p^0_i and h_i denoting the nominal and the contamination distribution under H_i, respectively. To represent ε-contamination with Kassam’s band model we set p^{′′}_0 = p^{′′}_1 = ∞ and ν = 0 in Eq. (17), which reduces to [26] q_0 = max {c_0q_1, p^′_0} q_1 = max {c_1q_0, p^′_1} .

(19)

The resulting densities correspond to the LFDs of Huber’s clipped likelihood ratio test [15], [17], which censors outliers and, thus, prevents them from having an unbounded effect on the test. Due to this property, it makes sense to use the centralized, fixed-sample-size LFDs also in the context of distributed sequential detection. While they are not minimax optimal in this case, they induce robustness by limiting the influence of large values at the cost of an increased average run length as we will see in Section VII.

B. The Robust Test Static and Its Density

In order to design a robust version of the CISPRT we replace the log-likelihood ratio η_k (t) of agent k at time instant t in Eq. (4) by the corresponding clipped log-likelihood ratio η^c_k(t) with

η^c_k(t) = log ( q_1(y_k(t)) q_0(y_k(t)) ) . (20)

This yields a robust test statistic Š_k(t) as

Š_k(t) = ∑ l∈N_k ∪{k} w_{kl} (ˇ S_l(t − 1) + η^c_l (t) ) . (21)

The probability density of η^c_k(t) is shown in the exemplary histogram in Fig. 2. Considering ε-contamination as defined in Eq. (18), the density is composed of two terms. The first one corresponds to the density of the regular log-likelihood ratio under the nominal distribution scaled by (1 − ε). The second one is the probability of drawing an outlier—denoted by ϵ. In the worst case, which is represented by the LFDs, the probability of drawing an outlier is placed at the maximum (minimum) of the log-likelihood ratio under H_0 (H_1). The probability density is then clipped at C_0 = − log (c_0) and C_1 = log (c_1) to avoid an unbounded influence of outliers. The excess probability that accumulates at the clipping points can be calculated as

A_{0,i} = Q_i(η_k(t) ≤ C_0) = (1 − ε)P^0_i (η_k (t) ≤ C_0) + iε ≈ (1 − ε)Q ( − C_0 − μ_p0_i σ^2_{p0i} ) + iε A_{1,i} = Q_i(η_k(t) ≥ C_1) = (1 − ε)P^0_i (η_k (t) ≥ C_1) + (1 − i)ε ≈ (1 − ε)Q ( C_1 − μ_p0_i σ^2_{p0i} ) + (1 − i)ε,

PSfrag replacements

Fig. 2: Typical histogram of the clipped log-likelihood ratio η^c_k(t) under H_0 and ε-contaminated noise with ε = 0.1

where μ_p0_i and σ^2_p0_i denote the mean and the variance of the nominal distribution under H_i, i ∈ [0, 1].

C. Mean and Variance of the Robust Test Statistic

The mean and the variance of the robust test statistic can be calculated by finding expressions for the mean μ_ηc_{,i} and the variance σ^2_ηc_{,i} of the clipped log-likelihood ratio under H_i first. Since the distribution is equal for all agents, the superscript k is dropped in the following derivation. We approximate the probability density from Fig. 2 by two weighted Kronecker deltas at C_0 and C_1 with a weighted uniform distribution in between. Note that the uniform distribution is just one convenient possibility to approach the density in this interval of extremely low weight compared to the two Kronecker deltas at the end points. The mean μ_ηc_{,i} and the variance σ^2_ηc_{,i} of the robust log-likelihood ratio are calculated according to

μ_ηc_{,i} = E_i{η^c} = ∫ Ω p_ηc_{,i}(x)x dx = ∫_{C1} C_0

(A_{0,i}δ(x − C_0) + A_{1,i}δ(x − C_1) + A_{2,i}) x dx

= A_{0,i}C_0 + A_{1,i}C_1 + 1 2 [ A_{2,i}x^2 ]_{C1} C_0

= A_{0,i}C_0 + A_{1,i}C_1 + A_{2,i}

C^2_1 − C^2_0 2 , (22)

SUBMITTED FOR PUBLICATION 6

PSfrag replacements

Fig. 3: Evolution of the probability density function of the robust test statisticŠ_k(t) of an agent with 3 neighbors over time

and σ^2_ηc_{,i} = E_i{(η^c)^2} − μ^2_ηc_{,i} = ∫ Ω p_ηc_{,i}(x)x^2 dx − μ^2_ηc_{,i} = ∫_{C1} C_0

(A_{0,i}δ(x − C_0) + A_{1,i}δ(x − C_1) + A_{2,i}) x^2 dx

− μ^2_ηc_{,i}

= A_{0,i}C^2_0 + A_{1,i}C^2_1 + A_{2,i}

C^3_1 − C^3_0 3 − μ^2_ηc_{,i}, (23)

respectively, with A_{2,i} =^{(1−A0,i −A1,i)}_{C1−C0} .

The derivation of the mean and the variance of the nonrobust test statistic S_k(t) in Section IV-A is based on the assumption of a Gaussian-distributed log-likelihood ratio η_k(t). While this assumption does not hold for the clipped loglikelihood ratio η^c_k(t), we can resort to the central limit theorem to state that the robust test statistic Š_k(t) is approximately normal [37], [38]. The evolution of the probability density function of Š_k(t) over time is depicted in Fig. 3 for an agent with three neighbors. As can be seen, the data exchange over the neighborhood causes the probability density function to become approximately Gaussian already after the first few time instants. An even faster convergence can be observed in denser networks. Hence, the mean and variance of Š_k(t) can be calculated by replacing μ_{η,i} and σ^2_{η,i} in (7) and (8) with their robust counterparts, i.e.,

E_i{Š_k(t)} = μ_ηc_{,i}t (24) Var_i{Š_k(t)} ≤ σ^2_ηc_{,i}ξt. (25)

D. Robust Decision Thresholds

The mean and the variance of the robust test statistic Š_k(t) in Eqs. (24) and (25) have the same form as those of the nonrobust test statistic S_k(t) in Eqs. (7) and (8). Therefore, we can derive robust decision thresholds by following the paradigm from Section IV-B, i.e., by replacing the mean and the variance of the log-likelihood ratio η_k(t) in Eqs. (14) and (15) with those of the clipped log-likelihood ratio η^c_k(t) from Eqs. (22) and (23). Thus, we obtain υ̌ ≥ 4σ^2_ηc_{,0}ξ μ_ηc_{,0} log (α 2 ) + log 1 − e^− μ2 ηc ,0 2σ2 ηc ,0 ξ

λ̌ ≤ 4σ^{2ηc ,1}ξ μ_ηc_{,1} log ( β 2 ) + log 1 − e^− μ2 ηc ,1 2σ2 ηc ,1 ξ , (26)

with tighter bounds arising from numerically evaluating 1 2 ∞∑ t=1 e −λ2−μ2 ηc ,1 t2 +2λμηc ,1t 2σ2 ηc ,1 ξt = β 1 2 ∞∑ t=1 e −υ2−μ2 ηc ,0 t2+2υμηc ,0t 2σ2 ηc ,0 ξt = α. (27)

VI. ROBUST DISTRIBUTED SEQUENTIAL DETECTION

USING ROBUST ESTIMATORS

In this section we show how to leverage the diversity of a distributed sensor network along with robust estimators to introduce robustness through the update equation of the CISPRT. We start by reformulating Eq. (4) as

S_k(t) = ∑ l∈N_k ∪{k} w_{kl} (S_l(t − 1)) + η̂_k(t), (28)

with η̂_k(t) denoting the weighted average of the collective innovations terms of node k and its neighborhood at time t. When no a priori knowledge about the reliability of the nodes is available, a common choice is to weight all the information equally. This leads to η̂_k(t) being the sample mean

η̂^{mean}_k (t) = 1 |N_k ∪ {k}| ∑ l∈N_k ∪{k} η_l(t), (29)

which is a non-robust estimator [4]. Since the update equation is recursive, replacing the sample mean with a robust alternative will robustify the consensus part as well and, thus, yield a test statistic that can handle distributional uncertainties. An advantage of introducing robustness in this manner instead of using LFDs as detailed in the previous section is the fact that the censoring takes place one stage later. Instead of clipping the log-likelihood ratio directly, the effect of large values on the innovations term is bounded by using a robust estimator in the combination rule. Thus, the thresholds and decision rules of the original CISPRT, which are based on the mean and the variance of the log-likelihood ratio, remain valid.

A first attempt at using this approach was presented in [32], where we successfully used the median, the M-estimator, and the sample myriad [39], [40] for sequential detection. In the sequel, we will briefly summarize these algorithms and investigate their suitability for different binary hypothesis tests.

A. The Median-CISPRT

A straightforward way of replacing the sample mean in Eq. (28) with a robust alternative is to use the median η̂^{median}_k (t). The estimate of the innovations term is calculated as

η̂^{median} k (t) = { η_k(^{|Nk |+1}_2 ) , |N_k| even 1 2 ( η_k(^{|Nk |+1}_2 ) + η_k(^{|Nk |+1}_2 + 1) ) , |N_k| odd , (30)

with η_k(t) denoting the vector of the log-likelihood ratios of node k and its neighbors sorted in ascending order.

B. The M-CISPRT

The M-CISPRT is obtained by using an M-estimate of the neighborhood-wide innovations part in Equation (28). Intuitively speaking, the M-estimator provides a weighted average with weights given by [4]

W (x) = {_{ψ(x)} x , x ≠ 0 ψ^′(0) , x = 0 , where ψ(x) is a score function and ψ^′(x) its first derivative. In this work we consider Huber’s score function defined as [4], [17]

ψ_{Hub}(x) = { x , |x| ≤ c_{Hub} c_{Hub}sign(x) , |x| > c_{Hub} ,

for some postive constant c_{Hub}.

The M-estimate of the innovations term is obtained by recursively calculating [4], [17] w_k(t, i) = W ( η_k (t) − η̂^M_k (t, i) σ̂(η_k(t)) ) (31)

η̂^M_k (t, i + 1) = ∑ l∈N_k ∪{k} wl(i)ηl(t, i) ∑ l∈N_k ∪{k} wl(i) (32)

until^{|η̂Mk (t,i+1)−η̂Mk (t,i)|} σ̂(η_k (t)) < ε for a small, positive constant ε.

The algorithm is initialized by setting η̂^M_k (t, 0) = η̂^{median}_k (t) and estimating the scale using the normalized median standard deviation according to [4]

σ̂_{mad}(η_k(t)) = 1.483 · median ( |η_k(t) − η̂^{median}_k (t)| ) , where the median is calculated as in Eq. (30).

C. The Myriad-CISPRT

The third robust estimator we consider in this work is the sample myriad, which estimates the innovations term according to [39], [40]

η̂^{myriad} k (t) = arg min_η ∏ l∈N_k ∪{k} [ m^2 + (η_l(t) − η)^2 ] (33)

where m is a freely tunable parameter. A common choice is to set m = σ̂_{mad}(η(t)) [40].

D. The Probability Density Function of the Log-Likelihood Ratio

We are concerned with shift-in-mean as well as shift-in-variance tests. In order to investigate the suitability of the proposed detectors in these two cases, we take a look at the probability density function of the estimator input, i.e., the neighborhood innovations of node k. Since uncontaminated measurements are assumed to be Gaussian, we can write

y_k(t) = μ^∘ + x(t)σ^∘,

where x(t) ∼ N (0, 1), and μ^∘ and σ^∘ denote the true mean and standard deviation of y_k(t). The log-likelihood ratio of node k as defined in Eq. (5) now becomes

Shift-in-mean (σ_0 = σ_1 = σ):

η_k(t) = σ^2_1 (y_k(t) − μ_0)^2 − σ^2_0 (y_k(t) − μ_1)^2 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= (y_k(t) − μ_0)^2 − (y_k(t) − μ_1)^2 2σ^2 = (σ^∘x(t) + (μ^∘ − μ_0))^2 − (σ^∘x(t) + (μ^∘ − μ_1))^2 2σ^2 = x(t) σ^∘ σ^2

(μ_1 − μ_0) +

(μ^∘ − μ_0)^2 − (μ^∘ − μ_1)^2 2σ^2 = ax(t) + b. Shift-in-variance (μ_0 = μ_1 = μ^∘ = 0):

η_k(t) = σ^2_1 (y_k(t) − μ_0)^2 − σ^2_0 (y_k(t) − μ_1)^2 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= σ^2_1 y_k(t)^2 − σ^2_0 y_k(t)^2

2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= y_k(t)^2 σ^2_1 − σ^2_0 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= (σ^∘)^2 x^2(t) σ^2_1 − σ^2_0 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= cx^2(t) + d.

The values of a, b, c, and d are clear from the context. Thus, in the shift-in-mean test η_k(t) follows a Gaussian distribution. In the shift-in-variance test, however, this is not the case. Since x(t) follows the standard normal distribution, x^2(t) is chisquared distributed with one degree of freedom, i.e., x^2(t) ∼ χ^2_1. Hence, the log-likelihood ratio follows a scaled and shifted χ^2_1 distribution, which is not symmetric but skewed.

Regarding our proposed algorithms, this has the following implication: Since the median is only a robust estimator for

PSfrag replacements

PSfrag replacements

Fig. 4: Simulation results for the shift-in-mean test. Due to the symmetry, the results are equal under H_0 and H_1

the mean of symmetric distributions, the Median-CISPRT is not suitable for general shift-in-variance problems. It might give correct detection results for certain parameter choices as can be seen in the promising simulation results from [32], but we cannot guarantee a reliable performance for arbitrary shift-in-variance tests. Therefore, we will consider the Median- CISPRT only for shift-in-mean tests.

VII. SIMULATIONS In this section, we evaluate and compare the performance of the proposed version of the CISPRT and the proposed robust detectors in the face of ε-contaminated noise. To this end, we consider the two different test scenarios introduced in Section II. In both scenarios, we use a network of N = 20 agents with uniformly distributed x- and y-coordinates on the interval [0, 1]. Agents within a radius of g = 0.6 are considered to be neighbors. The required false alarm and misdetection probabilities are assumed to be equal, ranging from 10^{−3} to 10^{−1}. To assess the performance of the different algorithms, we evaluate the average run length as well as the empirical error probabilities, i.e., the probability of false alarm when H_0 is true and the probability of misdetection under H_1. The results are averaged over N_{MC} = 10 000 Monte Carlo runs.

A. Scenario 1: Shift-in-Mean Test

In the first scenario, we consider a shift-in-mean problem where the objective is to decide between μ_0 = − 1 and μ_1 = 1 based on measurements that are disturbed by ε-contaminated noise. Here, σ^2 = 2, the amount of contamination is ε = 0.1, and contaminated measurements suffer from a ten times higher variance.

The simulation results are shown in Fig. 4. Due to the symmetry of the problem, the results are equal under both hypotheses. We observe that our proposed robust detection algorithms all meet and even fall below the required error probability while the CISPRT fails as the requirements get more stringent. At the same time, the Median-CISPRT, the

M-CISPRT, and the Myriad-CISPRT exhibit a slightly lower average run length than the CISPRT. Hence, the robustness property does not come at the cost of a higher testing time. This is in contrast to our results from [32], where the robustification via robust estimators came with a premium in average run length. This effect can be explained by the different decision thresholds due to the different weighting matrices. The decision thresholds in [32] are tighter than the ones proposed in this work but they are derived based on certain properties of the weighting matrix that are not meaningful in distributed detection setups as discussed in Section III-A. Thus, we can conclude that in a common shift-in-mean test, the introduction of robustness through robust estimators does not increase the average run length. The LFD-CISPRT, in contrast, needs more than twice the testing time than the CISPRT. This is in line with the results from [31] and [32] and due to the fact that the LFDs optimize the algorithm for the worst case, which is not attained by randomly sampling from an ε-contaminated distribution.

As far as the required error probabilities are concerned, all robust algorithms overachieve, i.e., they do not take advantage of the tolerable number of errors but deliver a probability of false alarm and misdetection close to zero. This can be explained by the way the decision thresholds are derived in Sections IV-B and V-D. As mentioned in [23], the approximations required to find a closed-form solution result in thresholds that are sufficient but not optimal.

B. Scenario 2: Shift-in-Variance Test

The second scenario is a shift-in-variance test. We test for the presence or absence of a signal with variance σ^2_x = 4. The noise variance is σ^2_n = 1, the amount of contamination is ε = 0.1, and contaminated measurements suffer from a ten times higher variance.

The simulation results are shown in Fig. 5, where the upper row considers the case where H_0 is true and the lower one pertains to H_1. Under H_0, the CISPRT breaks down while

PSfrag replacements

PSfrag replacements

PSfrag replacements

PSfrag replacements

Fig. 5: Simulation results for the shift-in-variance test under H_0 (upper row) and H_1 (lower row)

all robust algorithms meet and even fall below the required error probabilities due to the sufficient conditions on the decision thresholds. Under H_1, however, all algorithms—even the non-robust CISPRT—meet the error requirements. This is an expected result since, in a shift-in-variance test, outliers, i.e., very large values, actually help in correctly deciding for H_1. As far as the average run length is concerned, the robust algorithms exhibit a five to twelve times larger testing time in the more difficult case where H_0 is true. Moreover, the LFD-CISPRT is in line with the other robust detectors, which indicates that the considered scenario approaches the worst case. Under H_1, i.e., in the easier case, the average run length of the robust estimator approach is just a few time instants larger than that of the non-robust CISPRT while the LFD- CISPRT, again, needs considerably longer to complete the test.

VIII. CONCLUSION

In this work, we presented a general formulation of the CISPRT that is not only suitable for sequential binary hypothesis tests but also considers a network structure that is meaningful in the context of distributed detection. Furthermore, we presented two different approaches for robustifying the CISPRT and proposed four different robust sequential detection algorithms, namely, the LFD-CISPRT, the Median- CISPRT, the M-CISPRT, and the Myriad-CISPRT. After investigating their suitability for different test setups, we verified, evaluated, and compared their performance in a shiftin-mean and a shift-in-variance test. Our simulation results showed that the proposed detectors are robust against outliers of the ε-contamination type at no or minimal extra cost in terms of the average run length. Only the LFD-CISPRT comes with a notable increase in testing time due to its focus on the worst-case.

APPENDIX A MEAN AND VARIANCE OF THE LOG-LIKELIHOOD RATIO

In the following, we derive the mean and the variance of the log-likelihood ratio under the null hypothesis. The derivation under the alternative is analogous. To this end, we make use of the identities

E{y^2} = μ^2_y + σ^2_y E{y^3} = μ^3_y + 3μ_yσ^2_y E{y^4} = μ^4_y + 6μ^2_yσ^2_y + 3σ^4_y.

Note that we drop the superscript k since the measurements at each agent are assumed to be independently and identically distributed. For the sake of simplicity, the time dependence is omitted as well.

μ_{η,0} = E_0 { σ^2_1 (y − μ_0)^2 − σ^2_0 (y − μ_1)^2 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )}

= E_0 { σ^2_1 ( y^2 − 2μ_0y + μ^2_0 ) − σ^2_0 ( y^2 − 2μ_1y + μ^2_1 ) 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )}

= σ^2_1 ( E_0{y^2} − 2μ_0E_0{y} + μ^2_0 ) 2σ^2_0 σ^2_1 − σ^2_0 ( E_0{y^2} − 2μ_1E_0{y} + μ^2_1 ) 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= σ^2_1 ( μ^2_0 + σ^2_0 − 2μ^2_0 + μ^2_0 ) 2σ^2_0 σ^2_1 − σ^2_0 ( μ^2_0 + σ^2_0 − 2μ_0μ_1 + μ^2_1 ) 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= σ^2_1 σ^2_0 − σ^2_0 ( μ^2_0 + σ^2_0 − 2μ_0μ_1 + μ^2_1 ) 2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 )

= − μ^2_0 + μ^2_1 − 2μ_0μ_1 + σ^2_0 − σ^2_1 2σ^2_1

Z_1

+ log ( σ_0 σ_1 )

Z_2

E_0{η^2} = E_0 ( σ^2_1 (y − μ_0)^2 − σ^2_0 (y − μ_1)^2

2σ^2_0 σ^2_1

+ log ( σ_0 σ_1 ))2

= E_0 ( σ^2_1 (y − μ_0)^2 − σ^2_0 (y − μ_1)^2

)_2

4σ^4_0 σ^4_1

+ log ( σ_0 σ_1

)_2 + 2 σ^2_1 (y − μ_0)^2 − σ^2_0 (y − μ_1)^2 2σ^2_0 σ^2_1 log ( σ_0 σ_1 )

=

Z_3

E_0 ( σ^2_1 (y − μ_0)^2 − σ^2_0 (y − μ_1)^2

)_2

4σ^4_0 σ^4_1

+ log ( σ_0 σ_1

)_2

+ 2E_0 { σ^2_1 (y − μ_0)^2 − σ^2_0 (y − μ_1)^2 2σ^2_0 σ^2_1 } log ( σ_0 σ_1 )

= Z_3 + Z^2_2 + 2Z_1Z_2

Z_3 = E_0 ( σ^2_1 (y − μ_0)^2 − σ^2_0 (y − μ_1)^2

)_2

4σ^4_0 σ^4_1

= E_0 {( σ^2_1 ( y^2 − 2μ_0y + μ^2_0 ) − σ^2_0 ( y^2 − 2μ_1y + μ^2_1 ))_2 4σ^4_0 σ^4_1 }

= E_0 { σ^4_1 ( y^2 − 2μ_0y + μ^2_0

)_2

+ σ^4_0 ( y^2 − 2μ_1y + μ^2_1

)_2

4σ^4_0 σ^4_1 } E_0 { ( y^2 − 2μ_0y + μ^2_0 ) ( y^2 − 2μ_1y + μ^2_1 ) 2σ^2_0 σ^2_1 }

= E_0 {( y^4 + 4μ^2_0y^2 + μ^4_0 − 4μ_0y^3 + 2μ^2_0y^2 − 4μ^3_0y ) 4σ^4_0 } + E_0 { ( y^4 + 4μ^2_1y^2 + μ^4_1 − 4μ_1y^3 + 2μ^2_1y^2 − 4μ^3_1y ) 4σ^4_1 }

− E_0 { ( y^4 + 4μ_0μ_1y^2 + μ^2_0μ^2_1 − 2μ_1y^3 − 2μ_0y^3 + μ^2_0y^2 + μ^2_1y^2 − 2μ_0μ^2_1y − 2μ^2_0μ_1y ) 2σ^2_0 σ^2_1 }

Z_3 = ( E_0{y^4} + 4μ^2_0E_0{y^2} + μ^4_0 − 4μ_0E_0{y^3} + 2μ^2_0E_0{y^2} − 4μ^3_0E_0{y} ) 4σ^4_0 + ( E_0{y^4} + 4μ^2_1E_0{y^2} + μ^4_1 − 4μ_1E_0{y^3} + 2μ^2_1E_0{y^2} − 4μ^3_1E_0{y} ) 4σ^4_1 − ( E_0{y^4} + 4μ_0μ_1E_0{y^2} + μ^2_0μ^2_1 − 2μ_1E_0{y^3} − 2μ_0E_0{y^3} + μ^2_0E_0{y^2} + μ^2_1E_0{y^2} − 2μ_0μ^2_1E_0{y} − 2μ^2_0μ_1E_0{y} ) 2σ^2_0 σ^2_1 = μ^4_0 + 6μ^2_0σ^2_0 + 3σ^4_0 + 6μ^4_0 + 6μ^2_0σ^2_0 − 4μ^4_0 − 12μ^2_0σ^2_0 − 4μ^4_0 + μ^4_0 4σ^4_0 + μ^4_0 + 6μ^2_0σ^2_0 + 3σ^4_0 + 6μ^2_0μ^2_1 + 6μ^2_1σ^2_0 − 4μ^3_0μ_1 − 12μ_0μ_1σ^2_0 − 4μ_0μ^3_1 + μ^4_1 4σ^4_1 − μ^4_0 + 6μ^2_0σ^2_0 + 3σ^4_0 + ( μ^2_0 + σ^2_0 ) ( 4μ_0μ_1 + μ^2_0 + μ^2_1 ) − ( μ^3_0 + 3μ_0σ^2_0 ) (2μ_0 + 2μ_1) − μ_0 ( 2μ_0μ^2_1 + 2μ^2_0μ_1 ) + μ^2_0μ^2_1 2σ^2_0 σ^2_1 = 3 4 + μ^4_0 + μ^4_1 − 4 ( μ^3_0μ_1 + μ_0μ^3_1 ) + 6 ( μ^2_0σ^2_0 + μ^2_1σ^2_0 + μ^2_0μ^2_1 − 2μ_0μ_1σ^2_0 ) + 3σ^4_0 4σ^4_1 − μ^4_0 + 6μ^2_0σ^2_0 + 3σ^4_0 + 4μ^3_0μ_1 + μ^4_0 + μ^2_0μ^2_1 + 4μ_0μ_1σ^2_0 + μ^2_0σ^2_0 + μ^2_1σ^2_0 2σ^2_0 σ^2_1 − −2μ^4_0 − 2μ^3_0μ_1 − 6μ^2_0σ^2_0 − 6μ_0μ_1σ^2_0 − 2μ^2_0μ^2_1 − 2μ^3_0μ_1 + μ^2_0μ^2_1 2σ^2_0 σ^2_1 = 3 4 + μ^4_0 + μ^4_1 − 4 ( μ^3_0μ_1 + μ_0μ^3_1 ) + 6 ( μ^2_0σ^2_0 + μ^2_1σ^2_0 + μ^2_0μ^2_1 − 2μ_0μ_1σ^2_0 ) + 3σ^4_0 4σ^4_1 − 3σ^2_0 − 2μ_0μ_1 + μ^2_0 + μ^2_1 2σ^2_1

σ^2_{η,0} = E_0{η^2} − μ^2_{η,0} = Z_3 + Z^2_2 + 2Z_1Z_2 − ( Z^2_1 + Z^2_2 + 2Z_1Z_2 )

= Z_3 − ( μ^2_0 + μ^2_1 − 2μ_0μ_1 + σ^2_0 − σ^2_1

)_2

4σ^4_1

= Z_3 − μ^4_0 + μ^4_1 + 4μ^2_0μ^2_1 + σ^4_0 + σ^4_1 + 2μ^2_0μ^2_1 − 4μ^3_0μ_1 + 2μ^2_0σ^2_0 − 2μ^2_0σ^2_1 − 4μ_0μ^3_1 4σ^4_1 − 2μ^2_1σ^2_0 − 2μ^2_1σ^2_1 − 4μ_0μ_1σ^2_0 + 4μ_0μ_1σ^2_1 − 2σ^2_0 σ^2_1 4σ^4_1 = 3 4 + 4σ^2_0 (μ_0 − μ_1)^2 + 2σ^4_0 − σ^4_1 + 2σ^2_1 (μ_0 − μ_1)^2 + 2σ^2_0 σ^2_1 4σ^4_1 − 3σ^2_0 + (μ_0 − μ_1)^2

2σ^2_1 = 1 2 ( 1 + σ^4_0 σ^4_1 ) + (μ_0 − μ_1)^2 σ^2_0 σ^4_1 − σ^2_0 σ^2_1

The mean and the variance of the log-likelihood ratio under the alternative hypothesis are given by

μ_{η,1} = μ^2_0 + μ^2_1 − 2μ_0μ_1 + σ^2_1 − σ^2_0 2σ^2_0

+ log ( σ_0 σ_1 )

σ^2_{η,1} = 1 2 ( 1 + σ^4_1 σ^4_0 ) + (μ_0 − μ_1)^2 σ^2_1 σ^4_0 − σ^2_1 σ^2_0 .

APPENDIX B DECISION THRESHOLDS FOR THE CISPRT

The probability of false alarm can be written as [23]

P_{FA} = P_0(S_k(T ) ≥ υ) ≤ ∞∑ t=1 P_0(S_k(t) ≥ υ)

≤ ∞∑ t=1 Q ( υ − μ_{η,0}t σ_{η,0} √ ξt ) .

SUBMITTED FOR PUBLICATION 12

Using the property Q(x) ≤^1_2 e^{− x22} and following the derivation in [23], we obtain

P_{FA} ≤ 1 2 ∞∑ t=1 e −υ2−μ2η,0 t2+2υμη,0 t 2σ2 η,0 ξt

= 1 2 e υμη,0 σ2 η,0 ξ ∞∑ t=1 e −υ2 −μ2η,0 t2 2σ2 η,0 ξt

= 1 2 e υμη,0 σ2 η,0 ξ ⌊^υ_{2μη,0} ⌋ ∑ t=1 e −υ2−μ2η,0 t2 2σ2 η,0 ξt + ⌊^υ_{μη,0} ⌋ ∑ t=⌊^υ_{2μη,0} ⌋+1 e −υ2−μ2η,0 t2 2σ2 η,0 ξt + ⌊^{2υ}_{μη,0} ⌋ ∑ t=⌊^υ_{μη,0} ⌋+1 e −υ2 −μ2η,0 t2 2σ2 η,0 ξt + ∞∑ t=⌊^{2υ}_{μη,0} ⌋+1 e −υ2−μ2η,0 t2 2σ2 η,0 ξt

≤ 1 2 e υμη,0 σ2 η,0 ξ e^− υμη,0 σ2 η,0 ξ ⌊^υ_{2μη,0} ⌋ ∑ t=1 e^− μ2η,0 t 2σ2 η,0 ξ + e^− υμη,0 2σ2 η,0 ξ ⌊^υ_{μη,0} ⌋ ∑ t=⌊^υ_{2μη,0} ⌋+1 e^− μ2η,0 t 2σ2 η,0 ξ + e^− υμη,0 4σ2 η,0 ξ ⌊^{2υ}_{μη,0} ⌋ ∑ t=⌊^υ_{μη,0} ⌋+1 e^− μ2η,0 t 2σ2 η,0 ξ + ∞∑ t=⌊^{2υ}_{μη,0} ⌋+1 e^− μ2η,0 t 2σ2 η,0 ξ .

Approximating the sums above with infinite geometric series as in [23] and using the relation ∞∑ t=0 ar^t = a 1 − r , for |r| < 1, leads to an upper bound on the probability of false alarm according to

P_{FA} ≤ 1 2 e υμη,0 σ2 η,0 ξ 1 − e^− μ2 η,0 2σ2 η,0 ξ [ e^− υμη,0 σ2 η,0 ξ + e^− υμη,0 2σ2 η,0 ξ e^− υμη,0 4σ2 η,0 ξ + e^− υμη,0 4σ2 η,0 ξ e^− υμη,0 2σ2 η,0 ξ + e^− υμη,0 σ2 η,0 ξ ]

≤ e 4υμη,0 4σ2 η,0 ξ 1 − e^− μ2 η,0 2σ2 η,0 ξ [ e^− 4υμη,0 4σ2 η,0 ξ + e^− 3υμη,0 4σ2 η,0 ξ ]

≤ 2e υμη,0 4σ2 η,0 ξ 1 − e^− μ2 η,0 2σ2 η,0 ξ .

Requiring P_{FA} ≤ α and solving for υ yields the upper threshold υ as α ≤ 2e υμη,0 4σ2 η,0 ξ 1 − e^− μ2 η,0 2σ2 η,0 ξ α 2 1 − e^− μ2η,0 2σ2 η,0 ξ ≤ e υμη,0 4σ2 η,0 ξ

log ( α 2 ) + log 1 − e^− μ2η,0 2σ2 η,0 ξ ≤ υμ^{η,0} 4σ^2_{η,0}ξ

υ ≥ 4σ^2_{η,0}ξ μ_{η,0} log ( α 2 ) + log 1 − e^− μ2η,0 2σ2 η,0 ξ . Repeating the same procedure for the probability of misdetection and requiring P_{MD} ≤ β yields the lower threshold λ ≤ 4σ^2_{η,1}ξ μ_{η,1} log ( β 2 ) + log 1 − e^− μ2η,1 2σ2 η,1 ξ .

REFERENCES

[1] A. Tartakovsky, I. Nikiforov, and M. Basseville, Sequential Analysis:

Hypothesis Testing and Changepoint Detection. Boca Raton, Florida, USA: CRC Press, 2014.

[2] A. Wald, Sequential Analysis. New York City, New York, USA: Wiley, 1947.

[3] I. F. Akyildiz, W. Su, Y. Sankarasubramaniam, and E. Cayirci, “A survey on sensor networks,” IEEE Communications Magazine, vol. 40, no. 8, pp. 102–114, Aug 2002.

[4] A. M. Zoubir, V. Koivunen, Y. Chakhchoukh, and M. Muma, “Robust estimation in signal processing: A tutorial-style treatment of fundamental concepts,” IEEE Signal Processing Magazine, vol. 29, no. 4, pp. 61–80, July 2012.

[5] A. Novikov, “Optimal sequential multiple hypothesis tests,” Kybernetika, vol. 45, no. 2, pp. 309–330, 2009.

[6] ——, “Optimal sequential tests for two simple hypotheses,” Sequential analysis, vol. 28, no. 2, pp. 188–217, 2009.

[7] M. Fauß and A. M. Zoubir, “A linear programming approach to sequential hypothesis testing,” Sequential Analysis, vol. 34, no. 2, pp. 235–263, 2015.

[8] F. S. Cattivelli and A. H. Sayed, “Distributed detection over adaptive networks using diffusion adaptation,” IEEE Transactions on Signal Processing, vol. 59, no. 5, pp. 1917–1932, 2011.

[9] S.-Y. Tu and A. H. Sayed, “Mobile adaptive networks,” IEEE Journal of Selected Topics in Signal Processing, vol. 5, no. 4, pp. 649–664, 2011.

[10] A. H. Sayed, “Diffusion adaptation over networks,” in E-Reference Signal Processing, R. Chellappa and S. Theodoridis, Eds. New York: Elsevier, 2013.

[11] M. R. Balthasar, S. Al-Sayed, S. Leier, and A. M. Zoubir, “Optimal area coverage in autonomous sensor networks,” in Proceedings of the 2nd International Conference and Exhibition on Underwater Acoustics (UA2014), June 2014.

[12] M. R. Leonard and A. M. Zoubir, “Multi-target tracking in distributed sensor networks using particle PHD filters,” 2015, available online: https://arxiv.org/abs/1505.01668.

[13] V. Matta, P. Braca, S. Marano, and A. H. Sayed, “Distributed detection over adaptive networks: Refined asymptotics and the role of connectivity,” IEEE Transactions on Signal and Information Processing over Networks, vol. 2, no. 4, pp. 442–460, 2016.

[14] P. J. Huber, “Robust estimation of a location parameter,” The Annals of Mathematical Statistics, vol. 35, no. 1, pp. 73–101, 1964.

[15] ——, “A robust version of the probability ratio test,” The Annals of Mathematical Statistics, vol. 36, no. 6, pp. 1753–1758, 1965.

[16] P. J. Huber and V. Strassen, “Minimax tests and the Neyman-Pearson lemma for capacities,” The Annals of Statistics, pp. 251–263, 1973.

[17] P. J. Huber, Robust Statistics. Hoboken, New Jersey, USA: Wiley, 1981. [18] B. C. Levy, Principles of signal detection and parameter estimation.

Springer Science & Business Media, 2008.

[19] G. Gül and A. M. Zoubir, “Minimax robust hypothesis testing,” IEEE Transactions on Information Theory, 2017.

[20] D. Teneketzis and Y.-C. Ho, “The decentralized Wald problem,” Information and Computation, vol. 73, no. 1, pp. 23–44, 1987.

[21] R. S. Blum, S. A. Kassam, and H. V. Poor, “Distributed detection with multiple sensors II. Advanced topics,” Proceedings of the IEEE, vol. 85, no. 1, pp. 64–79, 1997.

[22] A. K. Sahu and S. Kar, “Distributed sequential detection for Gaussian binary hypothesis testing: Heterogeneous networks,” in 48th Asilomar Conference on Signals, Systems and Computers, Nov 2014, pp. 723–727.

[23] ——, “Distributed sequential detection for Gaussian shift-in-mean hypothesis testing,” IEEE Transactions on Signal Processing, vol. 64, no. 1, pp. 89–103, Jan 2016.

[24] M. H. DeGroot, “Minimax sequential tests of some composite hypotheses,” The Annals of Mathematical Statistics, pp. 1193–1200, 1960.

[25] N. Schmitz, “Minimax sequential tests of composite hypotheses on the drift of a wiener process,” Statistical Papers, vol. 28, no. 1, pp. 247–261, 1987.

[26] M. Fauß and A. M. Zoubir, “Old bands, new tracks—Revisiting the band model for robust hypothesis testing,” 2016, accepted for publication in the IEEE Transactions on Signal Processing. [Online]. Available: http://arxiv.org/abs/1510.04524 [27] V. V. Veeravalli, T. Basar, and H. V. Poor, “Minimax robust decentralized detection,” IEEE Transactions on Information Theory, vol. 40, no. 1, pp. 35–40, 1994.

[28] G. Gül, “Robust and distributed hypothesis testing,” pp. 1–133, 2017.

[29] G. Gül and A. M. Zoubir, “Theoretical bounds in minimax decentralized hypothesis testing,” IEEE Transactions on Signal Processing, vol. 65, no. 1, pp. 15–26, 2017.

[30] S. Al-Sayed, A. M. Zoubir, and A. H. Sayed, “Robust distributed estimation by networked agents,” IEEE Transactions on Signal Processing, vol. 65, no. 15, pp. 3909 – 3921, Aug 2017.

[31] M. R. Leonard and A. M. Zoubir, “Robust distributed sequential hypothesis testing for detecting a random signal in non-Gaussian noise,” in Proceedings of the 25th European Signal Processing Conference (EUSIPCO), Aug 2017.

[32] W. Hou, M. R. Leonard, and A. M. Zoubir, “Robust distributed sequential detection via robust estimation,” in Proceedings of the 25th European Signal Processing Conference (EUSIPCO), Aug 2017.

[33] M. R. Leonard, M. Stiefel, M. Fauß, and A. M. Zoubir, “Robust sequential testing of multiple hypotheses in distributed sensor networks,” in Proceedings of the 43nd IEEE International Conference on Acoustics, Speech and Signal Processing (ICASSP), April 2018, accepted.

[34] S. Kar and J. M. F. Moura, “Consensus + innovations distributed inference over networks: Cooperation and sensing in networked systems,” IEEE Signal Processing Magazine, vol. 30, no. 3, pp. 99–109, May 2013.

[35] L. Xiao and S. Boyd, “Fast linear iterations for distributed averaging,” Systems & Control Letters, vol. 53, no. 1, pp. 65–78, 2004.

[36] S. A. Kassam, “Robust hypothesis testing for bounded classes of probability densities,” IEEE Transactions on Information Theory, vol. 27, pp. 242–247, 1981.

[37] E. L. Lehmann and J. P. Romano, Testing Statistical Hypotheses, 3rd ed.

New York City, New York, USA: Springer, 2005.

[38] S. Kay, Intuitive Probability and Random Processes Using MATLAB ® .

New York City, New York, USA: Springer, 2006.

[39] J. G. Gonzalez and G. R. Arce, “Weighted myriad filters: A robust filtering framework derived from alpha-stable distributions,” in IEEE International Conference on Acoustics, Speech, and Signal Processing Conference Proceedings (ICASSP), vol. 5, May 1996, pp. 2833–2836.

[40] ——, “Statistically-efficient filtering in impulsive environments:

Weighted myriad filters,” in EURASIP Journal on Advances in Signal Processing, 2002, pp. 4–20.