arXiv:1903.04749v5 [eess.SP] 15 May 2019

Non-Uniform BCSK Modulation in Nutrient-Limited Relay-Assisted Molecular Communication System: Optimization and Performance Evaluation

Hamid Khoshfekr Rudsari, Mahdi Orooji, Member, IEEE, Mohammad Reza Javan, Member, IEEE, Nader Mokari, Senior Member, IEEE, and Eduard A. Jorswieck, Senior Member, IEEE

Abstract

In this paper, a novel non-uniform Binary Concentration Shift Keying (BCSK) modulation in the course of molecular communication is introduced. We consider the nutrient limiting as the main reason for avoiding the nanotransmitters to release huge number of molecules at once. The solution of this problem is in the utilization of the BCSK modulation. In this scheme, nanotransmitter releases the information molecules non-uniformly during the time slot. The 3-dimensional diffusion channel with 3- dimensional drift is considered in this paper. To boost the bit error rate (BER) performance, we consider a relay-assisted molecular communication via diffusion. Our computations demonstrate how the pulse shape of BCSK modulation affects the BER, and we also derive the energy consumption of non-uniform BCSK in the closed-form expression. We study the parameters that can affect the BER performance, in particular the distance between the nanotransmitter and the nanoreceiver, the drift velocity of the medium, and the symbol duration. Furthermore, we propose an optimization problem that is designed to find the optimal symbol duration value that maximizes the number of successful received bits. The proposed algorithm to solve the optimization problem is based on the bisection method. The analytical results

Hamid Khoshfekr Rudsari, Mahdi Orooji, and Nader Mokari are with the Department of Electrical and Computer Engineering, Tarbiat Modares University, Tehran 14115111, Iran.

Mohammad Reza Javan is with Department of Electrical and Robotic Engineering, Shahrood University of Technology, Shahrud 3619995161, Iran.

Eduard A. Jorswieck is with Department of Electrical Engineering and Information Technology, TU Dresden, Germany.

show that non-uniform BCSK modulation outperforms uniform BCSK modulation in BER performance, when the aggregate energy is fixed.

Index Terms

Molecular Communication, Nutrient Limiting, Binary Concentration Shift Keying Modulation, Bit Error Rate, Optimization

I. INTRODUCTION In nanonetworks, Molecular Communication (MC) is used for communication between nanotransmitters and nanoreceivers. The electromagnetic-based communication is not proficient when the communication between microscale and/or nanoscale robots comes into the account [1], [2]. Optical communication is also not useful for these microscale and nanoscale applications because the optical signal requires guided medium or line of sight links [3]. This problem is already solved in nature. In the natural world, chemical signals are used for inter- and intracellular communication at micro- and nanoscales [4]. Therefore, chemical signals are a good candidate for communication at both the macro- and microscopic scales. This is the base of MC. It is one of the most competent approach in nanonetworks for communication between nanomachines. In this communication paradigm, nanomachines use molecules to communicate with each other. Moreover, MC signals are biocompatible, and require very low energy, in the order of a femto-Joule (fJ), for transmitting a bit [3].

Inspired by the communication methods used by biological systems, a variety of MC frameworks are proposed in the literature [5]–[8]. Among them, microtubule MC is imagined for short-range communication [6], and ion signaling and MC via diffusion are proposed for short to medium range communication [7], [8]. In this article, we focus on the relay-assisted MC via diffusion (MCvD). It is worth noting that due to practical limitations such as long range distance between transmitter and receiver nodes and cell signaling in biological communication, relay-aided MC can be adopted. In other words, relays can significantly improve performance and enable the biological communication feasible between different types of cells [9]–[12].

As a part of the biological systems, the modulation process in MC systems demands the oscillatory behavior in nanotransmitters. This oscillation needs ON/OFF mechanism [13]. The nutrient limiting avoid nanotransmitters to synthesize huge number of information molecules (the molecules that are released from the transmitter node to convey the information) at once

DRAFT August 15, 2019

[14]. This problem, in nature, has been solved by spreading the releasing time of molecules. This is the main idea behind BCSK (Binary Concentration Shift Keying) modulation concept. In standard BCSK, the molecules are released uniformly during the time. Despite uniform BCSK, in this paper, we employ non-uniform pulse shapes in BCSK, and show that the manner of releasing the molecules in time, is going to significantly affect the performance of MC systems.

Different modulation techniques are introduced in MCvD. Mahfuz et al. employ two modulation techniques [15]. In the first technique, they consider transmitting bit “1” along the concentration of Q (number of) molecules, when for bit “0”, no molecule is transmitted. In the second modulation technique, they consider information-carrying particles being released as sinusoidal signals with predefined frequency. In [16], Kuran et al. propose two new modulation techniques, namely Concentration Shift Keying (CSK) and Molecule Shift Keying (MoSK). In CSK, the information is modulated using the concentration of the identical molecules, while different types of molecules are considered in MoSK. This idea is extended to use isomer as messenger molecules by Kim et al. [17].

The channel model considered in this paper is based on 3-dimensional (3-D) diffusion with drift in three dimensions which is studied in [18]. This model is the best fit with the blood vessel due to the turbulent behavior of the blood flow [19]–[21]. The relay-assisted MCvD system in 3-D environment is studied in [22]. In this paper, the authors optimize the location of the relay node, and select the appropriate number of molecules by solving a joint optimization problem. However, the drift of the channel is ignored in the aforementioned paper. The molecular relay channel in the case of 1-D and the capacity of the channel is investigated in [23]. In [24], the authors utilize relaying in MCvD systems in order to enhance the performance of the system in the case of long range distances between the nanomachines. They consider two strategies as sense-and-forward (SF) and decode-and-forward (DF) in the relay node to convey the message to the destination node. In [10], the authors introduce the scenario of multi-hop relaying in 3-D channel with no drift by evaluating three schemes to design the relay-assisted MCvD system. The schemes are based on different type of molecules and the number of relay nodes. In spite of the fact that the 3-D channel with drift is the most realistic scenario for the channel of MCvD, it has been neglected in the relay assisted channel models. In this paper, the relay assisted MCvD in the channel with 3-D drift velocity is considered.

In this paper, the bit error rate (BER) of the introduced non-uniform BCSK modulation is derived in closed form expression, and the analytical results reveal that the non uniformity of the molecules concentration shape can potentially improve the BER.

In the second part of the paper, the energy model of the MC, when the capacity of the vesicle is not constant, is considered. As the number of the released molecules increases, the BER decreases with the cost of spending more energy. Considering the limited energy per bit, we show the nonuniform BCSK has better BER compared to the uniform BCSK. We also study the trade off between the transmission rate and the probability of successfully receiving a bit. The molecules are transmitting in equal time slots, called the symbol duration. An optimization problem is designed to find the optimum symbol duration by maximizing the number of successful received bits. We propose an algorithm based on the bisection method to find the optimal value of the symbol duration.

The rest of the paper is organized as follows. In Section II, we study the system model including the channel model and BER analysis. In this section, we derive the mean and the variance of the number of the received molecules and derive a closed-form expression for bit error probability. In Section III, we study the energy model to evaluate the BER performance in terms of energy. In Section IV, we propose the optimization problem to find the optimal value of symbol duration by utilizing the bisection method. In Section V, the numerical result is shown. The paper is concluded in Section VI.

Notation: In this paper, exp(x) and B(k,l) denote the natural exponential function and the binomial distribution with k total number of experiments and the probability of l that each experiment yielding a successful result, respectively. The notation N (μ, σ^2) stands for the normal distribution with mean μ and variance σ^2. The notations erf(x) and Pr(X), refer to error function which is erf ( x ) =^{1√}_{2π} ∫_x 0 exp ( − y^2 ) dy, and the probability of happening the X event, respectively.

II. SYSTEM MODEL In this paper, we adopt Brownian motion [25], to model the movement of the molecules in the medium and consider the drift velocity to attain a comprehensive model for the channel in MCvD system. We employ a generic nanotransmitter as the transmitter node, which can be reused as often as necessary. These types of transmitters are not natural and produced artificially [13], [26]. The receiver in our model is a nanomachine [27], which acts as a passive receiver. The passive receiver counts the number of molecules that arrive in its boundary but does not absorb and remove them from the medium [28]. The nanotransmitter, transmits the information in equal

DRAFT August 15, 2019

Fig. 1. Relay-Assisted MCvD system with drift

symbol durations. The inter-symbol interference (ISI) is defined as the received molecule during the current symbol duration that is transmitted in the previous symbol durations. The noise is created by molecules from the other sources which is accounted in the receiver. The maximuma-posterior (MAP) rule is employed in the receiver to detect the transmitted information.

In the employed model, we have three nodes, namely a nanotransmitter (node S), a nanoreceiver in the destination (node D), and a relay nanomachine (node R). The model is illustrated in Fig. 1.

This system acts as a relay-assisted MCvD system. Node S is assumed to be a point source. It is also assumed that the nodes do not have any mobility and fixed in their positions. During the transmission node R is located between nodes S and D. It has full-duplex transmission and utilizes DF strategy. We assume node S transmits information to node R in the n^{th} time slot, node R decodes the received message from node S at the end of the n^{th} time slot, and retransmits it to node D in the (n + 1)^{th} time slot. Finally, node D detects the information at the end of the (n + 1)^{th} time slot. The medium has drift velocity in three directions, and it has uniform temperature and viscosity.

The BCSK modulation technique is based on releasing the same number of molecules in each sub slot of a time slot [29]. We propose a new BCSK modulation in which the pulse shape of molecules is non uniform. We divide each time slot into I identical sub slots, and the time

Fig. 2. Modulation scheme to send bit “1”, a). Exponential function for non-uniform BCSK, b). Sinc function for non-uniform BCSK, c). Cosine function for non-uniform BCSK, d). uniform pulse BCSK modulation scheme (the number of molecules to send bit “1” in (a), (b), (c) and (d) are equal as

∑_{10} i=1 g(i) = 10000).

slot duration is denoted by t_s. Therefore, each sub slot has

(_1 I × t_s ) duration. In Fig. 2, g(i) is the packet of molecules for each sub slot i. We should shape g(i) with specific function. In Fig. 2, we plot non-uniform BCSK with different pulse shapes. In the introduced scheme, N molecules with the pulse shape of g(i) are released into the medium to represent transmitting bit “1”. In the proposed modulation model, the transmitter does not release any molecule to represent transmitting bit “0” [15]–[17], [30].

In the relay-assisted MCvD system, we should use two different molecules in order to reduce ISI which are denoted by T and U at the transmitter and relay node, respectively. It is worth noting that the relay node counts the number of molecules of type T and the U molecules does not affect it. In addition, the destination node (node D) counts the number of molecules of type U and is insensitive to molecules of type T .

DRAFT August 15, 2019

A. Channel Model

In this paper, the Brownian motion of the released molecules into the medium is biased in drift velocity of the medium. The operation of propagating the molecules is administered by both diffusion and drift as a result of the external active mobility. Therefore, we need to consider the Brownian motion with drift in the channel model. We assume no collision occurs between the molecules that are propagating. The released molecules can be diffused with drift in the medium continuously.

We adopt 3-D fluid environment with drift in 3 directions. We aim to consider the probability of arriving the molecules in the volume of the passive spherical receiver which is located at (W_x, W_y, W_z) with radius of r_W . The relay node is also located between the transmitter and the receiver nodes, at (R_x, R_y, R_z) with radius r_R. In addition, the point source is located at (0,0,0), and the velocity of the medium is (V_x, V_y, V_z). The employed environment is shown in Fig. 1.

The probability density function (pdf) of the molecules in the 3-D diffusion with drift environment for the point source located at (0,0,0) and a passive spherical receiver with radius r_R located at (R_x,R_y,R_z) is given by [18] f(x, y, z, t_s) = 1 √ (4πD_T t_s)^3 exp ( − (x + R_x − V_xt_s)^2 + (y + R_y − V_yt_s)^2 + (z + R_z − V_zt_s)^2 4D_T t_s ) , (1) where D_T is the diffusion coefficient of T molecules in the medium, and (x, y, z) is the location of a point distanced √ x^2 + y^2 + z^2 from the center of node R. The value of D_T depends on the temperature^1, viscosity of the fluid^2, and the Stokes radius of T molecules [32].

To achieve the probability of arriving the molecules in the volume of the relay node, the integration of (1) over the volume of the relay node is required. As studied in [18], the CDF of arriving time in (1), which is the probability of arriving the molecule of type T within time t_s in the volume of the relay node is given by:

F (t_s) = r^2_R 144πD_T t_s exp ( −(R_z − V_zt_s)^2 4D_T t_s ) · ( 4 3∑ k=0 α(k, t_s) + 2 3∑ k=1 β(k, t_s) + 2ϕ(t_s) ) , (2)

1Body temperature is 310^∘ K [31].

2Viscosity of blood at body temperature is 2.46 × 10^{−3} kg/sec.m [31].

where α(k, t_s), β(k, t_s), and ϕ(t_s) are given as follows [18]: α(k, t_s) = [ exp ( − (^{2k+1}_8 r_R + R_y − V_yt_s)^2 4D_T t_s ) + exp ( − (−^{2k+1}_8 r_R + R_y − V_yt_s)^2 4D_T t_s )]

× [ erf ( √ 1 − (2k + 1)^2 64 r_R − V_xt_s + R_x 2 √ D_T t_s ) − erf (− √ 1 − (2k + 1)^2 64 r_R − V_xt_s + R_x 2 √ D_T t_s )] , (3a) β(k, t_s) = [ exp ( − (^k_4 r_R + R_y − V_yt_s)^2 4D_T t_s ) + exp ( − (−^k_4 r_R + R_y − V_yt_s)^2 4D_T t_s )]

× [ erf ( √ 1 − k^2 16 r_R − V_xt_s + R_x 2 √ D_T t_s ) − erf (− √ 1 − k^2 16 r_R − V_xt_s + R_x 2 √ D_T t_s )] , (3b)

ϕ(t) = exp ( − (R_y − V_yt_s)^2 4D_T t_s ) · [ erf (r_R − V_xt_s + R_x 2 √ D_T t_s ) − erf (−r_R − V_xt_s + R_x 2 √ D_T t_s ) ] . (3c)

The molecular distribution for released molecules from node R toward node D is similar to (1). The probability of arriving the molecule of type U within time t_s from relay node toward the destination (node D) is given by (2) and (3), where R_x, R_y, and R_z are changed to W_x − R_x, W_y − R_y, and W_z − R_z, respectively. Note that the other parameters in (2) and (3) except t_s, are changed to the required parameters for the molecules of type U.

The CDF in (2) is a function of the medium velocity, diffusion coefficient of T molecules, the location of node R, and time slot duration. Thus, we can write F (t_s) = P_{ar}(V, D_T , R, t_s), where P_{ar} is the probability of arriving T molecules into the volume of the receiver within time t_s, V = (V_x, V_y, V_z), and R = (R_x, R_y, R_z).

In the scenario of multiple relays (more than one relay node) located at (R_{1k}, R_{2k}, R_{3k}) for k = 1, 2, ..., K, the value of (R_x, R_y, R_z) in (2) is replaced with (R_{1(k−1)} − R_{1(k)}, R_{2(k−1)} − R_{2(k)}, R_{3(k−1)} − R_{3(k)}). It is worth noting that the investigation of multi-hop MCvD systems is performed in [10].

Let M^T_{s,r}[n] denote the total number of T molecules absorbed by node R and arrived at node R at the end of the n^{th} time slot. The total number of molecules, denoted by M^T_{s,r}[n] is given by [16], [33] M^T_{s,r}[n] = N^T_{Cs,r}[n] + N^T_{P s,r}[n] + N_{Nos,r}[n] + N_{NCs,r}[n], (4) where N^T_{Cs,r}[n], N^T_{P s,r}[n], N_{Nos,r}[n], and N_{NCs,r}[n], are explained at Table I.

DRAFT August 15, 2019

TABLE I SPECIFICATION OF DENOTED TERMS FOR THE RECEIVED MOLECULES

Specification Denoted Term The number of molecules transmitted and received during the current time slot N^T_{Cs,r} [n] The number of molecules transmitted in the previous time slot while they are received during the current time slot (ISI) N^T_{P s,r} [n]

The number of molecules from other sources which act as noise NNos,r [n] The error in the counting of the arrived molecules by node R NNCs,r [n]

As regard the independent movement of the messenger molecules with specific probability of arriving the receiver, N^T_{Cs,r}[n] obeys a binomial distribution as [16], [31], [33], [34] N^T_{Cs,r}[n] ∼ I−1∑ i=0 B(x_s[n]g(i), P_{1,i}), (5) where x_s[n] represents the bit transmitted by node S at the n^{th} time slot. In (5) P_{j,i} = P_{ar}(V, D, R, t_{j,i}) is the probability of arriving the molecules within time t_{j,i}, where t_{j,i} = ( jt_s −^{its}_I ) , is the time of each sub slot i of the j^{th} time slot.

The ISI length is finite because we can ignore the ISI effect after a finite number of previously transmitted symbols [35]. Therefore, we can write N^T_{P s,r}[n] as N^T_{P s,r}[n] ∼ J∑ j=1 I−1∑ i=0 B(x_s[n − j] g(i), q_{j,i}), (6) where J indicates the ISI length, x_s[n−j] represents the bit transmitted by node S at the (n−j)^{th} time slot and q_{j,i} = P_{j+1,i} − P_{j,i}.

We can approximate the binomial distribution in (5) and (6) by a normal distribution, if g(i) in each sub slot is large enough, and g(i)P_{ar}(V, D_T , R, t_s) is not zero [34]. We know the mean and variance of the sum of independent normal distributions are the sum of their means and variances, respectively. Therefore, N^T_{Cs,r}[n] obeys a normal distribution given by N^T_{Cs,r}[n] ∼ N ( x_s[n] I−1∑ i=0 g(i) P_{1,i} , x_s[n] I−1∑ i=0 g(i) P_{1,i}(1 − P_{1,i}) ) . (7)

Then, N^T_{P s,r}[n] becomes N^T_{P s,r}[n] ∼ N (_J∑ j=1 I−1∑ i=0 x_s[n − j] g(i) q_{j,i} , J∑ j=1 I−1∑ i=0 x_s[n − j] g(i) q_{j,i}(1 − q_{j,i}) ) . (8)

We assume the distribution of N_{Nos,r}[n] is normal as [33] N_{Nos,r}[n] ∼ N (μ_{nos,r}, σ^2_{nos,r}), (9) where μ_{nos,r} and σ^2_{nos,r} are the mean and variance of noise, respectively. The distribution of counting noise N_{NCs,r}[n] is considered as [33] N_{Ncs,r}[n] ∼ N (0, σ^2_{ncs,r}), (10) where σ^2_{ncs,r} is the variance of counting noise and is dependent on the mean values of the molecules received by node R as (13) and (14) [33].

Since the distributions of (7), (8), (9), and (10) are normal, M^T_{s,r}[n] obeys the normal distribution as follows

Pr(M^T_{s,r}[n] | x_s[n] = 0) ∼ N (μ_{0s,r}, σ^2_{0s,r}), (11) Pr(M^T_{s,r}[n] | x_s[n] = 1) ∼ N (μ_{1s,r}, σ^2_{1s,r}), (12)

where μ_{0s,r}, σ^2_{0s,r}, μ_{1s,r} and σ^2_{1s,r} are derived from (7), (8), (9), and (10), respectively as follows

μ_{0s,r} = π_1 J∑ j=1 I−1∑ i=0 g(i) q_{j,i} + μ_{nos,r}, (13)

μ_{1s,r} = π_1 J∑ j=1 I−1∑ i=0 g(i) q_{j,i} + π_1 I−1∑ i=0 g(i) P_{1,i} + μ_{nos,r}, (14)

σ^2_{0s,r} = π_1 J∑ j=1 {_{I−1}∑ i=0 g(i)q_{j,i} ( 1 − q_{j,i} ) + π_0 (_{I−1}∑ i=0 g(i) q_{j,i} )_2} + σ^2_{nos,r} + μ_{0s,r}, (15)

σ^2_{1s,r} = π_1 J∑ j=1 {_{I−1}∑ i=0 g(i)q_{j,i} ( 1 − q_{j,i} ) + π_0 (_{I−1}∑ i=0 g(i) q_{j,i} )_2} + I−1∑ i=0 g(i) P_{1,i} ( 1 − P_{1,i} )

+ σ^2_{nos,r} + μ_{1s,r}, (16)

where Pr ( x_s[n] = 1 ) = π_1 and Pr ( x_s[n] = 0 ) = π_0. The details of the calculation for mean and variance of N^T_{P s,r} are provided in Appendix A.

Relay-node (node R) decides based on the MAP rule in detection as below [36]

x̂_r[n] = 1 if M^T_{s,r}[n] ≥ τ_R 0 if M^T_{s,r}[n] < τ_R, (17)

where τ_R is the detection threshold at node R, and x̂_r[n] is the information bit detected by node R at the end of the n^{th} time slot.

DRAFT August 15, 2019

Since our system is a relay-assisted MCvD system, node R has to forward the information bit detected at the end of the n^{th} time slot. Similar to the mathematical manipulations derived for node S and node R, the distribution of the total number of U molecules arrived at node D, denoted by M^U_{r,d}[n + 1], which detected at the end of the (n + 1)^{th} time slot can be derived from

Pr(M^U_{r,d}[n + 1] | x_r[n + 1] = 0) ∼ N (μ_{0r,d}, σ^2_{0r,d}), (18) Pr(M^U_{r,d}[n + 1] | x_r[n + 1] = 1) ∼ N (μ_{1r,d}, σ^2_{1r,d}), (19) where x_r[n + 1] is the transmitted bit at the beginning of the (n + 1)^{th} time slot from node R. The calculation of mean and variance values of molecules transmitted by node R and received by node D (μ_{0r,d}, σ^2_{0r,d}, μ_{1r,d}, and σ^2_{1r,d}), is similar to the calculation of mean and variance values of molecules which are transmitted by node S and received by node R, and are therefore omitted here.

B. BER Analysis

We study the BER analysis of the relay-assisted MCvD system, which is introduced in [36]. The probability of error between two nodes for the n^{th} transmitted bit is calculated as follows:

P_e[n] = Pr(x_s[n] = 1)Pr ( x̂_d(n + 1) = 0 | x_s[n] = 1 )

+ Pr(x_s[n] = 0)Pr ( x̂_d(n + 1) = 1 | x_s[n] = 0 ) . (20)

Before the calculation of BER, we should determine the Pr(x_r[n] = 1), which is given by Pr(x_r[n] = 1) = π_1Pr(x̂_r[n − 1] = 1 | x_s[n − 1] = 1) + π_0Pr(x̂_r[n − 1] = 1 | x_s[n − 1] = 0),

(21)

where Pr(x_s[n − 1] = 1) and Pr(x_s[n − 1] = 0) are π_1 and π_0, respectively. We consider the MAP rule detection in (17) and use (13), (14), (15) and (16) to calculate (21) as follows:

Pr(x̂_r[n − 1] = 1 | x_s[n − 1] = 1) = Pr(M^T_{s,r}[n − 1] ≥ τ_R | x_s[n − 1] = 1) = 1 2 ( 1 − erf ( τ_R − μ_{1s,r} √ 2σ^2_{1s,r} )) , (22)

Pr(x̂_r[n − 1] = 1 | x_s[n − 1] = 0) = Pr(M^T_{s,r}[n − 1] ≥ τ_R | x_s[n − 1] = 0) = 1 2 ( 1 − erf ( τ_R − μ_{0s,r} √ 2σ^2_{0s,r} )) . (23)

Now we can calculate (20) from (22) and (23). At the final step we can write BER for the direct transmission from (20)-(23) given by

P_{eD} [n] = 1 2 + 1 4 [ erf ( τ_D − μ_{1s,d} √ 2σ^2_{1s,d} ) − erf ( τ_D − μ_{0s,d} √ 2σ^2_{0s,d} )] , (24)

where τ_D is the detection threshold at node D. The BER for the relay-assisted transmission is calculated as follows:

P_{eSR} [n] = 1 2 + 1 8 [ erf ( τ_R − μ_{1s,r} √ 2σ^2_{1s,r} ) − erf ( τ_R − μ_{0s,r} √ 2σ^2_{0s,r} )] · [ erf ( τ_D − μ_{0r,d} √ 2σ^2_{0r,d} ) − erf ( τ_D − μ_{1r,d} √ 2σ^2_{1r,d} )] , (25) where P_{eD} and P_{eSR} denote the bit error probability for the direct transmission and the bit error probability for the relay-assisted transmission, respectively.

III. ENERGY MODEL

In a communication via a diffusion system, energy is consumed for the production of the messenger molecules and releasing them toward the destination nanomachine [5]. In our energy model, the energy cost for sending bit “1”, is considered as the sum of the total energy of each sub slot i in g(i) pulse shape. The steps of the messenger molecule production and releasing known as exocytosis are [4]:

• Synthesis of the messenger molecules from their building blocks: The energy cost of a single messenger molecule is denoted by E_S . Since we should consider the synthesis of g(i) packets in the energy model, the energy cost of it would be g(i)E_S.

• Production of a secretory vesicle, which is a packet of the messenger molecules [5]: We use one vesicle for each g(i) packet of the molecules and the energy cost is denoted by E_V (i). Since we use one vesicle for each g(i), we would have C_v = g(i) where C_v is the capacity of each vesicle and its unit is the number of molecules.

• Carrying the secretory vesicles to the cell membrane: The energy cost of it denoted by E_C . • Releasing the molecules via the fusion of the vesicle and the cell membrane: The energy cost of extraction of a vesicle to the medium denoted by E_E , which is provided in Table II.

The capacity of each vesicle C_v can be approximated by [5]:

C_v = ( r_v r_{mm} √ 3 )_3 = g(i), (26)

where r_v is the radius of a vesicle and r_{mm} is the radius of the messenger molecule. Note that

DRAFT August 15, 2019

TABLE II ENERGY MODEL COSTS

Parameter Term Values Energy cost for adding a single amino acid to an amino acid chain EAM 202.88 zJ [5] The cost of synthesizing ESY 415 zJ [1], [37] The cost of phosphorylation EP H 83 zJ [1], [37] The cost of releasing molecules into the medium EE 830 zJ [38]

the value of r_v differs for each g(i) due to non-uniform BCSK assumption. Therefore, r_v is not constant in our energy model and we should change r_v to r_v(i) which can be calculated as r_v(i) = √ 3 r_{mm} ×^3 √ g(i). (27) In this paper, we use proteins as messenger molecules. Proteins are produced by combining amino acids to create a specific amino acid chain at the subunit plant. The energy cost of each step to transmit proteins as messenger molecules that are explained above can be obtained as follows [5]: E_S = E_{AM} ( N_{aa} − 1 ) , (28) E_v(i) = E_{SY} ( 4πr^2_v(i) ) , (29) E_C = E_{P H} ⌈ r_{unit}/2 8 ⌉ , (30) where ⌈X⌉, N_{aa}, r_{unit} are the ceiling function which maps X to the least integer greater than or equal to X, the number of amino acids, the radius of the transmitter unit in nanometer scale, respectively. The values of parameters E_{AM} , E_{SY} , and E_{P H} are provided in Table II. The zJ term in the aforementioned table is the zepto Joule whose value is 10^{−21} Joules.

By using all of the energies given above and (27), the total energy for sending each g(i) is derived as E_{Ti} = E_{AM} ( N_{aa} − 1 ) g(i) + ( E_{SY} ( 4π( √ 3 r_{mm}^3 √ g(i))^2 ) + E_{P H} ⌈ r_{unit}/2 8 ⌉ + E_E ) . (31) According to (31), the total energy for sending bit “1” in non-uniform BCSK modulation is

E_T = I−1∑ i=0 E_{Ti} . (32)

E_T is directly proportional to pulse shape in non-uniform BCSK modulation as seen in (31) and (32).

TABLE III PROPOSED ALGORITHM BASED ON THE BISECTION METHOD

Initialization:

Set 0 < ϵ < 1, Lower bound = 0, and Upper bound = a sufficienctly large number, e.g., 10^3 in our setting Iterations:

Step 1: l = (Lower bound + Upper bound)/2. Step 2: Solve the concave feasibility problem (37). Step 3: If (37) is feasible,

Lower bound = l, else

Upper bound = l.

Step 4: If | Upper bound − Lower bound | ≤ ϵ,

stop, else

go back to Step 1.

IV. SYMBOL DURATION OPTIMIZATION PROBLEM In this section we introduce the optimization problem to find the optimal value of the symbol duration. The transmission data rate, denoted by R, is R = 1 t_s . (33)

By increasing the symbol duration, the achievable data rate decreases. There is a trade off between t_s and BER, as t_s increases, BER decreases [39]. The product of the success probability of a received bit and data rate gives the aforementioned tradeoff. In the binary modulation, for BER more than 0.5, we can change BER to 1 − 0.5 [40]. It is due to the fact that the transmitter node transmits one bit in each time slot, therefore, the probability of successful reception, denoted by P_Υ [n], is [40]

P_Υ [n] = (1 − 2P_{eSR} [n])^N , (34)

where N is the number of bits in each symbol. However, in this paper N = 1. We formulate the optimization problem to find the optimal value of t^∗_s as follows:

max_{ts} P_Υ [n](t_s) · R(t_s). (35)

DRAFT August 15, 2019

TABLE IV VALUES AND RANGES OF MCVD SYSTEM PARAMETERS

Parameter Variable Values Diffusion Coefficient DT , DU 4 × 10^{−9} m^2/s [31] Drift Velocity (Vx, Vy, Vz ) [1, 100] μm/s [18] Location of node D (WX , Wy, Wz ) [20, 200] μm [18] Symbol duration ts [1, 16] ms [18] Radius of the receiver rR, rW 50 μm [18] Molecular noise mean σ^2_{nos,r}, σ^2_{nor,d} 100 [33] Molecular noise variance μnos,r , μ_{nor,d} 100 [33] Probability of sending bit “1” π1 0.5 The ISI length J [1, 30] The number of i sub slot I 10 Number of amino-acids Naa 51 [5] Stokes’ radius of insulin rs 2.68 nm [42] Radius of insulin molecule rmm 2.5 nm [1] Radius of the transmitter runit 10 μm [4]

The objective function in (35) is quasi-concave, therefore, the optimization problem (35) is quasi-concave. The discussion of the quasi-concavity of the objective function in (35) based on the numerical assessments is provided in Appendix B.

We employ the bisection method to solve the optimization problem (35), in which the optimal symbol duration is determined by solving a concave feasibility problem at each step. The lsublevel set (l ∈ R) of a function h : R^n → R is defined as [41] ζ_l = {x ∈ dom h | h(x) ≥ l}. (36) Note that R is the set of real numbers. Thus, the new optimization problem by considering the l-sublevel set of the objective function in (35) as constraint, is

Find t_s s.t P_Υ [n](t_s) · R(t_s) − l > 0.

(37)

We provide the proposed algorithm based on the bisection method for solving the optimization problem in Table III, where ϵ is some positive small number.

V. NUMERICAL RESULT

In this section, we show the numerical results to calculate the error probability performance of a relay-assisted MCvD system with drift for BCSK modulation and evaluate the BER in terms of the budget of energy. Also, we present how the MCvD system parameters influence the performance.

The proposed system parameters used in the analysis of BER and energy are provided in Table IV. We also consider protein based messenger molecules in our system. The number of amino acids that are required to form a protein depends on the size of protein. Furthermore, adding a single amino acid to an amino acid chain, regardless of the type of the amino acid, has a constant cost of energy [43]. We assume that the diffusion coefficient of T and U molecules are equal. We also assume J = 10 in the analysis of the system unless otherwise stated. However, the performance of the system is evaluated under the different values of ISI length.

At first, we assume that node R is located between nodes S and D. Note that node R has the same modulation scheme as node D. It is also assumed that in all figures in this section W_x = 2R_x, W_y = 2R_y, and W_z = 2R_z. Hence, the analysis is based on the location of the relay node. Without loss of generality, it is assumed that the mean and variance values of molecular noise are considered as 100 [33].

The BER performance of MCvD system for exponential, sinc, cosine, and uniform pulse shapes as a function of the symbol duration, t_s, are presented in Fig. 3. In addition, the analysis is based on two different locations of the relay node, where R = (100 μm, 12 μm, 14 μm) and R = (100 μm, 14 μm, 14 μm). The energy consumption to transmit bit “1” is also identical for each different value of the relay nodes location. As shown in this figure, the BER performance improves by increasing the time slot duration. The location of the relay node also impacts the BER performance. The BER of MCvD system for the relay and destination nodes in case they are closer to the transmitter, is smaller. The exponential function outperforms other pulse shapes in the identical time slot, location of the relay, and energy consumption. On the other hand, the BER performance of the sinc function is better compared to uniform pulse and cosine function. The MCvD system reaches the BER around 10^{−5} in case of utilizing the exponential function, the pulse shape set to t_s = 18 ms, the destination node is located at (200 μm, 24 μm, 28 μm), and the energy consumed to transmit bit “1” is 1000 fJ.

In Fig. 4, we present the BER performance of non-uniform BCSK modulation as a function of

DRAFT August 15, 2019

Fig. 3. BER of the MCvD system with the relay node for exponential, sinc, cosine and uniform pulse shape in non-uniform BCSK modulation, as a function of symbol duration (ts) for different locations of relay node and different values of energy for transmitting bit “1” (Rx = 100 μm, Rz = 14 μm, Vx = 100 μm/s, Vy = 40 μm/s, and Vz = 40 μm/s).

the location of the node R. It is assumed that R_x = 100 μm. We can observe that by increasing R_z, for fix value of R_y = 14 μm, the BER increases. It is due to the fact that by increasing the distance between the transmitter and the receiver nodes, the probability of hitting the molecules by the receiver decreases. In addition, the BER performance of the relay-assisted MCvD system for fixed value of R_z = 14 μm and as a function of R_y is shown in this figure. By increasing R_y, BER is also increased. Also, as shown in Fig. 4, the exponential pulse shape for non-uniform BCSK modulation has the best BER performance among other examples. It is worth noting that the analysis is based on of two different values of energy consumption. It can be viewed from the Fig. 4 that the more consumed energy, the less the value of BER is. The BER of the proposed MCvD system changes from 10^{−5} to around 10^{−3} by increasing R_z from 14 μm to 14.25 μm in case of considering R_y = 14 μm and exponential function as the pulse shape of the system. Hence, the performance of the system is extremely sensitive to the locations of the relay and destination node.

In Fig. 5, the BER performance of different pulse shapes for non-uniform BCSK modulation,

Fig. 4. BER of the MCvD system with the relay node for exponential, sinc, cosine and uniform pulse shape in non-uniform BCSK modulation, as a function of location of the relay node for different values of energy for transmitting bit “1” (Rx = 100 μm, Vx = 100 μm/s, Vy = 40 μm/s, Vz = 40 μm/s, and ts = 18 ms).

fixed value of V_x = 100 μm, and different values of drift velocity of V_y and V_z is depicted. It shows that by increasing V_z from 0 to 40 μm/s and for V_y = 40 μm/s and fixed value of consumed energy as E_T = 1000 fJ, BER of the system decreases from 6 × 10^{-5} to 1.7 × 10^{-5} in case of exponential function as the pulse shape. In the scenario of utilizing sinc function as the pulse shape, by considering the mentioned setting of the system parameters, BER decreases from 0.1841 to 0.1522, which is smaller compared to the exponential function for pulse shaping. On the other hand, by assuming the fixed value of V_z = 40 μm/s and different values of V_y from 0 to 40 μm/s, the BER of uniform pulse shape decreases from 0.267 to 0.1592. On the other hand, in case of utilizing the exponential function, BER decreases from 0.0258 to 1.7 × 10^{-5}, which has the best performance among the other pulse shapes with the aggregated consumed energy is 100 fJ. By taking the aforementioned explanation into consideration, increasing the drift velocity improves the BER performance of the system in fixed energy consumed to transmit bit a “1”. We can see that increasing the drift velocity can improve the BER performance, because the drift velocity can make the diffusion and propagating molecules faster. Thus, increasing

DRAFT August 15, 2019

Fig. 5. BER of the MCvD system with the relay node for exponential, sinc, cosine and uniform pulse shape in non-uniform BCSK modulation, as a function of drift velocity for different values of energy for transmitting bit “1” (Rx = 100 μm, Ry = 12 μm, Rz = 14 μm, Vx = 100 μm/s, and ts = 18 ms).

the drift velocity can improve the arriving probability of molecules which results in the BER performance improvement. Increasing the drift velocity also impacts the number of molecules received from other sources, which are denoted by N_{Nos,r}[n] and treated as noise. Furthermore, BER is improved by increasing the drift velocity as shown in Fig. 5, which implies that the impact of received molecules during the current time slot overcomes the noise and ISI effects.

The length of ISI impacts the BER performance [35]. In Fig. 6, the BER performance for the exponential function as the pulse shape at the transmitter, as a function of ISI length from 0 to 40, for different values of time slot is shown. It could be seen that by increasing the ISI length, the BER increases. It is due to the fact that the molecules transmitted in the previous time slots are received in the current time slot. By increasing the value of t_s, the BER decreases, because the molecules have enough time to arrive at the relay node, and after that to destination node. It also could be find that by increasing the time slot duration, the previously transmitted molecules have more time to arrive at the receiver in their time slot, therefore, the BER decreases. By considering the ISI length from 6 to 14 for t_s = 16 ms, the BER increases from 0.037 to

Fig. 6. BER of the MCvD system with the relay node for exponentially function pulse shape in non-uniform BCSK modulation, as a function of ISI length for different values of symbol duration (Rx = 100 μm, Ry = 12 μm, Rz = 14 μm, Vx = 100 μm/s, Vy = 40 μm/s, and Vz = 40 μm/s).

0.0566. However, for ISI length greater than 17, the BER goes over 0.1, for which the impact of ISI could be ignored.

The performance of the proposed algorithm to obtain the optimal value of the symbol duration is demonstrated in Fig 7. We consider four cases for the mixture of the location of the relay node and V_y when the pulse shape is exponential function. As we discussed, the optimal symbol duration obtains the maximum number of successful received bits. By considering V_y = 60 μm/s, the location of the relay node as (100 μm, 12 μm, 13 μm), and optimal symbol duration as 13.89 ms, the number of successful received bits reaches to 70.8. We observe that by increasing the velocity of the medium in fixed location of the relay node, the optimal symbol duration is decreased. This is due to the Brownian motions behavior. Increasing drift velocity causes faster propagation of the molecules into the medium. In addition, the number of molecules that are received by the receiver node are increased. Therefore, we can find the smaller value of the symbol duration to reach the minimum BER. It also could be realized that for nearest location

DRAFT August 15, 2019

Fig. 7. The optimization evaluation based on the proposed algorithm to find the optimal symbol duration ts (Rx = 100 μm, Vx = 100 μm/s, and Vz = 40 μm/s).

of the relay node and the destination node, the number of successful received bits increases. On the other hand, the symbol duration decreases. It is due to the fact that, by decreasing the distance between the transmitter and receiver, the molecules need smaller time to arrive at the receiver. In addition, the probability of arriving molecules in short distances, is more than the long ones. Hence, the number of successful received bits increases.

Note that we use MAP rule detection in Fig. 3, Fig. 4, Fig. 5, and Fig. 6, at receiver node. We can observe from Fig. 3, Fig. 4, and Fig. 5, that the pulse shaping in BCSK modulation can make a significant difference in BER performance considering parameters of MCvD system and budget of energy.

VI. CONCLUSION The nutrient limiting is the main reason to utilize the BCSK modulation in MC systems.

In this paper, we proposed a new non-uniform BCSK modulation and analyzed the BER of a relay-assisted MCvD system in a 3-D environment with drift with respect to the energy in nanotransmitter. We also derived closed-form expression for the means and the variances of the number received molecules to calculate BER in the direct and the relay-assisted transmission.

In addition, we studied the effect of the system parameters such as the distance between nanotransmitter and nanoreceiver, drift velocity of medium and symbol duration on the BER performance. We also employed an iterative algorithm to find the optimal value of symbol duration in terms of maximizing the number of successfully received bits. Finally, we compared the difference between uniform and non-uniform BCSK modulation considering the energy and BER performance. As a future work, one can optimize the pulse shape in the introduced modulation model to minimize the BER in a channel with degradation of molecules. The other future works can focus on the outage performance, subject to the evaluation of the Signal-to- Noise-Ratio (SINR) or other goodputs, such as the capacity of the channel. One can also optimize the other parameters of the system, such as the number of allocated molecules to the transmitter node. Furthermore, interested readers can investigate applications of MC, e.g., the mobile MC and drug delivery system on the basis of the introduced non-uniform BCSK modulation. Position of the relay in relay-assisted MCvD system has a massive impact on the BER performance. To solve this issue, one of our future works is based on the optimization of the location of the relay node based on the minimization of BER or other outputs of the system.

APPENDIX A THE CALCULATIONS OF MEAN AND VARIANCE FOR ISI

In this appendix, the details for calculation of mean and variance values of N^T_{P s,r} in (8), are provided.

We approximate the binomial distribution of each sub slot i in every time slot j to normal distribution in (8), in terms of g(i) is large enough and g(i) × q_{j,i} is not zero. The mean of ISI for the j^{th} time slice is calculated as follows: E(N^T_{P s,r}[n, j]) = π_0E(N^T_{P s,r}[n, j] | x_s[n − j] = 0) + π_1E(N^T_{P s,r}[n, j] | x_s[n − j] = 1) = π_1 I−1∑ i=0 g(i)q_{j,i}. (38)

The variance value of N^T_{P s,r} for j^{th} time slice is calculated as

var(N^T_{P s,r}[n, j]) = E((N^T_{P s,r}[n, j])^2) − E^2(N^T_{P s,r}[n, j]), (39)

DRAFT August 15, 2019

where var(X) denotes the variance of random variable X and E((N^T_{P s,r}[n, j])^2) can be calculated as follows:

E((N^T_{P s,r}[n, j])^2) = π_0E((N^T_{P s,r}[n, j])^2 | x_s[n − j] = 0) + π_1E((N^T_{P s,r}[n, j])^2 | x_s[n − j] = 1)

= π_1 (_{I−1}∑ i=0 g(i)q_{j,i}(1 − q_{j,i}) + (^{I−1}∑ i=0 g(i)q_{j,i} )_2 ) . (40) Therefore, var(N^T_{P s,r}[n, j]) becomes var(N^T_{P s,r}[n, j]) = π_1 (_{I−1}∑ i=0 g(i)q_{j,i}(1 − q_{j,i}) + (^{I−1}∑ i=0 g(i)q_{j,i} )_2 ) − ( π_1 I−1∑ i=0 g(i)q_{j,i} )_2

= π_1 (_{I−1}∑ i=0 g(i)q_{j,i}(1 − q_{j,i}) ) + π_0π_1 (_{I−1}∑ i=0 g(i)q_{j,i} )_2 . (41)

The mean and variance values for ISI are, respectively, derived as E(N^T_{P s,r}[n]) = J∑ j=1 E(N^T_{P s,r}[n, j]), (42)

var(N^T_{P s,r}[n]) = J∑ j=1 var(N^T_{P s,r}[n, j]). (43)

APPENDIX B THE DISCUSSION OF THE QUASI-CONCAVITY OF THE PROPOSED OPTIMIZATION PROBLEM The derivation of the proposed objective function in (35) with respect to the optimization variable t_s is not tractable due to the complexity of the BER formula in (25) which is also dependent on (13)-(16). By assuming the objective function in (35) as F , we plot the first derivative of the objective function F with respect to t_s in Fig. 8 by considering the exponential function for g(i). Note that if we simulate the first derivative of F with respect to t_s for all possible values of t_s, the results are always similar to Fig. 8. From out extensive simulations, we deduce that the first derivative of F with respect to t_s is non-negative for the values of t_s up to a point denoted by t^∗_s and is non-positive the values above it, i.e., it is non-decreasing for t_s ≤ t^∗_s and is non-increasing for t_s ≥ t^∗_s. Hence, the first derivative of the objective function in (35) is given by ∂F ∂t_s > 0, t_s ≤ t^∗_s ∂F ∂t_s < 0, t_s ≥ t^∗_s. (44a)

(44b)

Fig. 8. The first derivative of the objective function proposed in (35) with respect to ts, as a function of time slot duration (Rx = 100 μm, Ry = 12 μm, Rz = 13 μm, Vx = 100 μm/s, Vy = 40 μm/s, and Vz = 40 μm/s).

Therefore, (35) is quasi-concave. Finally, due to the quasi-concavity of the objective function, we conclude that our proposed optimization problem is quasi-concave.

REFERENCES

[1] R. A. Freitas, Nanomedicine, volume I: basic capabilities. Landes Bioscience Georgetown, TX, 1999, vol. 1. [2] S. Sengupta, M. E. Ibele, and A. Sen, “Fantastic voyage: Designing self-powered nanorobots,” Angewandte Chemie International Edition, vol. 51, no. 34, pp. 8434–8445, 2012.

[3] N. Farsad, H. B. Yilmaz, A. Eckford, C. B. Chae, and W. Guo, “A comprehensive survey of recent advancements in molecular communication,” IEEE Communications Surveys & Tutorials, vol. 18, no. 3, pp. 1887–1919, 2016.

[4] B. Alberts, A. Johnson, J. Lewis, M. Raff, K. Roberts, and P. Walter, Molecular biology of the cell. Garland Science, 2007.

[5] M. Ş. Kuran, H. B. Yilmaz, T. Tugcu, and B. Özerman, “Energy model for communication via diffusion in nanonetworks,” Nano Communication Networks, vol. 1, no. 2, pp. 86–95, 2010.

[6] A. Enomoto, M. Moore, T. Nakano, R. Egashira, T. Suda, A. Kayasuga, H. Kojima, H. Sakakibara, and K. Oiwa, “A molecular communication system using a network of cytoskeletal filaments,” in Proceedings of the 2006 NSTI Nanotechnology Conference, 2006.

[7] T. Nakano, T. Suda, M. Moore, R. Egashira, A. Enomoto, and K. Arima, “Molecular communication for nanomachines using intercellular calcium signaling,” in 5th IEEE Conference on Nanotechnology, 2005, pp. 478–481.

DRAFT August 15, 2019

[8] M. Pierobon and I. F. Akyildiz, “A physical end-to-end model for molecular communication in nanonetworks,” IEEE Journal on Selected Areas in Communications, vol. 28, no. 4, 2010.

[9] A. Einolghozati, M. Sardari, and F. Fekri, “Decode and forward relaying in diffusion-based molecular communication between two populations of biological agents,” in Proceedings IEEE ICC, Jun. 2014, pp. 3975–3980.

[10] A. Ahmadzadeh, A. Noel, and R. Schober, “Analysis and design of multi-hop diffusion-based molecular communication networks,” IEEE Transactions on Molecular, Biological and Multi-Scale Communications, vol. 1, no. 2, pp. 144–157, 2015.

[11] B. Atakan and O. B. Akan, “On molecular multiple-access, broadcast, and relay channels in nanonetworks,” in Proceedings of the 3rd International Conference on Bio-Inspired Models of Network, Information and Computing Sytems, 2008, p. 16.

[12] T. Nakano, Y. Okaie, and J.-Q. Liu, “Channel model and capacity analysis of molecular communication with Brownian motion,” IEEE communications letters, vol. 16, no. 6, pp. 797–800, 2012.

[13] U. Chude Okonkwo, R. Malekian, and B. Maharaj, Advanced Targeted Nanomedicine. Springer, 2019. [14] Y. S. Polikanov, G. M. Blaha, and T. A. Steitz, “How hibernation factors rmf, hpf, and yfia turn off protein synthesis,” Science, vol. 336, no. 6083, pp. 915–918, 2012.

[15] M. U. Mahfuz, D. Makrakis, and H. T. Mouftah, “On the characterization of binary concentration-encoded molecular communication in nanonetworks,” Nano Communication Networks, vol. 1, no. 4, pp. 289–300, 2010.

[16] M. S. Kuran, H. B. Yilmaz, T. Tugcu, and I. F. Akyildiz, “Modulation techniques for communication via diffusion in nanonetworks,” in Proceedings IEEE ICC, Kyoto, Japan, Jun. 2011, pp. 1–5.

[17] N. R. Kim and C. B. Chae, “Novel modulation techniques using isomers as messenger molecules for nano communication networks via diffusion,” IEEE Journal on Selected Areas in Communications, vol. 31, no. 12, pp. 847–856, 2013.

[18] M. R. Bhatnagar et al., “3-d diffusive-drift molecular channel characterization for active and passive receivers,” IEEE Transactions on Molecular, Biological and Multi-Scale Communications, 2019.

[19] H. Chanson, Applied hydrodynamics: an introduction to ideal and real fluid flows. CRC Press, 2009. [20] C. K. Batchelor and G. Batchelor, An introduction to fluid dynamics. Cambridge university press, 1967. [21] L. Felicetti, M. Femminella, G. Reali, and P. Liò, “A molecular communication system in blood vessels for tumor detection,” in Proceedings of ACM The First Annual International Conference on Nanoscale Computing and Communication. ACM, 2014, p. 21.

[22] S. K. Tiwari, T. R. T. Reddy, P. K. Upadhyay, and D. B. Da Costa, “Joint optimization of molecular resource allocation and relay positioning in diffusive nanonetworks,” IEEE Access, vol. 6, pp. 67 681–67 687, 2018.

[23] T. Nakano and J.-Q. Liu, “Design and analysis of molecular relay channels: An information theoretic approach,” IEEE Transactions on NanoBioscience, vol. 9, no. 3, pp. 213–221, 2010.

[24] A. Einolghozati, M. Sardari, and F. Fekri, “Relaying in diffusion-based molecular communication,” in 2013 IEEE International Symposium on Information Theory. IEEE, 2013, pp. 1844–1848.

[25] H. Mori, “Transport, collective motion, and Brownian motion,” Progress of theoretical physics, vol. 33, no. 3, pp. 423–455, 1965.

[26] R. F. Fakhrullin, A. I. Zamaleeva, R. T. Minullina, S. A. Konnova, and V. N. Paunov, “Cyborg cells: functionalisation of living cells with polymers and nanomaterials,” Chemical Society Reviews, vol. 41, no. 11, pp. 4189–4206, 2012.

[27] T. Nakano, T. Suda, Y. Okaie, M. J. Moore, and A. V. Vasilakos, “Molecular communication among biological nanomachines: A layered architecture and research issues,” IEEE transactions on nanobioscience, vol. 13, no. 3, pp. 169–197, 2014.

[28] A. Noel, Y. Deng, D. Makrakis, and A. Hafid, “Active versus passive: Receiver model transforms for diffusive molecular communication,” in 2016 IEEE Global Communications Conference (GLOBECOM). IEEE, 2016, pp. 1–6.

[29] H. B. Yilmaz, N. R. Kim, and C. B. Chae, Modeling, Methodologies and Tools for Molecular and Nano-scale Communications. Springer, 2017.

[30] N. Garralda, I. Llatser, A. Cabellos Aparicio, E. Alarcón, and M. Pierobon, “Diffusion-based physical channel identification in molecular nanonetworks,” Nano Communication Networks, vol. 2, no. 4, pp. 196–204, 2011.

[31] N. R. Kim, A. W. Eckford, and C. B. Chae, “Symbol interval optimization for molecular communication with drift,” IEEE Transactions on NanoBioscience, vol. 13, no. 3, pp. 223–229, 2014.

[32] H. J. V. Tyrrell and K. Harris, Diffusion in liquids: A theoretical and experimental study. Butterworth-Heinemann, 2013. [33] A. Singhal, R. K. Mallik, and B. Lall, “Performance analysis of amplitude modulation schemes for diffusion-based molecular communication,” IEEE Transactions on Wireless Communications, vol. 14, no. 10, pp. 5681–5691, 2015.

[34] H. B. Yilmaz, C. B. Chae, B. Tepekule, and A. E. Pusane, “Arrival modeling and error analysis for molecular communication via diffusion with drift,” in Proceedings of the Second Annual International Conference on Nanoscale Computing and Communication. ACM, 2015, p. 26.

[35] D. Kilinc and O. B. Akan, “Receiver design for molecular communication,” IEEE Journal on Selected Areas in Communications, vol. 31, no. 12, pp. 705–714, 2013.

[36] N. Tavakkoli, P. Azmi, and N. Mokari, “Performance evaluation and optimal detection of relay-assisted diffusion-based molecular communication with drift,” IEEE Transactions on NanoBioscience, vol. 16, no. 1, pp. 34–42, 2017.

[37] D. L. Nelson, A. L. Lehninger, and M. M. Cox, Lehninger principles of biochemistry. Macmillan, 2008. [38] L. Eliasson, F. Abdulkader, M. Braun, J. Galvanovskis, M. B. Hoppa, and P. Rorsman, “Novel aspects of the molecular mechanisms controlling insulin secretion,” The Journal of physiology, vol. 586, no. 14, pp. 3313–3324, 2008.

[39] S. Kadloor, R. S. Adve, and A. W. Eckford, “Molecular communication using Brownian motion with drift,” IEEE Transactions on NanoBioscience, vol. 11, no. 2, pp. 89–99, 2012.

[40] Z. Han, D. Niyato, W. Saad, T. Başar, and A. Hjørungnes, Game theory in wireless and communication networks: theory, models, and applications. Cambridge university press, 2012.

[41] S. Boyd and L. Vandenberghe, Convex optimization. Cambridge university press, 2004.

[42] T. Seki, H. Kanbayashi, S. Chono, Y. Tabata, and K. Morimoto, “Effects of a sperminated gelatin on the nasal absorption of insulin,” International journal of pharmaceutics, vol. 338, no. 1-2, pp. 213–218, 2007.

[43] E. Bermek, R. Nurten, D. Tiryaki, and S. Gökçe, “Biyofizik ders notları,” İstanbul Üniversitesi Tıp Fak. Yayınları, no.

188, pp. 145–150, 1997.

DRAFT August 15, 2019