arXiv:1910.13756v1 [physics.plasm-ph] 30 Oct 2019

A note on the experiment parameters for the non-resonant streaming instability:

competition between left and right circularly polarized modes^�

Chun-Sung Jao^a, Sergei Vafin^{a,b}, Ye Chen^a, Matthias Gross^a, Mikhail Krasilnikov^a, Gregor Loisch^a, Timon Mehrling^c, Jacek Niemiec^d, Anne Oppelt^a, Alberto Martinez de la Ossa^e, Jens Osterhoff^c, Martin Pohl^{a,b}, Frank Stephan^a

aDESY, Zeuthen, Germany bInstitute of Physics and Astronomy, University of Potsdam, Potsdam-Golm, Germany cDESY, Hamburg, Germany dInstitute of Nuclear Physics PAN, Krakow, Poland eInstitute of Experimental Physics, University Hamburg, Germany

Abstract

A non-resonant streaming instability driven by cosmic-ray currents, also called Bell’s instability, is proposed as a candidate for providing the required magnetic turbulence of efficient diffusive shock accelerations. To demonstrate the saturation level and mechanism of the non-resonant streaming instability in a laboratory environment, we attempt to develop an experiment at the Photo Injector Test Facility at DESY, Zeuthen site (PITZ). As an electron beam is used to replace the proton beam to carry the cosmic-ray current in our experiment, the polarization of the non-resonant streaming instability will be modified from the left-handed (LH) mode to the right-handed (RH) mode. The theoretical instability analysis shows that the growth rate of this RH non-resonant mode may be smaller than it of the LH resonant mode. However the LH resonant mode can be ignored in our experiment while the expected wavelength is longer than the used plasma cell. The results of PIC simulations will also support this contention and the occurrence of non-resonant streaming instability in our experiment.

1. Introduction

With the progress of experimental technologies, laboratory astrophysics became an alternative method of astrophysical study besides the classical observations and numerical simulations. Via the connection between astrophysics and laboratory experiments, we seek to expand our understanding of physical processes by simulating the extreme astrophysical environments in the laboratory [1].

Bell’s instability is an electromagnetic streaming instability driven by cosmic-ray current, which is considered as a candidate for the amplification of the interstellar magnetic field [2]. This magnetic-field amplification is required to increase the efficiency of diffusive shock acceleration by confining cosmic-ray particles in the vicinity of the shock, which allows particles to gain energy through multiple shock crossing [3]. The analytical treatments based on Magnetohydrodynamics (MHD) and kinetic aspects both support the prospect of this non-resonant streaming instability in magnetic field amplification [2, 4, 5]. The nonlinear saturation level of the Bell’s instability at a few times the strength of the homogeneous magnetic field is also found in fully kinetic particle-in-cell (PIC) simulation [6, 7].

Email addresses: csjao899@gmail.com (Chun-Sung Jao),

ye.lining.chen@desy.de (Ye Chen), martin.pohl@desy.de (Martin

Pohl)_1

This work was first presented in the 12th International Conference on High Energy Density Laboratory Astrophysics (HEDLA18) in Kurashiki, Okayama, Japan. The respective proceedings were submitted to the Virtual Special Issue of High Energy Density Physics and were not accepted after the refereeing process.

To understand the problem of magnetic field amplification in astrophysics, we attempt to develop a laboratory experiment for Bell’s instability at the Photo Injector Test Facility at DESY, Zeuthen site (PITZ) [8]. However, numerous competing instabilities may occur in the so-called beam-plasma system [9]. To understand the characteristic of those unstable modes becomes essential for the preliminary study; for instance, to distinguish between the left- and right-circularly-polarized waves (or, says, the resonant and non-resonant modes) [10, 11]. In this paper, we will show the plan of selection for the non-resonant streaming instability in our experiment.

2. Photo Injector Test Facility at DESY, Zeuthen site (PITZ)

The Photo Injector Test facility at the Zeuthen site of DESY (PITZ) was built to test, develop and experimentally optimize high-brightness photoelectron sources for superconductinglinac-driven SASE FELs, such as the Free electron LASer in Hamburg (FLASH) and the European X-ray Free Electron Laser (European XFEL)[12, 13]. The main setup of PITZ consists of an L-band 1.6-Cell normal conducting (NC) RF gun, an L-band NC booster cavity, and various systems for electronbeam diagnostics, as shown in Fig. 1. Reliable production of high-quality electron beams by the PITZ gun along with its multiple beam diagnostics provide excellent opportunities for laboratory astrophysics.

For the proposed laboratory experiment of Bell’s instability at DESY, the PITZ gun will be used as electron source. The

Preprint submitted to arXiv October 31, 2019

Figure 1: General layout of the PITZ beam line.

plasma environment for inducing the instability will be provided by the Gas Discharge Plasma (GDP) cell of PITZ [14]. Based on available equipment of the PITZ accelerator, first beam-dynamics simulations have been performed for producing quasi-continuous-wave (cw) electron beams with an average beam current at the level of milliamperes and a mean beam energy of a few MeV as required for the laboratory experiments. The resulting beam parameters are: a peak beam current of 12 mA, an average current of about 2 mA, an RMS transverse beam size of about 1 mm and a mean kinetic beam energy of about 3 MeV. Such electron beams can be continuously injected into the plasma cell for a few ms, implying that the non-resonant streaming instability has to develop and saturate in a time period shorter than that.

Here we briefly summarize the physical conditions of the beam-plasma system at PITZ [8], which will be applied in the linear instability analysis. Our laboratory conditions allow the plasma density range from 10^{12} to 10^{15} cm^{−3} within a plasma column length up to 45 cm. The number density of the electron beam is expected to be in the range 10^8 to 10^9 cm^{−3}, the Lorentz factor in the range 5 to 10, and the beam radius around 1 mm. Since investigations of possible improvements of beam parameters are in progress [15], for the preparatory investigations,we extend the beam density range to 10^{11} cm^{−3}. In addition, the lowest value of the external magnetic field should be about 1 mT to avoid the effect of the geomagnetic field on the laboratory experiment, but we can be easily provide up to 0.1 T in our laboratory.

3. Characteristics of the non-resonant streaming instabilities

3.1. Bell’s MHD treatment

The MHD treatment is first employed for the linear instability analysis. In the Bell’s model [2], a cosmic-ray current is assumed to be directed along a background magnetic field, B_0, into a stationary and homogeneous plasma with number density n_0. The current density, j = n_bqv_b, is determined by the particle density,n_b, the charge, q, and the bulk velocity of cosmic-ray particles, v_b, respectively. The linear analysis indicates that a nearly purely growing, parallel propagating, nonresonant mode could be excited with peak growth rate [2, 4]

γ_{max} ≃ j 2 � μ_0 ρ at k_{max} ≃ j 2 μ_0 B_0

. (1)

Here ρ = m_in_0 is the density of background plasma and m_i is the mass of background ions. Significant magnetic-field perturbations can be expected for kr_{L,b} ≫ 1, where the Larmor radius of the beam particles, r_{L,b} = Γ_bm_bv_b/eB_0, is calculated using only the beam speed, v_b, and the rest mass of beam particles, m_b. The instability conditions can be rewritten as

Γ_bρ_bv^2_b 2 μ_0 B^2_0

≫ 1, (2)

which indicates that the kinetic energy of the beam must be much larger than the initial magnetic energy. Here Γ_b = (1 − v^2_b/c^2)^{−1/2} is the beam gamma-factor. For example, assuming an electron beam with number density 10^9 cm^{−3} drifting into a plasma system with the beam-parallel magnetic field of 0.1 T, a beam energy of at least 1 GeV is required to induce Bell’s instability.

The type of beam particles, electrons or ions, enters equations (1) and (2) only through v_b and m_b, and it is instructive to express these equations in terms of the electron plasma and Larmor frequency, ω_{pe} and ω_{ce}, and the rest masses of plasma ions and electrons, m_i and m_e, as well as that of the beam particles, m_b,

γ_{max} ≃ 1 2 v_b c � m_e m_i n_b n_e ω_{pe} at λ_{max} ≃ 4π c v_b n_e n_b ω_{ce} ω_{pe} c ω_{pe} . (3) As the beam-particle mass, m_b, does not appear in equation (3), we conclude that an electron beam can replace the proton beam, provided one considers electron and protons of the same speed, v_b, or with the same current density, v_bn_b = const.. This may appear to make electron beams favorable on account of their higher speed, but

k_{max}r_{L,b} ≃

Γ_b 2 v^2_b c^2 m_b m_e n_b n_e � ω_{pe} ω_{ce}

�_2 ≫ 1 ⇒ p_bv_b 2 m_ec^2 n_b n_e � ω_{pe} ω_{ce}

�_2

≫ 1, (4)

does contain m_b explicitly, which in the second line we express using the beam momentum, p_b,. We see that for the same current density (v_bn_b = const.) beam particles with higher momentum can more easily satisfy this condition. For the same beam energy that would favor proton beams.

In the MHD picture, the growth rate of the instability must be smaller than the gyro-frequency of background ions,

γ_{max} ω_{ci} ≃ 1 2 v_b c � m_i m_e n_b n_e ω_{pe} ω_{ce}

≪ 1 , (5)

which is also more difficult to maintain, if an electron beam is used in the experiment, as it limits the current density carried by the beam.

3.2. Kinetic aspect

To extend the linear treatment to a more general parameter regime, a kinetic theoretical model for the cold beam-plasma system is also employed for to understand the characteristics of the streaming instabilities, it also covers other instabilities in the beam-plasma system, which is helpful to understand the competition of instabilities in the nonlinear evolution processes.

Based on the electromagnetic dispersion equation, equation (A.4) shown in Appendix A, the solutions of ω_L, equation (A.6), and ω_R, equation (A.7), can describe the left and right circular polarization wave modes, respectively. As indicated, a variety of instabilities in the beam-plasma system with finite v_b is expected in both modes. In particular, while an electron beam is employed, the left-handed (LH) wave corresponds to the resonant instability, whereas the right-handed (RH) one to non-resonant [16] (more detail in Appendix A).

The maximum growth rate of the electron-beam-induced resonant streaming instability (LH mode, top panels) and nonresonant streaming instability (RH mode, bottom panels) are shown in Fig. 2. As indicated, with increasing external magnetic field (from B_0 = 0.001 T to 0.1 T), the linear growth rates of both the resonant and the non-resonant streaming instability increases significantly (from γ_{max} ∼ 10^5 Hz to ∼ 10^7 Hz). As one of the most basic conditions of our experiment, the growth rate has to be large enough for the instability to develop within both the beam duration and the plasma life time. Hence a stronger external magnetic field would be beneficial for our experiment. For example for B_0 = 0.1 T the density ratio n_b/n_e > 2.5 × 10^{−3} (the marked regime) would be required for an efficient development of the non-resonant RH mode.

To be noted from Fig. 2(c) is that the growth rate of the resonant LH mode can be larger than that of the non-resonant RH mode, if an electron beam is employed in our system [5]. However, as we shall see below, fitting the mode into the plasma cell imposes serious constraints on the parameters of the system. Adopting a strong external magnetic field, B_0 = 0.1 T, and the density ratio n_b/n_e > 2.5 × 10^{−3} (the marked regime in Fig. 2(c)), the wavelength of the most unstable resonant and non-resonant modes are shown in Fig. 3. We find that the resonant LH mode perturbation has a wavelength larger than our plasma cell (> 100 cm ), and we will set it aside in our preliminary study.

4. Comparison with PIC simulations

In addition to the linear instability analysis, to understand the properties of Bell’s instability induced by an electron beam, a fully relativistic, massively parallel particle-in-cell (PIC) code OSIRIS [17, 18, 19] is employed for the nonlinear calculations. As reported in our previous study [8], to mimic the laboratory environment, we assume a stationary plasma with number density n_0 = 10^{13} cm^{−3} within a two-dimensional periodic system in the z-x plane (72.8 cm × 3.0 cm) and a uniform, continuous, and infinite-width cold electron beam with relativistic Maxwellian momentum distribution drifting along the z direction. As the parameter set marked in Fig. 3, the constant number density and Lorentz factor of the electron beam are set to be n_b = 8.0 × 10^{10} cm^{−3} and Γ_b = 10, respectively, and the background magnetic field is set as B_0 = 0.1 T, which is also along the z direction. The background electrons initially drift in the −z direction for current neutrality. To reduce the computation time, the mass ratio between ions and electrons is set to be m_i/m_e = 50.

Before showing the simulation results, we perform a linear instability analysis for the simulation parameters. Based on the MHD-based Bell’s formula, the peak linear growth rate is expected to be γ_{max} = 1.01 × 10^8 Hz at the wavelength λ_{max} = 26.1 cm. The MHD assumption in Bell’s formula is satisfied, as γ_{max}/ω_{c,i} < 1. With the Larmor radius of beam electrons r_{L,b} = 17 cm, the criterion of Bell’s instability k_{max}r_{L,b} > 1 is fulfilled as well. Nevertheless, the fully kinetic linear analysis reveals an unstable mode in a broad wavelength range, λ > 15 cm, with predicted peak growth rate γ_{max} = 7.8×10^7 Hz at the wavelength λ_{max} ≃ 26 cm. The predicted peak growth rate from the kinetic model is smaller than that from the MHDbased formula but the wavelengths are similar.

Fig. 4 shows spatial maps of the magnetic field at T = 9.18×10^{−8} s (16384ω^{−1}_{ci} , panel (a)) and 1.61×10^{−7} s (32768ω^{−1}_{ci} , panel (b)). There is no obvious structure in the field component along the homogeneous field (B_z). As for the B_x and B_y components, the magnetic-field structures are coherent and correspond to circularly polarized plane waves travelling in the beam direction. The filamentation instability is totally suppressed by the limited size of the simulation system in the transverse direction. Moreover, we also see that the amplitude of magnetic-field perturbations induced by Bell’s instability, B_x and B_y, can grow to the level of background magnetic field (> 0.1T ), but the wavelength of the dominant magnetic field perturbation changes in the nonlinear evolution processes. By examining the time history of perturbed magnetic field at different wavelengths [8], the fastest growing modes, those with wavelength λ = 18.2 cm, 24.3 cm, and 36.4 cm, saturate around T ∼ 10^{−7} s, which corresponds to around 7 (or 10) growth times for our theoretical model (or Bell’s prediction). In particular, the wave modes with wavelength λ = 36.4 cm has highest saturation level, and the short-wavelength mode with λ = 18.2 cm saturates at a lower level. As for other wave modes with more shorter wavelengths, such as λ = 14.6 cm and 12.1 cm, which are stable modes in the linear analysis, the perturbations are always small and only at the level of numerical noise.

5. Discussion and Summary

A non-resonant instability driven by cosmic-ray currents, also called Bell’s instability, is a candidate for providing the magnetic-field amplification needed for efficient diffusive shock acceleration. To understand its mechanism and properties, a laboratory experiment for Bell’s instability is planned at DESY. The required electron source and plasma environment are proposed to be provided by the PITZ accelerator. The possibility of generating quasi-cw electron beams has been studied at PITZ based on a specially designed field emitter and velocity bunching by the booster cavity [15].

Figure 2: Maximum growth rate (in units Hz) of the left-handed resonant mode (top panels) and right-handed non-resonant mode (bottom panels) of the electron beam induced electromagnetic streaming instability as function of the beam-to-plasma density ratio and beam gamma-factor with fixed parameters n_e = 10^{13} cm^{−3} and (a) B_0 = 0.001 T , (b) B_0 = 0.01 T, and (c) B_0 = 0.1 T. We adopt the marked parameter regime in panel (c) for the further linear analysis.

In our preliminary studies, we first use linear analysis to examine the most basic physical conditions that permit Bell’s instability to occur in the laboratory, the linear growth rate and corresponding wavelength in particular. Both Bell’s MHDbased treatment and our kinetic theoretical model are employed, but only the kinetic model can work outside of the MHD limit and include temperature and anisotropy effects. The kinetic model can also provide linear analysis of other instabilities in the beam-plasma system. The linear instability analysis predicts the wavelength range of the unstable modes of both left and right circular polarization modes.

While an electron beam is employed in our beam-plasma system, the right circular polarization mode is expected to be the one corresponding to the non-resonant streaming instability. According to our laboratory parameters, even the growth rate of the resonant LH mode is generally larger than the non-resonant RH mode, the resonant LH mode can still be set aside in our preliminary study due to its over-wavelength. In other words, only the non-resonant RH mode can occur in our experiment while its wavelength is predicted to be far smaller than the size of our plasma cell. The presented PIC simulations also support this contention; in particular, the simulation results shows the occurrence of the electron-beam induced Bell’s instability as well as the saturation level and the spectrum of magneticfield fluctuations, which also defend the possibility to simulate Bell’s instability at PITZ. In the context of a real experiment, the simulations are indispensable for determining the feasibility of Bell’s instability in the laboratory. By using the B-dot probe as magnetic-field detector [20], we may measure the time evolution and spatial profile of magnetic field perturbations in the plasma cell. A comparison with the simulation data would then reveal whether or not the characteristics of the magnetic turbulence (says, growth rate and the corresponding wavelength) are consistent the properties of the fully evolved Bell’s mode.

Appendix A. kinetic theoretical modelling for the cold beam-plasma system

To study the electromagnetic streaming instability for parallel orientation of the wave vector with respect to the ambient homogeneous magnetic field B_0 [21, 22], the following plasma system is considered. In the cold beam-plasma approximation, the distribution functions of the beam, background electrons and ions, respectively, are described by

f_b(p_⊥, p_z) = n_b δ(p_⊥) 2πp_⊥ δ(p_z − p_b), (A.1)

f_e(p_⊥, p_z) = n_e δ(p_⊥) 2πp_⊥ δ(p_z − p_e), (A.2)

f_i(p_⊥, p_z) = n_i δ(p_⊥) 2πp_⊥ δ(p_z). (A.3)

The bulk momentum of the background electrons, p_e, drifting along the magnetic field (z-axis) is set for the current neutrality. Then we derive the well-known dispersion equation [23]

Figure 3: The wavelength of the instability (in units cm) of the most unstable left-handed resonant mode (top panel) and right-handed non-resonant mode (bottom panel) of the electron beam induced electromagnetic streaming instability as function of the beam-to-plasma density ratio and beam gamma-factor. The other (fixed) parameters are B_0 = 0.1 T and n_e = 10^{13} cm^{−3}. We adopt the set of red-star-marked parameters for the further numerical simulation.

1 − � kc ω �_2 − ω^2_{pi} ω(ω ± ω_{ci}) − ω^2_{pb} ω^2 ω − kv_b Γ_b(ω − kv_b ± ω_{cb}/Γ_b) − ω^2_{pe} ω^2 ω − kv_e Γ_e(ω − kv_e ± ω_{ce}/Γ_e)

= 0, (A.4)

which can be simplified to a quadratic equation

ω^2 + x_{L,R}ω ± x_{L,R}ω_{ci} = 0, (A.5)

under the assumptions, |ω − kv_e| ≪ |ω_{ce}| /Γ_e, |kc/ω| ≫ 1, and |ω| ≪ |kv_b ∓ ω_{cb}/Γ_b|. The analytical solution of equation (A.5) are ω_L = 1 2 � −x_L + � x_L(x_L + 4ω_{ci}) � , (A.6)

ω_R = 1 2 � −x_R + � x_R(x_R − 4ω_{ci}) � , (A.7)

where x_L =

(kV_A)^2 ω_{ci} + α e_b e_e

(kv_b)^2 kv_b + ω_{cb}/Γ_b

, (A.8) x_R = −

(kV_A)^2 ω_{ci} + α e_b e_e

(kv_b)^2 kv_b − ω_{cb}/Γ_b

, (A.9)

α = n_b/n_e, V_A = B_0/(4πn_im_i)^{1/2}. For v_b = 0, equations (A.6) and (A.7) describe purely oscillating Alfvén-proton-cyclotron and whistler fluctuations, respectively. In addition, solutions of ω_L, equation (A.6), and ω_R, equation (A.7), will be complex while −4ω_{ci} < x_L < 0 and 0 < x_R < 4ω_{ci}, respectively, which indicates a variety of instabilities in the beam-plasma system.

Based on equations (A.6) and (A.7), we can find analytical expressions for the maximum growth rates and corresponding wavenumber (wavelength) of the unstable modes. While the assumption |ω| ≪ |kv_b ∓ ω_{cb}/Γ_b| will be easily violated for the resonant instabilities, here we will consider only nonresonant modes for the limiting case |x_{L,R}| ≲ 0.5ω_{ci}. Thus, equations (A.6) and (A.7) reduce to

ω_L = − x_L 2 + √ ω_{ci} x_L, (A.10)

ω_R = − x_R 2 + √ −ω_{ci} x_R. (A.11) Then the instability conditions are simply x_L < 0 and x_R > 0, which can be evaluated as the instability conditions for an electron (RH mode) and proton (LH mode) beam, respectively,

0 < k < ω_{ce} Γ_bv_b + α ω_{ci} v_b � v_b V_A

�_2

, and (A.12)

0 < k < − ω_{ci} Γ_bv_b + α ω_{ci} v_b � v_b V_A

�_2

. (A.13)

Equations (A.12) and (A.13) can both be inferred as the instability conditions shown in equations (2). The maximum growth rates are

γ_{max,L,R} = k_{L,R}V_A � � � 3 − � 1 + 2/a_{L,R} 1 + � 1 + 2/a_{L,R} � � � 1/2 , (A.14)

where

k_L = ω_{ci} v_bΓ_b � −1 + a_L � 1 + � 1 + 2/a_L � , (A.15)

k_R =

|ω_{ce}| v_bΓ_b � −1 + a_R � 1 + � 1 + 2/a_R � , (A.16)

a_L = αΓ_bm_p 4m_i � v_b V_A

�_2

, (A.17)

a_R = αΓ_bm_e 4m_i � v_b V_A

�_2

. (A.18)

Additionally, we have assumed that the background plasma is singly ionized which is the case in many applications. For a_{L,R} ≫ 1, we find γ_{max,L,R} = k_{L,R}V_A, (A.19)

k_L =

2a_L ρ_p

, (A.20)

k_R =

2a_R ρ_e

, (A.21)

in agreement with equations (1) and (3) in the Bell’s MHD treatment. 5

Figure 4: Spatial maps of the magnetic-field components B_x (top panel), B_y (middle panel), and B_z (bottom panel) at (a) 9.18×10^{−8} s (16384ω^{−1}_{ci} ) and (b) 1.61×10^{−7} s (32768ω^{−1}_{ci} ) for the electron-beam-induced Bell’s instability.

Acknowledgements

This research is supported by the Deutsches Elektronen- Synchrotron (DESY) Strategy Fund. The computational resources for the numerical simulations are provided by DESY and the Norddeutsche Verbund zur Förderung des Hoch- und Höchstleistungsrechnens (HLRN). The work of J. N. is supported by Narodowe Centrum Nauki through research project DEC-2013/10/E/ST9/00662.

References

[1] W. E. Amatucci, A review of laboratory investigations of space plasma waves, URSI Radio Science Bulletin 2006 (319) (2006) 32–66.

[2] A. R. Bell, Turbulent amplification of magnetic field and diffusive shock acceleration of cosmic rays, MNRAS 353 (2004) 550–558.

[3] K. M. Schure, A. R. Bell, L. O’C Drury, A. M. Bykov, Diffusive shock acceleration and magnetic field amplification, Space Science Reviews 173 (1) (2012) 491–519.

[4] V. N. Zirakashvili, V. S. Ptuskin, Diffusive shock acceleration with magnetic amplification by nonresonant streaming instability in supernova remnants, ApJ 678 (2008) 939.

[5] E. Amato, P. Blasi, A kinetic approach to cosmic-ray-induced streaming instability at supernova shocks, MNRAS 392 (2009) 1591.

[6] J. Niemiec, M. Pohl, A. Bret, T. Stroman, Aperiodic magnetic turbulence produced by relativistic ion beams, The Astrophysical Journal 709 (2) (2010) 1148.

[7] O. Kobzar, J. Niemiec, M. Pohl, A. Bohdan, Spatio-temporal evolution of the non-resonant instability in shock precursors of young supernova remnants, Monthly Notices of the Royal Astronomical Society 469 (4) (2017) 4985–4998.

[8] C.-S. Jao, S. Vafin, Y. Chen, M. Gross, M. Krasilnikov, G. Loisch, T. Mehrling, J. Niemiec, A. Oppelt, A. M. de la Ossa, J. Osterhoff, M. Pohl, F. Stephan, Preliminary study for the laboratory experiment of cosmic-rays driven magnetic field amplification, High Energy Density Physics 32 (2019) 31 – 43.

[9] A. Bret, Weibel, two-stream, filamentation, oblique, bell, buneman...

which one grows faster?, The Astrophysical Journal 699 (2) (2009) 990– 1003.

[10] M. S. Weidl, D. Winske, C. Niemann, On the background-gyroresonant

character of bell’s instability in the large-current regime, The Astrophysical Journal 872 (1) (2019) 48.

[11] M. S. Weidl, D. Winske, C. Niemann, Three regimes and four modes for the resonant saturation of parallel ion-beam instabilities, The Astrophysical Journal 873 (1) (2019) 57.

[12] F. Stephan, M. Krasilnikov, High brightness photo injectors for brilliant light sources, in: E. Jaeschke, S. Khan, J. R. Schneider, J. B. Hastings (Eds.), Synchrotron Light Sources and Free-Electron Lasers: Accelerator Physics, Instrumentation and Science Applications, Springer International Publishing, Cham, 2014, pp. 1–38.

[13] Y. Chen, M. Krasilnikov, F. Stephan, E. Gjonaj, T. Weiland, M. Dohlus, Modeling and simulation of rf photoinjectors for coherent light sources, Nuclear Inst. and Methods in Physics Research, A 889 (2018) 129 – 137.

[14] G. Loisch, et al., Experimental Investigation of High Transformer Ratio Plasma Wakefield Acceleration at PITZ, in: Proceedings, 8th International Particle Accelerator Conference: Denmark, 2017, p. TUPIK018.

[15] Y. Chen, G. Loisch, M. Gross, C.-S. Jao, M. Krasilnikov, A. Oppelt, et al., Generation of quasi continuous-wave electron beams in an l-band normal conducting pulsed rf injector for laboratory astrophysics experiments, Nuclear Inst. and Methods in Physics Research, A 903 (2018) 119 – 125.

[16] A. B. Mikhailovskii, Theory of plasma instabilities, Vol 1: instabilities of a homogeneous plasma, Springer, 1974.

[17] R. A. Fonseca, L. O. Silva, F. S. Tsung, V. K. Decyk, W. Lu, C. Ren, W. B. Mori, S. Deng, S. Lee, T. Katsouleas, J. C. Adam, Osiris: A threedimensional, fully relativistic particle in cell code for modeling plasma based accelerators, in: P. M. A. Sloot, A. G. Hoekstra, C. J. K. Tan, J. J. Dongarra (Eds.), Computational Science — ICCS 2002, Springer Berlin Heidelberg, Berlin, Heidelberg, 2002, pp. 342–351.

[18] R. A. Fonseca, S. F. Martins, L. O. Silva, J. W. Tonge, F. S. Tsung, W. B. Mori, One-to-one direct modeling of experiments and astrophysical scenarios: pushing the envelope on kinetic plasma simulations, Plasma Physics and Controlled Fusion 50 (12) (2008) 124034.

[19] R. A. Fonseca, J. Vieira, F. Fiuza, A. Davidson, F. S. Tsung, W. B. Mori, L. O. Silva, Exploiting multi-scale parallelism for large scale numerical modelling of laser wakefield accelerators, Plasma Physics and Controlled Fusion 55 (12) (2013) 124011.

[20] E. T. Everson, P. Pribyl, C. G. Constantin, A. Zylstra, D. Schaeffer, N. L.

Kugland, C. Niemann, Design, construction, and calibration of a threeaxis, high-frequency magnetic probe (b-dot probe) as a diagnostic for exploding plasmas, Review of Scientific Instruments 80 (11) (2009) 113505.

[21] R. Schlickeiser, Relativistic kinetic theory of plasma waves, Phys. Scr.

T75 (1998) 33.

[22] M. Lazar, R. Schlickeiser, Relativistic kinetic dispersion theory of linear parallel waves in magnetized plasmas with isotropic thermal distributions, New J. Phys. 8 (2006) 66.

[23] B. B. Kadomtsev, Reviews of plasma physics., Reviews of Plasma Physics 15.