arXiv:2112.05189v1 [math.GM] 9 Dec 2021

An approximate numerical method for ordinary differential equation systems with applications to a flight mechanics model

Fabio Silva Botelho Department of Mathematics Federal University of Santa Catarina Florianópolis - SC, Brazil

Abstract This short communication develops a new numerical procedure suitable for a large class of ordinary differential equation systems found in models in physics and engineering. The main numerical procedure is analogous to those concerning the generalized method of lines, originally published in the here referenced books of 2011 and 2014, [3, 5] respectively. Finally, in the last section, we apply the method to a model in flight mechanics.

1 Introduction

Consider the first order system of ordinary differential equations given by du_j dt = f_j({u_l}), on [0, t_f ] ∀j ∈ {1, · · · , 4}, with the boundary conditions

u_1(0) = 0, u_2(0), u_4(0) = 0, u_4(t_f ) = u_f .

Here u = {u_l} ∈ W^{1,2}([0, t_f ], R^4 ) and f_j are functions at least of C^1 class, ∀j ∈ {1, 2, 3, 4}. Our proposed method is iterative so that we choose an starting solution denoted by ũ. At this point, we define the number of nodes on [0, t_f ] by N and set d = t_f /N. Similarly to a proximal approach, we propose the following algorithm (in a similar fashion as those found in [3, 5, 4]).

1. Choose ũ ∈ W^{1,2}([0, t_f ], R^4 ). 2. Solve the equation system K du_j dt − (K − 1) dũ_j dt = f_j({u_l}), on [0, t_f ] ∀j ∈ {1, · · · , 4}, (1) with the boundary conditions

u_1(0) = 0, u_2(0), u_4(0) = 0, u_4(t_f ) = u_f .

3. Replace ũ by u and go to item (2) up to the satisfaction of an appropriate convergence criterion.

In finite differences, observe that the system may be approximated by

(u_j )_n − (u_j )_{n−1} = K − 1 K ((ũ_j )_n − (ũ_j )_{n−1}) + f_j({(u_l)_{n−1}}) d K In particular, for n = 1, we get

(u_j )_1 = (u_j )_0 + f_j({(u_l)_1}) d K + K − 1 K ((ũ_j )_1 − (ũ_j )_0) + (E_j )_1,

where (E_j )_1 = [f_j({(u_l)_0}) − f_j({(u_l)_1})] d K ≈ O ( d^2 K ) . Similarly, for n = 2 we have

(u_j )_2 − (u_j )_0 = [(u_j )_2 − (u_j )_1] + [(u_j )_1 − (u_j )_0]

= f_j({(u_l)_1}) d K + K − 1 K ((ũ_j )_2 − (ũ_j )_1)

+f_j({(u_l)_1}) d K + K − 1 K ((ũ_j )_1 − (ũ_j )_0) + (E_j )_1

= 2f_j ({(u_l)_1}) d K − 2f_j ({(u_l)_2}) d K + 2f_j ({(u_l)_2}) d K + K − 1 K ((ũ_j )_2 − (ũ_j )_0) + (E_j )_1, (2)

Summarizing

(u_j )_2 = (u_j)_0 + 2f_j ({(u_l)_2}) d K + K − 1 K ((ũ_j )_2 − (ũ_j )_0) + (E_j )_2,

where (E_j )_2 = (E_j )_1 + (f_j({(u_l)_1}) − f_j({(u_l)_2})) 2d K . Reasoning inductively, for all 1 ≤ k ≤ N, we obtain

(u_j )_k = (u_j )_0 + f_j({(u_l)_k}) kd K + K − 1 K ((ũ_j )_k − (ũ_j )_0) + (E_j )_k,

where,

(E_j )_k = (E_j )_{k−1} + k(f_j({u_l}_{k−1}) − f_j({u_l}_k) d K = k∑ m=1 (k − m + 1)[f_j ({(u_l)_{m−1}}) − f_j({(u_l)_m})] d K ≈ O ( (k^2 + k)d^2 2K ) , (3) ∀j ∈ {1, · · · , 4}. In particular, for k = N, for K > 0 sufficiently big, we obtain

(u_j )_N = (u_j )_0 + f_j({(u_l)_N }) Nd K + K − 1 K ((ũ_j )_N − (ũ_j )_0) + (E_j )_N

≈ (u_j )_0 + f_j({(u_l)_N }) Nd K + K − 1 K ((ũ_j )_N − (ũ_j )_0), ∀j ∈ {1, 2, 3, 4}. (4)

In such a system we have 4 equations suitable to find the unknown variables (u_0)_3, (u_N )_1, (u_N )_2, (u_N )_3, considering that (u_N )_4 = (u_4)_f is known.

Through the system (4) we obtain u_N through the Newton’s Method for a system of only the 4 indicated variables.

Having u_N , we obtain u_{N−1} through the equations

(u_j )_N − (u_j )_{N−1} ≈ f_j({(u_l)_{N−1}}) d K + K − 1 K ((ũ_j )_N ) − (ũ_j )_{N−1}),

also through the Newton’s Method.

Similarly, having u_{N−1} we obtain u_{N−2} through the system

(u_j )_{N−1} − (u_j )_{N−2} ≈ f_j({(u_l)_{N−2}}) d K + K − 1 K ((ũ_j )_{N−1}) − (ũ_j )_{N−2}),

and so on up to finding u_1.

Having calculated u, we replace ũ by u and repeat the process up to an appropriate convergence criterion is satisfied.

The problem is then approximately solved.

2 Applications to a flight mechanics model

We present numerical results for the following system of equations, which models the in plane climbing motion of an airplane (please, see more details in [7]).

ḣ = V sin γ, γ̇ =^1_{mf V} (F sin[a + a_F ] + L) −^g_V cos γ, V̇ =^1_{mf} (F cos[a + a_F ]) − D) − g sin γ ẋ = V cos γ, (5)

with the boundary conditions, h(0) = h_0, V (0) = V_0 x(0) = x_0 h(t_f ) = h_f , (6)

where t_f = 532s, h is the airplane altitude, V is its speed, γ is the angle between its velocity and the horizontal axis, and finally x denotes the horizontal coordinate position.

For numerical purposes, we assume (Air bus 320) m_f = 120, 000Kg, S_f = 260m^2, a = 0.0945 rad, g = 9.8m/s^2,

ρ(h) = 1.225(1 − 0.0065h/288.15)^{4.225} Kg/m^3, a_F = 0.03225, (C_L)_a = 5 (C_D)_0 = 0.0175, K_1 = 0.0, K_2 = 0.06 C_L = (C_D)_0 + K1C_L + K_2C^2_L, L = 1 2 ρ(h)V^2C_LS_f , D = 1 2 ρ(h)V^2C_DS_f ,

F = 240000 and where units refer to the International System.

To simplify the analysis, we redefine the variables as below indicated:

h = u_1, γ = u_2 V = u_3 x = u_4. (7)

Thus, denoting u = (u_1, u_2, u_3, u_4) ∈ U = W^{1,2}([0, t_f ]; R^4 ), the system above indicated may be expressed by

u̇_1 = f_1(u) u̇_2 = f_2(u) u̇_3 = f_3(u) u̇_4 = f_4(u), (8)

where,

f_1(u) = u_3 sin(u_2), f_2(u) =^1_{mf u3} (F sin[a + a_F ] + L(u)) −^g_{u3} cos(u_2), f_3(u) =^1_{mf} (F cos[a + a_F ] − D(u)) − g sin(u_2) f_4(u) = u_3 cos(u_2). (9)

We solve this last system for the following boundary conditions:

h(0) = 0 m, V (0) = 150m/s, x(0) = 0 m, h(t_f ) = 11000 m.

(10)

We have obtained the following solutions for h, γ, V and x. Please see figures 1, 2, 3 and 4, respectively. We have set N = 3000 nodes and K = 509.

Figure 1: The solution h (in m) for t_f = 532s.

Figure 2: The solution γ (in rad) for t_f = 532s.

Figure 3: The solution V (in m/s) for t_f = 532s.

Figure 4: The solution x (in m) for t_f = 532s.

3 Acknowledgements

The author is grateful to Professor Pedro Paglione of Technological Institute of Aeronautics, ITA, SP-Brazil, for his valuable suggestions and comments which help me a lot to improve some important parts of this text, in particular on the part concerning the model in flight mechanics addressed.

References

[1] R.A. Adams and J.F. Fournier, Sobolev Spaces, 2nd edn. (Elsevier, New York, 2003).

[2] F. Botelho, Existence of solution for the Ginzburg-Landau system, a related optimal control problem and its computation by the generalized method of lines, Applied Mathematics and Computation, 218, 11976-11989, (2012).

[3] F. Botelho, Topics on Functional Analysis, Calculus of Variations and Duality, Academic Publications, Sofia, (2011).

[4] F.S. Botelho, Functional Analysis, Calculus of Variations and Numerical Methods in Physics and Engineering, CRC Taylor and Francis, Florida, 2020.

[5] F.S. Botelho, Functional Analysis and Applied Optimization in Banach Spaces, (Springer Switzerland, 2014).

[6] J.C. Strikwerda, Finite Difference Schemes and Partial Differential Equations, SIAM, second edition (2004).

[7] N.X. Vinh, Flight Mechanics of High Performance Aircraft, (Cambridge University Press, New York, 1993)