arXiv:2501.09207v1 [physics.optics] 15 Jan 2025

Relationship between total reflection and Fabry-Perot bound states in the continuum

Zitao Mai and Ya Yan Lu Department of Mathematics, City University of Hong Kong, Kowloon, Hong Kong, China (Dated: January 19, 2025)

Bound states in the continuum (BICs) have interesting properties and important applications in photonics. A particular class of BICs are found in Fabry-Perot (FP) cavities formed by two parallel periodic dielectric layers separated by a distance h. A periodic dielectric layer can totally reflect a plane incident wave with a particular frequency and a particular wavenumber. Existing FP-BICs are found when h is close to the values deduced from a phase-matching condition related to the reflection coefficient, but they are obtained in FP-cavities where the periodic layers have a reflection symmetry in the periodic direction. In this paper, we further clarify the connection between total reflections and FP-BICs. Our numerical results indicate that if the wavenumber is zero or the periodic layers have a reflection symmetry in the periodic direction, FP-BICs can indeed be found near the parameters of total reflections. However, if the wavenumber is nonzero and the periodic layer is asymmetric (in the periodic direction), we are unable to find a FP-BIC (with a frequency and a wavenumber near those of a total reflection) by tuning h or other structural parameters. Consequently, a total reflection does not always lead to a FP-BIC even when the parameters of the FP-cavity are tuned.

I. INTRODUCTION

In recent years, many studies on photonic bound states in the continuum (BICs) and their applications have been reported [1–6]. In open linear wave systems, a BIC is a localized eigenmode with a frequency in the radiation continuum [7]. By perturbing the ideal structure with a BIC or changing the wavevector, resonant states with arbitrarily high quality factors (Q factors) can be created [8– 10], leading to strong local field enhancement [11, 12], sharp features in transmission and reflection spectra [13– 15], and numerous applications in photonics [16, 17]. It is known that BICs are formed through different physical mechanisms, such as symmetry mismatch and destructive interference [7]. Some BICs are robust against small structural perturbations that preserve the relevant symmetry [18–20]. A nonrobust BIC is usually destroyed by an arbitrary perturbation, but is may survive if the perturbation contains one or more tunable parameters [21]. In structures with two periodic or translationally invariant directions, an electromagnetic BIC is a polarization singularity, can be associated with an integer topological charge [18, 22], and be observed as a polarization vortex in momentum space [23, 24]. Some special BICs, the so-called super-BICs or merging BICs [6, 8, 10, 25–28], turn to ultra-high-Q resonances when the wavevector is perturbed, and they also exhibit bifurcations when the structure is perturbed [29].

A Fabry-Perot (FP) BIC is a special eigenmode in a FP-cavity formed by two parallel thin mirrors separated by a distance, where the mirror can be a loseless dielectric periodic layer with one- or two-dimensional periodicity, such as a periodic array of dielectric cylinders [1, 30] or a photonic crystal slab [31]. The BIC is trapped between two mirrors and has only an evanescent field outside the cavity. For the same frequency and wavevector as the BIC, plane waves can propagate to or from infinity and partially transmit through the mirrors. It appears that

FP-BICs are first found for linearized water waves in two dimensions, where the “mirrors” are a pair of identical and infinitely long solid cylinders parallel to the water surface [32–34]. It is also known that FP-BICs exist in closed waveguides [35]. In that case, the FP-cavity is formed by placing two scatterers in the waveguide core, and the propagating modes of the waveguide, instead of plane waves, serve as the radiation channels. The appearance of FP-BICs has been explained as the destructive interference of two resonances coupled to a single radiation channel [7], but the theory is approximate and does not give definite predictions on the existence and nonexistence of FP-BICs.

In between the two mirrors, the wave field of a FP- BIC is dominated by propagating waves that are selfconsistently reflected by the mirrors. It is natural to look for FP-BICs around the frequency and wavevector at which a propagating wave is totally reflected by the mirror, and set the distance between the two mirrors by a phase matching condition related to the reflection coefficient [1, 33–35]. However, due to the existence of evanescent waves, the FP-cavity with such a distance does not usually have a BIC. When a plane wave impinges upon a periodic layer (i.e. the mirror), an infinite number of evanescent diffraction orders are excited. The evanescent waves excited at one mirror can generate transmitted and reflected propagating waves (of small amplitudes) at the other mirror, leading to radiations outside the FP-cavity. Therefore, the natural question is whether the FP-cavity with a slightly different distance can have a BIC. Existing studies indicate that the answer appears to be yes, but the results are either obtained numerically for special structures with particular parameters [1, 30, 33, 34] or asymptotically for special structures as the distance tends to infinity [35]. Moreover, the FP- BICs in closed waveguides are characterized by the frequency only, namely, they do not have a wavevector for the transverse direction. symmetric structues. The existing numerical studies for FP-BICs in periodic structures have focused on symmetric structures only [1, 30, 31].

In this paper, we present accurate numerical results to further clarify the relation between total reflections and FP-BICs, taking into account the different symmetry of the structure, the wavevector for transverse spatial variables, and structural parameters in addition to the distance. In most cases, we show that FP-BICs indeed exist when the distance between the two mirrors or other parameters are slightly adjusted. But if the periodic structure does not have a reflection symmetry in the periodic direction and the wavenumber is nonzero, we show that FP-BICs may not exist when structural parameters are slightly tuned.

The rest of the paper is organized as followed. In Sec. II, we recall the definitions and basic properties for diffraction and eigenvalue problems involving a periodic structure with a 1D periodicity, and clarify the assumptions about total reflections and BICs. In Sec. III, we derive an approximate condition for FP-BICs using one propagating and one evanescent waves. Numerical examples for FP-BICs in periodic structures with different symmetry are presented in Sec. IV. The paper is concluded with some remarks in Sec. V.

II. PRELIMINARIES

In this section, we describe single-layer and doublelayer (Fabry-Perot) structures and recall the definitions and basic properties of total reflections and BICs. First, we define a dielectric periodic layer in a Cartesian coordinate system with spatial variables {x, y, z}. The periodic layer is given for −d < z < d by a real dielectric function ϵ_p(y, z) which is independent of x and periodic in y with period L. Assuming this periodic layer is surrounded by air, the dielectric function for the entire single-layer structure is then

ϵ^{(1)}(y, z) = { ϵ_p(y, z), |z| < d, 1, |z| > d. (1) In Fig. 1, we show a schematic of a FP-cavity. It consists of two identical periodic layers separated by a distance h. These two layers are perpendicular to the z axis with their middle planes at z = ±(h/2 + d), respectively. In addition, we let the upper periodic layer be the mirror reflection of the lower layer, so that the resulting FP-cavity has an up-down reflection symmetry. The dielectric function of the entire double-layer structure is

ϵ^{(2)}(y, z) = ϵ_p(y, z + d + h/2), −D < z < −h/2, ϵ_p(y, d + h/2 − z), h/2 < z < D, 1, otherwise, (2) where D = 2d + h/2.

For both single- and double-layer structures, we consider time-harmonic electromagnetic waves that are invariant in x and depend on time as e^{−iωt}, where ω is the

FIG. 1. A Fabry-Perot cavity consisting of two periodic layers seperated by a distance h. The periodic layers are invariant in x, periodic in y with period L, perpendicular to the z axis, and have a thickness of 2d. They are mirror reflections (with respect to the z = 0 plane) of each other.

angular frequency. For the E-polarization, the x component of the electric field, denoted as u, satisfies the following Helmholtz equation

∂^2_y u + ∂^2_z u + k^2_0 ϵ(y, z)u = 0 (3)

where k_0 = ω/c is the free space wavenumber and c is the speed of light in vacuum, and ϵ is either ϵ^{(1)} or ϵ^{(2)}.

For the single-layer structure, we consider the diffraction of a plane incident wave u^{(i)} = e^{i[β0y−γ0(z−d)]}, z > d, (4) specified above the layer, where β_0 ∈ (−π/L, π/L], |β_0| < k_0, and γ_0 = (k^2_0 − β^2_0 )^{1/2} > 0. The total wave u satisfies Eq. (3) for ϵ = ϵ^{(1)}, and can be written as u = u^{(i)} + u^{(r)} for z > d and u = u^{(t)} for z < −d, respectively, where u^{(r)} and u^{(t)} are the reflected and transmitted waves, and they can be expanded as

u^{(r)} = ∞∑ m=−∞ R_{m,0} e^{i[βmy+γm(z−d)]}, z > d, (5)

u^{(t)} = ∞∑ m=−∞ T_{m,0} e^{i[βmy−γm(z+d))]}, z < −d, (6) where

β_m = β_0 + 2πm L , γ_m = √ k^2_0 − β^2_m (7)

are wavenumbers of the m-th diffraction order, R_{m,0} and T_{m,0} are the corresponding reflection and transmission coefficients. In the following, we assume

|β_0| < k_0 = ω c < 2π L − |β_0|. (8) In that case, for all m ≠ 0, γ_m is purely imaginary with a positive imaginary part, the zeroth diffraction order is the only propagating order, and the power balance law implies that |T_{0,0}|^2 + |R_{0,0}|^2 = 1.

It is known that T_{0,0} can sometimes be exactly zero for a real frequency ω^∗ and a real wavenumber β^∗_0 [36]. In that case, |R_{0,0}| = 1, and the power of the incident wave is completely converted to the reflected wave. This phenomenon, referred to as zero transmission or total reflection, is robust when the periodic layer has the relevant symmetry [14, 36]. More precisely, if ϵ_p is symmetric in y or z, namely, ϵ_p(−y, z) = ϵ_p(y, z) or ϵ_p(y, −z) = ϵ_p(y, z), and if zero transmission occurs at a real pair (ω^∗, β^∗_0 ), then for any sufficiently small loseless perturbation of ϵ_p that preserves the symmetry in y or z, the zero transmission phenomenon still occurs, either at a frequency near ω^∗ for the same β^∗_0 , or at a wavenumber near β^∗_0 for the same ω^∗. It should be noted that robustness is not and does not imply existence. It is rather difficult to specify conditions on ϵ_p to guarantee the occurrence zerotransmission phenomenon, but some limited results are available [13, 15, 35]. On the other hand, assuming the existence of a zero transmission, it is possible to derive approximate formulas for ω^∗ or β^∗_0 [37, 38].

For the FP-cavity, we are interested in guided modes satisfying Eq. (3) with ϵ = ϵ^{(2)} and the boundary condition u → 0 as z → ±∞. Due to the periodicity in y, any guided mode is given in the Bloch form u(y, z) = e^{iβ0y}ϕ(y, z), (9) where β_0 ∈ (−π/L, π/L] and ϕ is periodic in y with period L. For |z| > D, we can expand u as u(y, z) = ∞∑ m=−∞ c^±_me^{i(βmy±γmz)}, ±z > D, (10) where β_m and γ_m are given in Eq. (7). Regular guided modes exist below the light line, i.e., k_0 < |β_0|, and they depend on β_0 and ω continuously. A BIC is also a guided mode, but it exists above the light line, i.e., k_0 > |β_0|. For simplicity, we assume condition (8) is satisfied. In that case, γ_0 is positive and all γ_m for m ≠ 0 are purely imaginary. Since for any guided mode, u → 0 as z → ±∞, we must have c^±_0 = 0.

If L is the true minimum period in y, i.e., the structure is not periodic with period L/n for any integer n ≥ 2, BICs appear as isolated points in the β_0-ω plane. Let β^⋄_0 and ω^⋄ be the Bloch wavenumber and the frequency of a BIC, then for a real β_0 near β^⋄_0 , Eq. (3) with ϵ = ϵ^{(2)} has a resonant state satisfying Eqs. (9) and (10) with a complex frequency ω and a nonzero c^±_0 . Since the resonant state radiates power to z = ±∞ through the outgoing plane waves e^{i(β0y±γ0z)}, it must decay with time and has a negative Im(ω). Consequently, Im(γ_0) is also negative and e^{±iγ0 z} is unbounded as z → ±∞. The Q factor of the resonant state, Q = −0.5Re(ω)/Im(ω), usually satisfies Q ∼ 1/|β_0 − β^⋄_0 |^2, but for some special BICs (the so-called super-BICs), Q ∼ 1/|β_0 − β^⋄_0 |^m for m ≥ 4.

If the single periodic layer exhibits a total reflection with frequency ω^∗ and wavenumber β^∗_0 , we can determine the distance h of the FP-cavity, such that the plane wave between the mirrors is self-consistently reflected. Let the reflection coefficient be R_{0,0} = e^{iθ∗} for some θ^∗ ∈ (−π, π] and γ^∗_0 = √ (ω^∗/c)^2 − (β^∗_0 )^2. When the plane wave is reflected by the lower mirror at z = −h/2, travels to the upper mirror, is reflected by the upper mirror at z = h/2, and travels down to the lower mirror again, it acquires the phase 2(θ^∗ +γ^∗_0 h) which must be 2πn for some integer n. Therefore, the plane wave is consistently reflected if the distance h satisfies

h = h^∗_n := nπ − θ^∗ γ^∗_0

, (11)

where n is any integer such that h^∗_n is positive. However, this does not imply that the FP-cavity with h = h^∗_n has a BIC with frequency ω^∗ and Bloch wavenumber β^∗_0 . Evanescent waves that decay towards a periodic layer can actually generate propagating waves. Thus, the total propagating plane wave with frequency ω^∗ and wavenumber β^∗_0 is no longer totally reflected by the mirrors. In fact, the FP-cavity with h = h^∗_n usually does not even have a BIC with wavenumber β_0 = β^∗_0 and frequency ω near ω^∗. In the following, we consider the distance h and other structural parameters, and investigate whether the FP-cavity has a BIC with ω near ω^∗ and β_0 near or equal to β^∗_0 when h or other parameters are slightly varied.

III. APPROXIMATION WITH ONE EVANESCENT WAVE

Before we present numerical results for FP-BICs with distance, frequency and wavenumber near or at h^∗_n, ω^∗ and β^∗_0 associated with a total reflection, we first consider a model assuming that the wave field in the FP-cavity consists of one propagating and one evanescent waves. The model helps us to understand why the FP-BIC, if it exists, does not have the exact total-reflection values h^∗_n, ω^∗ and β^∗_0 . It also gives rise to approximate formulas for h and ω (or β_0) of the FP-BIC.

For the single periodic layer bounded by z = ±d, if β_0 ∈ (0, π/L), the negative first diffraction order has the slowest decay rate in z. If we replace the incident wave in Eq. (4) by an evanescent wave of diffraction order −1, i.e. u^{(i)} = e^{i[β−1y−γ−1(z−d)]}, z > d, (12) then the reflected and transmitted waves are

u^{(r)} = ∞∑ m=−∞ R_{m,−1} e^{i[βmy+γm(z−d)]}, z > d, (13)

u^{(t)} = ∞∑ m=−∞ T_{m,−1} e^{i[βmy−γm(z+d))]}, z < −d, (14) where T_{m,−1} and R_{m,−1} are transmission and reflection coefficients for the m-th diffraction order.

Now, we assume the FP-cavity has a BIC and its wave field between the two mirrors is u ≈ a^+_0 e^{i[β0y+γ0(z−h/2)]} + a^+_{−1} e^{i[β−1y+γ−1(z−h/2)]} +a^−_0 e^{i[β0y+γ0(z+h/2)]} + a^−_1 e^{i[β−1y+γ−1(z+h/2)]} (15)

for −h/2 < z < h/2. The total transmitted propagating wave for z > D is (a^+_0 T_{0,0} + a^+_{−1} T_{0,−1})e^{i[β0y+γ0(z−D)]}. Thus an approximate condition for the FP-BIC is

a^+_0 T_{0,0} + a^+_{−1} T_{0,−1} = 0. (16)

However, the above condition is not convenient to use, since a^+_0 and a^+_{−1} are still undetermined.

We can find an alternative condition based on the wave field in the cavity being self-consistently reflected. At z = h/2, the amplitudes of the reflected zeroth and negative first diffraction orders are related to the amplitudes of the incident waves by

D^{−1} [ a^−_0 a^−_1 ] = R [ a^+_0 a^+_{−1} ] , (17)

where D = [ e^{iγ0 h} 0 0 e^{iγ−1h} ] , R = [ R_{0,0} R_{0,−1} R_{−1,0} R_{−1,−1} ] . (18)

Similarly, at h = −h/2, we have

D^{−1} [ a^+_0 a^+_{−1} ] = R [ a^−_0 a^−_1 ] . (19)

Actually, the FP-BIC is either even or odd in z, thus (a^−_0 , a^−_1) = ±(a^+_0 , a^+_{−1}). Therefore, either DR − I or DR + I is a singular matrix, where I is the 2 × 2 identity matrix. We can write the approximate condition for FP- BICs as

det(DR ± I) = 0 (20)

or det[(DR)^2 − I] = 0. If we keep only the propagating wave in the cavity, then D and R become their (1, 1) entries, and the condition is simplified to [e^{iγ0 h}R_{0,0}]^2 = 1 This immediately leads to Eq. (11).

Since Eq. (20) is a complex equation, it can be used to calculate two real quantities, for example ω and h, assuming β_0 is fixed. Moreover, we can further simplify Eq. (20) to obtain approximate linear equations for h and ω. Let (ω^∗, β^∗_0 ) correspond to a total reflection and h^∗ = h^∗_n be given by Eq. (11) for an even integer n, then the BIC (if it exists) should be even in z, so that det(DR − I) = 0. Taking the partial derivative of this equation with respect to ω and h at (ω^∗, h^∗), we have [ h^∗ω^∗/(c^2γ^∗_0 ) − R^′_{00}(ω^∗) ] (ω − ω^∗) −γ^∗_0 (h − h^∗) ≈ ie^{iγ∗−1h∗} R^∗_{0,−1}R^∗_{−1,0}/R^∗_{00} (21) where R^∗_{j,k} = R_{j,k}(ω^∗), R^′_{00}(ω^∗) is the derivative of R_{00} with respect to ω at ω^∗, γ^∗_j = [(ω^∗/c)^2 − (β^∗_j )^2]^{1/2} for j, k ∈ {0, −1}. The real and imaginary parts of Eq. (21) form a linear system of two equations for h and ω. If the BIC is odd in z, we can derive a similar linear system from det(DR + I) = 0.

IV. NUMERICAL EXAMPLES

In this section, we present numerical examples for BICs in FP-cavities constructed from two periodic arrays of circular or triangular cylinders separated by a distance h. In Fig. 2, we show a periodic array of circular cylinders

FIG. 2. Three periodic arrays of cylinders with period L in the y direction. Cross sections of the cylinders: (a) circular disks with radius a, (b) equilateral triangles with side length Lt and a reflection symmetry in y, (c) equilateral triangles with side length Lt and a reflection symmetry in z.

with radius a and two periodic arrays of triangular cylinders that are symmetric in y and z, respectively. The cross sections of all triangular cylinders are equilateral triangles of side length L_t. The dielectric constant of all circular or triangular cylinders is ϵ_c = 6.6. The medium outside the cylinders is air. All three periodic arrays of cylinders are regarded as a periodic layer of thickness 2d = L, where L is the period of the array in the y direction.

For each periodic array, we first calculate two total reflections with a zero and a nonzero β^∗_0 , respectively, then for each total reflection, we select a distance h^∗_n, and try to find FP-BICs by varying the Bloch wavenumber β_0, the distance h or other structural parameters such as a and L_t. The numerical method is based on a nonlinear eigenvalue formulation at z = ±D for one period of y [39, 40] and a contour integral method for solving nonlinear eigenvalue problems [41, 42].

A. Circular cylinders

For the periodic array of circular cylinders with a = 0.3L and shown in Fig. 2(a), we found two total reflections with β^∗_0 = 0 and β^∗_0 = 0.5(π/L), respectively, and they are listed in Table I as TR1 and TR2. For each total reflection, we choose a distance h^∗_n, denoted as h^∗ for simplicity, from formula (11) for a small integer n, to form a Fabry-Perot cavity. The cavity with distance h^∗

Solutions a/L h/L β0L/π ωL/(2πc) TR1 0.3 0.43394 0 0.99310 RM1 0.3 0.43394 0 0.99330−0.000039i BIC1 0.3 0.41637 0 0.99557 BIC2 0.30152 0.43394 0 0.99069

TR2 0.3 0.62438 0.5 0.70413 RM2 0.3 0.62438 0.5 0.70679−0.000072i BIC3 0.3 0.58363 0.5 0.71054 BIC4 0.30816 0.62438 0.5 0.69511 BIC5 0.3 0.62438 0.51884 0.70511

TABLE I. FP-cavity with two periodic arrays of circular cylinders of radius a separated by a distance h. The different rows show total reflections, resonant modes and BICs.

has only a resonant mode with a complex frequency and Bloch wavenumber β_0 = β^∗_0 . The two resonant modes are listed in Table I as RM1 and RM2, respectively.

To find BICs in this Fabry-Perot structure, we have to change a structural parameter or vary the Bloch wavenumber β_0. For the total reflection with β^∗_0 = 0, we found two FP-BICs, BIC1 and BIC2 in Table I, by changing the distance from h^∗ = 0.43394L to h = 0.41637L and changing the radius a from 0.3L to 0.30152L, respectively. The frequencies of these two BICs are given in Table I. For the total reflection with β^∗_0 = 0.5(π/L), we similarly found two FP-BICs, listed in Table I as BIC3 and BIC4, by changing h and a, respectively. In that case, it is also possible to find a FP-BIC by keeping h = h^∗ and a = 0.3L and changing β_0. The result is the BIC5 given in Table I. The wave field patterns of BIC1 and BIC5 are shown in Fig. 3.

FIG. 3. Field patterns (real part of u) of BIC1 and BIC5 as in Table I.

The FP-BICs listed in Table I are consistent with existing theories about their robustness and parametric dependence [19, 21]. Since the FP-cavity has reflection symmetry in both y and z, a typical BIC with its frequency ω and a nonzero Bloch wavenumber β_0 satisfying (8) is robust. This means that when a structural parameter is slightly perturbed without breaking the symmetry, the BIC will continue to exist, but will have a slightly different frequency and a slightly different wavenumber [19]. For example, when h is decreased from 0.62438L to 0.58363L, BIC5 is turned to BIC3, and when a is increased from 0.3L to 0.30816L, BIC5 is turned to BIC4. The robustness theory also implies that if β_0 is fixed and one structural parameter is changed, the BIC can be preserved if another structural parameter is properly adjusted. For example, if a is slightly increased and h is changed accordingly, BIC3 is turned to BIC4 with β_0 fixed at 0.5(π/L).

The two FP-BICs with β_0 = 0, i.e., BIC1 and BIC2 in Table I, are not typical BICs. For structures with a reflection symmetry in y, the typical BICs with β_0 = 0 are symmetry-protected standing waves that are antisymmetric in y. Both BIC1 and BIC2 are symmetric standing waves (symmetric in y), unprotected by symmetry, and nonrobust [8]. In fact, they are the simplest super-BICs with the Q factor of nearby resonant modes proportional to 1/β^4_0 . Nevertheless, by adjusting a second parameter, such a BIC can still exist continuously as one structural parameter is varied. For example, when a is increased from 0.3L to 0.30152L and h is increased from 0.41637L to 0.43394L, BIC1 is turned to BIC2, and both are standing waves with β_0 = 0.

B. Triangular cylinders: symmetric in y

For the periodic array of triangular cylinders shown in Fig. 2(b), we assume the side length is L_t = 0.7L and found two total reflections with β^∗_0 = 0 and β^∗_0 = 0.2(π/L), respectively. For each case, the FP-cavity with a distance h^∗, chosen from formula (11) for a small integer n, does not have a BIC with the same Bloch wavenumber β^∗_0 . Instead, the cavity only has resonant modes with a complex frequency. In Table II, the rows with RM1 and RM2 show L_t, h^∗, β^∗_0 and the complex frequency of the corresponding resonant modes. As in the previous subsection, we can find BICs near the total reflections by changing h, changing L_t or varying β_0. The results are listed in Table II. The wave field patterns of BIC2 and BIC4 are shown in Fig. 4.

While the single periodic array of triangular cylinders considered in this subsection does not have a reflection symmetry in z, the FP-cavity, consisting of two arrays that are mirror reflection of each other, has reflection symmetry in both y and z. As such, we have the same statements about BIC4, BIC5 and BIC6 as those for BIC3, BIC4 and BIC5 of Table I, and the same statements about BIC1 and BIC2 as in the previous subsec-

Solutions Lt/L h/L β0L/π ωL/(2πc) TR1 0.7 0.00272 0 0.83010 RM1 0.7 0.00272 0 0.83007−0.000097i BIC1 0.7 0.02274 0 0.82634 BIC2 0.69045 0.00272 0 0.83774 BIC3 0.7 0.00272 ±0.10028 0.82958

TR2 0.7 0.48667 0.2 0.84515 RM2 0.7 0.48667 0.2 0.84546−0.000011i BIC4 0.7 0.50135 0.2 0.84354 BIC5 0.69630 0.48667 0.2 0.84830 BIC6 0.7 0.48667 0.20895 0.84495

TABLE II. FP-cavity with two periodic arrays of triangular cylinders with side length Lt and a reflection symmetry in y, separated by a distance h. The different rows show total reflections, resonant modes, and BICs.

FIG. 4. Field patterns (real part of u) of BIC2 and BIC4 as in Table II.

tion. In particular, the symmetric standing waves BIC1 and BIC2 are not typical BICs. For a structure with such a BIC, if a parameter is slightly changed, the perturbed structure does not usually have a symmetric standing wave, and may or may not have a pair of BICs with nonzero and opposite β_0. For example, when h is changed from 0.02274L to 0.00272L, the symmetric standing wave BIC1 is destroyed, but the perturbed system has a pair of BICs with nonzero and opposite β_0, listed in Table II as BIC3. On the other hand, for the FP-cavity with BIC1 of Table I in subsection A, if the distance is increased from h = 0.41637L to 0.43394L, the symmetric standing wave is destroyed, and there are no other BICs with small but nonzero β_0. The existence or nonexistence of BICs with nonzero β_0 can be explained by the bifurcation theory for such non-generic BICs [29].

C. Triangular cylinders: asymmetric in y

In this subsection, we consider the FP-cavity formed by two periodic arrays of triangular cylinders shown in Fig. 2(c). The periodic arrays and the FP-cavity have a reflection symmetry in z, but are asymmetric in y. For the single periodic array with L_t = 0.5L, we found two total reflections with β^∗_0 = 0 and β^∗_0 = 0.2(π/L), respectively. For each case, we choose a distance h^∗_n for a small integer n, denoted as h^∗ for simplicity, and calculate the associated resonant mode. The total reflections and the resonant modes are listed in Table III as TR1, TR2, RM1 Solutions Lt/L h/L β0L/π ωL/(2πc) TR1 0.5 0.64101 0 0.74436 RM1 0.5 0.64101 0 0.74413−i0.61×10^{−6} BIC1 0.5 0.64732 0 0.74409 BIC2 0.49248 0.64101 0 0.75165

TR2 0.5 0.11847 0.2 0.70935 RM2 0.5 0.11847 0.2 0.71161−i0.89×10^{−4}

TABLE III. FP-cavity with two periodic arrays of triangular cylinders with no reflection symmetry in y. The different rows show total reflections, resonant modes and BICs.

and RM2, respectively.

In connection with the total reflection at β^∗_0 = 0, we are able to find BICs by slightly changing h or L_t. The results are listed in Table III as BIC1 and BIC2. The wave field pattern of BIC1 is shown in Fig. 5. Notice that all BICs

FIG. 5. Field pattern (real part of u) of BIC1 in Table III.

with β_0 = 0 in periodic structures without a reflection symmetry in y are nonrobust. If a structural parameter is varied, such a BIC will normally be destroyed. But if a second parameter is adjusted accordingly following the first one, the BIC can exist continuously. For example, as L_t is reduced from 0.5L to 0.49248L and h is also changed from 0.64732L to 0.64101L, BIC1 is turned to BIC2.

For the total reflection at β^∗_0 = 0.2(π/L), the FP-cavity with the distance h^∗ = 0.11847L does not have a BIC for any β_0 near β^∗_0 . In Fig. 6, we show the real and imaginary parts of the complex frequency ω and the Q factor of the corresponding resonant modes for β_0L/π ∈ [0.2, 0.26]. It

FIG. 6. Complex frequency and Q factor of the resonant modes in an asymmetric FP-cavity with distance h^∗ = 0.11857L, for β0 ≥ 0.2π/L.

is clear that Im(ω) has a local maximum which is negative, and the Q factor is always finite. According to the theory on parametric dependence of BICs [21], a BIC in such a periodic structure without a reflection symmetry in y can form a curve in the plane of two generic structural parameters. This implies that in the h-L_t plane, there maybe a curve, and at each point on the curve the FP-cavity has a BIC for some ω and some β_0. Since the probability of a random point falling on a curve is zero, it is not surprising that no BIC can be found for L_t = 0.5L and h = h^∗.

To find out whether BICs exist near this total reflection with nonzero β^∗_0 when the structural is slightly changed, we consider five parameters: distance h, side length L_t, refractive index of the cylinders n_1 = √ ϵ_c, height H_t of the triangle (cross section of the cylinders) in the y direction, and rotation angle θ of the triangle about its center, where H_t and θ are illustrated in Fig. 7. When each of

FIG. 7. (a) An isosceles triangle with base Lt and height Ht. (b) An equilateral triangle rotated by angle θ.

these parameters is varied, we search the wavenumber β_0 around β^∗_0 for a local maximum of Im(ω), where ω is the complex frequency of the resonant modes. A BIC can be identified if Im(ω) = 0. However, in all five cases, we are unable to find a BIC with ω near ω^∗ and β_0 near β^∗_0 . In Fig. 8, we show the result for varying h from h^∗ to h^∗ + 0.25L. A particular case for h = h^∗ + 0.015L is shown in Fig. 8(b). Similar to the case for h = h^∗ shown in the middle panel of Fig. 6, Im(ω) has a local maximum, which is still negative, at some β_0 > β^∗_0 . The maximum value of Im(ω) and the β_0 that attains the local maximum are shown in Fig. 8(a) as functions of h − h^∗. We only show the results for h > h^∗, since the local maximum of Im(ω) increases as h is increased from h^∗. Since

FIG. 8. (a) The local maximum of the imaginary part of the frequency of the resonant mode and the related wavenumber β coming from adding a d on h. (b) When d = 0.03, the trajectory of the imaginary part of the frequency of the resonant mode for varying β.

the studied ranges of h and β_0 are quite large compared with h^∗ and β^∗_0 , we conclude that this FP-cavity has no BIC for h near h^∗ and β_0 near β^∗_0 . Similar results are shown in Fig. 9, where each of these four parameters,

FIG. 9. Local maximum of Im(ω) and β0 at the local maximum for resonant modes in a FP-cavity with a varying (a) refractive index n1, (b) side length Lt, (c) height Ht or δ = Ht − ( √ 3/2)Lt, and (d) rotation angle θ.

n_1, L_t, H_t and θ, is varied. For all cases, we are unable to find a BIC even when one structural parameter has varied a large amount.

It appears that for FP-cavities without a reflection symmetry in y, it is unlikely (at least not always possible) to find a BIC with ω near ω^∗ and β_0 near β^∗_0 if β^∗_0 is nonzero, by varying one structural parameter. As we mentioned earlier, if the structure has a BIC, then the BIC should form a curve in the plane of two generic structural parameters [21]. If an initial pair of parameters related to a total reflection is far away from the curve, we will not be able to reach the curve by a small variation of the parameters. Even if the initial pair is close to the curve, and we are able to move to the curve by varying one parameter, the β_0 of the BIC on the curve could be very different from β^∗_0 of the total reflection. In that case, there is still no BIC with (ω, β_0) near (ω^∗, β^∗_0 ).

V. CONCLUSION

In this work, we investigated the existence of FP-BICs near total reflections in Fabry-Perot cavities formed by two periodic arrays of circular or triangular dielectric cylinders separated by a distance h. A total reflection of a single periodic array is associated with a frequency ω^∗ and a wavenumber β^∗_0 . Our numerical results indicate that the reflection symmetry in y plays a key role and whether β^∗_0 is zero or nonzero is also important. More specifically, if the periodic array is symmetric in y, it is likely to find a BIC with frequency ω near ω^∗ and Bloch wavenumber β_0 = β^∗_0 by slightly tuning one structural parameter, such as the distance h, that does not break the symmetry in y. For the case of β^∗_0 ≠ 0, it is also likely to find a BIC with β_0 near β^∗_0 without tuning any structural parameter. If the array does not have a reflection symmetry in y and β^∗_0 = 0, it is still likely to find a BIC with β_0 = 0 by tuning one structural parameter. But if the array is not symmetric in y and β^∗_0 ≠ 0, it is unlikely to find a BIC with (ω, β_0) near (ω^∗, β^∗_0 ) by varying any structural parameter. The last case indicates that a total reflection does not always lead to a FP-BIC, even when the parameters of the FP-cavity are slightly tuned.

The FP-BICs found in Sec. IV, listed in Tables I, II and III, belong to different categories. They can be robust or nonrobust, and the nonrobust BICs include ordinary ones and super-BICs. Those BICs with a nonzero β_0 in structures with a reflection symmetry in y, i.e., BICs 3-5 in Table I and BICs 4-6 in Table II, are robust. Those BICs with β_0 = 0 in structures without a reflection symmetry in y, i.e., BIC1 and BIC2 in Table III, are nonrobust (ordinary ones), but can still be preserved by adjusting a second parameter when the first parameter is varied. Those FP-BICs with β_0 = 0 in structures that are symmetric in y, i.e., BIC1 and BIC2 in both Table I and II, are also nonrobust but they are the so-called super-BICs. A super-BIC may bifurcate to a par of normal robust BICs with nonzero and opposite β_0 when a parameter is varied. The BIC3 in Table II can be regarded as the robust BICs bifurcated from BIC1 or BIC2, also in Table II, as one parameter is varied. However, it should be emphasized that the existing theories on robustness, parametric dependence and super-BICs, do not imply the existence or nonexistence of FP-BICs near total reflections. Our work is a numerical study. Further theoretical studies are needed to clarify the connection between total reflections and FP-BICs.

ACKNOWLEDGMENTS

The authors acknowledge support from the Research Grants Council of Hong Kong Special Administrative Region, China (Grant No. CityU 11307720).

[1] D. C. Marinica, A. G. Borisov, and S. V. Shabanov, “Bound states in the continuum in photonics,” Phys. Rev. Lett. 100, 183902 (2008).

[2] E. N. Bulgakov and A. F. Sadreev, “Bound states in the continuum in photonic waveguides inspired by defects,” Phys. Rev. B 78, 075105 (2008).

[3] Y. Plotnik, O. Peleg, F. Dreisow, M. Heinrich, S. Nolte, A. Szameit, and M. Segev, “Experimental Observation of Optical Bound States in the Continuum,” Phys. Rev. Lett. 107, 183901 (2011).

[4] C. W. Hsu, B. Zhen, J. Lee, S.-L. Chua, S. G. Johnson, J. D. Joannopoulos, and M. Soljačić, “Observation of trapped light within the radiation continuum,” Nature 499, 188 (2013).

[5] A. Kodigala, T. Lepetit, Q. Gu, B. Bahari, Y. Fainman, and B. Kanté, “Lasing action from photonic bound states in continuum,” Nature 541, 196 (2017).

[6] J. Jin, X. Yin, L. Ni, M. Soljačić, B. Zhen, and C. Peng, “Topologically enabled ultrahigh-Q guided resonances robust to out-of-plane scattering,” Nature 574, 501 (2019).

[7] C. W. Hsu, B. Zhen, A. D. Stone, J. D. Joannopoulos and M. Soljačić, “Bound states in the continuum,” Nat. Rev. Mater. 1, 16048 (2016).

[8] L. Yuan and Y. Y. Lu, “Strong resonances on periodic arrays of cylinders and optical bistability with weak incident waves,” Phys. Rev. A 95, 023834 (2017).

[9] K. Koshelev, S. Lepeshov, M. Liu, A. Bogdanov, and Y.

Kibshar, “Asymmetric Metasurfaces with High-Q Resonances Governed by Bound States in the Continuum,” Phys. Rev. Lett. 121, 193903 (2018).

[10] L. Yuan and Y. Y. Lu, “Perturbation theories for symmetry-protected bound states in the continuum on two-dimensional periodic structures,” Phys. Rev. A 101, 043827 (2020).

[11] V. Mocella and S. Romano, “Giant field enhancement in photonic resonant lattices,” Phys. Rev. B 92, 155117 (2015).

[12] Z. Hu, L. Yuan, and Y. Y. Lu, “Resonant field enhancement near bound states in the continuum on periodic structures,” Physical Review A 101, 043825 (2020).

[13] S. P. Shipman and H. Tu, “Total resonant transmission and reflection by periodic structures,” SIAM J. Appl. Math. 72, 216-239 (2012).

[14] C. Blanchard, J.-P. Hugonin, and C. Sauvan, “Fano resonant modes in photonic crystal slabs near optical bound states in the continuum,” Phys. Rev. B 94, 155303 (2016).

[15] L. Yuan, M. Zhang, and Y. Y. Lu, “Real transmission and reflection zeros of periodic structures with a bound state in the continuum,” Phys. Rev. A 106, 013505 (2022).

[16] A. F. Sadreev, “Interference traps waves in an open system: bound states in the continuum,” Rep. Prog. Phys. 84, 055901 (2021).

[17] K. L. Koshelev, Z. F. Sadrieva, A. A. Shcherbakov, Y. S.

Kivshar, and A. A. Bogdanov, “Bound states in the continuum in photonic structures,” Phys.-Uspekhi 93, 528 (2023).

[18] B. Zhen, C. W. Hsu, L. Lu, A. D. Stone, and M. Soljačić, “Topological Nature of Optical Bound States in the Continuum,” Phys. Rev. Lett. 113, 257401 (2014).

[19] L. Yuan and Y. Y. Lu, “Bound states in the continuum on periodic structures: perturbation theory and robustness,” Optics Letters 42, 4490-4493 (2017).

[20] L. Yuan and Y. Y. Lu, “Conditional robustness of propagating bound states in the continuum in structures with two-dimensional periodicity,” Physical Review A 103, 043507 (2021).

[21] A. Abdrabou, L. Yuan, W. Lu, and Y. Y. Lu, “Parametric dependence of bound states in the continuum: A general theory,” Physical Review A 107, 033511 (2023).

[22] E. N. Bulgakov and D. N. Maksimov, “Bound states in the continuum and polarization singularities in periodic arrays of dielectric rods,” Phys. Rev. A 96, 063833 (2017).

[23] H. M. Doeleman, F. Monticone, W. den Hollander, A.

Alù and A. F. Koenderink, “Experimental observation of a polarization vortex at an optical bound state in the continuum,” Nat. Photon. 12, 397 (2018).

[24] Y. Zhang, A. Chen, W. Liu, C. W. Hsu, B. Wang, F.

Guan, X. Liu, L. Shi, L. Lu, and J. Zi, “Observation of Polarization Vortices in Momentum Space,” Phys. Rev. Lett. 120, 186103 (2018).

[25] M. Kang, S. Zhang, M. Xiao, and H. Xu, “Merging Bound States in the Continuum at Off-High Symmetry Points,” Phys. Rev. Lett. 126, 117402 (2021).

[26] M.-S. Hwang, H.-C. Lee, K.-H. Kim, K.-Y. Jeong, S.- H. Kwon, K. Koshelev, Y. Kivshar, and H.-G. Park, “Ultralow-threshold laser using super-bound states in the continuum,” Nat. Commun. 12, 4135 (2021).

[27] M. Kang, L. Mao, S. Zhang, M. Xiao, H. Xu, and C.

T. Chan, “Merging bound states in the continuum by har- nessing higher-order topological charges,” Light Sci. Appl. 11, 228 (2022).

[28] E. Bulgakov, G. Shadrina, A. Sadreev, and K. Pichugin, “Super-bound states in the continuum through merging in grating,” Phys. Rev. B 108, 125303 (2023).

[29] N. Zhang and Y. Y. Lu, “Bifurcation of bound states in the continuum in periodic structures,” Opt. Lett. 49, 1461 (2024).

[30] R. F. Ndangali and S. V. Shabanov, “Electromagnetic bound states in the radiation continuum for periodic double arrays of subwavelength dielectric cylinders,” J. Math. Phys. 51, 102901 (2010).

[31] L. S. Li and H. Yin, “Bound states in the continuum in double layer structures,” Sci. Rep. 6, 26988 (2016).

[32] M. McIver, “An example of non-uniqueness in the twodimensional water-wave problem,” J. Fluid Mech. 315, 257–266 (1996).

[33] C. M. Linton and N. Kuznetsov, “Non-uniqueness in twodimensional water wave problems: numerical evidence and geometrical restrictions,” Proc. R. Soc. Lond. A 453, 2437–2460 (1997).

[34] R. Porter, “Trapping of water waves by pairs of submerged cylinders,” Proc. R. Soc. Lond. A 458, 607–624 (2002).

[35] L. Chesnel and V. Pagneux, “From zero transmission to trapped modes in waveguides,” J. Phys. A: Math. Theor. 52, 165304 (2019).

[36] E. Popov, L. Mashev and D. Maystre, “Theoretical study of the anomalies of coated dielectric gratings,” Optica Acta 33(5), 607–619 (1986).

[37] S. Fan, W. Suh and J. D. Joannopoulos, “Temporal coupled-mode theory for the Fano resonance in optical resonators,” J. Opt. Soc. Am. A 20(3), 569–572 (2003).

[38] H. Wu, L. Yuan and Y. Y. Lu, “Approximating transmission and reflection spectra near isolated nondegenerate resonances,” Phys. Rev. A 105, 063510 (2022).

[39] Z. Hu and Y. Y. Lu, “Standing waves on two-dimensional periodic dielectric waveguides,” J. Opt. 17, 065601 (2015).

[40] L. Yuan and Y. Y. Lu, “Propagating Bloch modes above the lightline on a periodic array of cylinders,” J. Phys. B: At. Mol. Opt. Phys. 50, 05LT01 (2017).

[41] J. Asakura, T. Sakurai, H. Tadano, T. Ikegami, and K.

Kimura, “A numerical method for nonlinear eigenvalue problems using contour integrals,” JSIAM Letters 1, 52– 55 (2009).

[42] W.-J. Beyn, “An integral method for solving nonlinear eigenvalue problems,” Linear Algebra and its Applications 436, 3839—3863 (2012).