arXiv:chao-dyn/9905025v1 16 May 1999

Experimental Generation and Observation of Intrinsic Localized Spin Wave Modes in an Antiferromagnet

U. T. Schwarz, L. Q. English, and A. J. Sievers Laboratory of Atomic and Solid State Physics, Cornell University, Ithaca, NY 14853-2501 (May 1999)

By driving with a microwave pulse the lowest frequency antiferromagnetic resonance of the quasi 1- D biaxial antiferromagnet (C2H5NH3)2CuCl4 into an unstable region intrinsic localized spin waves have been generated and detected in the spin wave gap. These findings are consistent with the prediction that nonlinearity plus lattice discreteness can lead to localized excitations with dimensions comparable to the lattice constant.

PACS numbers: 05.45.-a, 76.50.+g,75.50.Ee

Although solitons continue to play an important role in condensed matter physics [1–3] in the last decade it was recognized that nonlinearity plus lattice discreteness can lead to a different class of excitations with dimensions comparable to the lattice constant [4–6]. Such intrinsic localized modes (ILMs) have been identified in a variety of classical molecular dynamics simulations [7–9] and with macroscopic mechanical [10] and electrical [11] models, all of which ignore the possible role of quantum mechanics [12]. Some effort has gone into identifying specific condensed matter signatures as evidence of ILM production but all require intricate arguments: these include far infrared absorption [13], radiation ionization tracks [14], the temperature dependent Mössbauer effect [4] and resonant Raman scattering [15]. As yet evidence of externally generated ILMs in a lattice of atomic dimensions is missing. The large amplitude modulational instability of an antiferromagnetic resonance (AFMR) for some antiferromagnets has been suggested [16,17] as a mechanism for the generation of intrinsic localized spin wave modes (ILSMs) and in this letter we describe the experimental observation and control of such nanoscale excitations.

Because the driving field necessary to create ILMs via the modulational instability scales with the frequency of the antiferromagnetic resonance, ω_{AFMR}, (C_2H_5NH_3)_2CuCl_4 with the lowest frequency resonance at ω_{AFMR} = 1.5 GHz was chosen for this first study. This antiferromagnet, often referred to as C(2)CuCl_4, is a layered organic material with a strong ferromagnetic coupling of the magnetic Cu^{2+} ions within a layer and with a weak antiferromagnetic coupling between these layers. Because of this weak interlayer coupling the total spin in each layer can be represented by a classical one with respect to describing the lowest frequency mode dynamics. This spin system with its biaxial anisotropy is described in more detail in Ref. [17].

The C(2)CuCl_4 single crystals were grown from aqueous solution of ethylamine hydrochloride and copper (II) chloride in a closed vessel by slowly decreasing the temperature [18]. For the measurement, platelets with well defined surfaces and a typical dimension of 3×3×0.5 mm^3 were chosen.

FIG. 1. (a) Schematic experimental setup. Details are given in the text. (b) Experimental measurement road map. The horizontal line for t < 0 identifies the AFMR frequency. During the high power driving pulse (shaded area) the detection electronic is blocked. The solid lines A ... F show the AFMR for increasing pump-pulse power levels. The vertical dotted lines identify different time-cuts described in the text.

The experimental setup is shown schematically in Fig. 1(a). The first oscillator provides the high power pulse and the second oscillator the probe beam. Because the expected experimental signature of ILSM generation after a strong microwave pulse near the ω_{AFMR} is the breakup of the AFMR into a broad band, the generation/detection system is tailored to produce a large AC field at the driving frequency ω_{excite} and a high sensitivity over a broad band below but close to ω_{excite}. A single 3 mm diameter loop of copper wire is used as a non-resonant antenna for the excitation and pickup of the broad band signal in reflection. A pump signal of up to 100 W can be obtained from the oscillator and solid state amplifier. To create short pulses a fast GaAs switch is used in front of the amplifier. The signal of a second, tunable oscillator is overlayed by means of a directional coupler. With a second fast switch, synchronized by a digital delay generator, the reflected signal from the pump pulse is suppressed. The weak reflected signal from the second oscillator passes through two low noise amplifiers and is detected with a spectrum analyzer which was used as a variable bandwidth detector locked to the frequency of the probe oscillator. The minimum noise level of the system is −120 dBm at 100 kHz bandwidth. In this measurement setup the absorption can be obtained as a function of time and frequency by first measuring the time dependent absorption at the frequency of the second oscillator, and then scanning this oscillator frequency during subsequent pump pulses. The time resolution is limited to 20 μs by the spectrum analyzer, and the sensitivity, by the flatness of the exciting loop impedance. Care was taken not to saturate any electronic circuits, as this could produce an artificial nonlinear response. The exciting coil and sample are immersed in pumped liquid helium at 1.2 K.

To provide a road map to the experimental data-taking procedure a schematic view of the power and time dependence of the AFMR is shown in Fig. 1 (b). The AFMR frequency before the pulse, t < 0, is represented by the horizontal line. During the high power driving pulse (shaded area) the detection electronics is blocked. After the trailing edge (t = 0) of the driving pulse the spin wave is highly excited and its frequency is decreased due to the intrinsic nonlinearity of the spin Hamiltonian. From this state the system relaxes back to equilibrium with the longitudinal relaxation time T_1. The absorption by the spin system can be examined for different power levels of the driving pulse [lines labeled A ... F in Fig. 1(b)] or for different time delays at a fixed power [dotted lines in Fig. 1(b)] or as a function of the driving pulse length. Measurements varying all of these experimental parameters have been carried out and are described below.

Figure 2 shows the absorption spectra 20 μs (≫ T_2 of the AFMR) after the trailing end of a pump pulse for six different powers. The power of the 400 μs long driving pulse varied from 50 mW to 1.6 W. On the low frequency side of each spectrum are two magnetostatic volume modes while the shoulder on the high frequency side is a surface mode [19]. With increasing power levels the AFMR first collapses into a broad asymmetric shape and then at still higher powers returns to a sharp AFMR. Note that the magnetostatic modes do not show the same behavior as the AFMR. These experimental results demonstrate that the AFMR is indeed unstable with increasing amplitude but only up to a specific amplitude while for still larger amplitudes the AFMR uniform mode

FIG. 2. Absorption spectra measured 20 μs after a 400 μs driving pulse for the different power levels. (A) 50 mW, (B) 100 mW, (C) 160 mW, (D) 320 mW, (E) 500 mW, and (F) 1.6 W of the 1.46 GHz (arrow) driving pulse. For clarity the spectra are shifted on the linear ordinate. The asymmetric wing on the low frequency side of the AFMR is the expected signature of localized mode production. The dot-dashed line marks the lowest frequency ωAFMR for an applied static field HDC = 12 mT.

again becomes stable.

The results in Fig. 2 illustrate some of the criteria for the creation of ILSMs. First there is a minimum transverse amplitude above which the extended mode becomes unstable but then, surprisingly, there is also a maximum amplitude associated with this instability of the extended mode. This was not expected from our molecular dynamics simulations. Next the frequency interval of the instability region is observed to become larger as the frequency shift ω_{excite} − ω_{AFMR} becomes larger. For optimum conditions, localization could be observed for powers as low as 50 mW in a 400 μs driving pulse. Varying the pulse width from 50 μs to 400 μs while keeping the energy in the pulse fixed does not change these criteria.

The narrow linewidth of curve F shown in Fig. 2 after the strongest driving pulse is a handy test to exclude any temperature related effect, such as the heating of the crystal by the intense microwave pulses. From low power linear measurements both the temperature dependence of the AFMR frequency, which goes to zero at the Néel temperature T_N = 10.2 K, and its linewidth are known. If the frequency shift of 75 MHz between the low power trace (dashed line in Fig. 2) and high power trace were caused by an increased temperature in the crystal, the line width should nearly double. This is not observed so temperature effects are not the source of the unusual lineshape results.

The frequency response at several delay times for 200 mW excitation in a 200 μs pulse is shown in Fig.

FIG. 3. Absorption spectra measured 20 μs, 220 μs, 420 μs, 620 μs and 6 ms after a 200 μs long driving pulse at 1.46 GHz (arrow). The spectra are shifted on the ordinate by equal amounts. The dot-dashed line marks ωAFMR as in Fig. 2.

3. The five traces at 20 μs, 220 μs, 420 μs, 620 μs and 6 ms show the evolution of this absorption feature from a broad resonance back to an AFMR at times smaller than T_1 = 1.50 ms. For times larger than 2T_1 only the AFMR survives. The radical difference between the line shapes at t = 20 μs and t = 420 μs is consistent with the idea that the breakup into ILSMs is only possible when the effects of nonlinearity and dispersion are much stronger than the dissipation effect [16].

MD simulations can be used to demonstrate that the extended spin wave is unstable against breakup into localized modes for the specific amplitude of the extended wave produced in our experiments. Details on molecular dynamics procedures for simulating localized spin waves in C(2)CuCl_4 can be found in Ref. [17]. The solid line in Fig. 4(a) shows the calculated frequency dependence of the AFMR as a function of its transverse amplitude S_y in the hard axis direction. To compare this simulation to our experiment, we extract from the shift of 75 MHz or 0.05 ω_{AFMR} of trace (F) in Fig. 2 the spin wave amplitude S_y = 0.06 as marked with (F) in Fig. 4(a). Correspondingly the points A to F superimposed on this curve identify different AFMR frequency shifts observed in the high power measurements of Fig. 2. To test for the instability threshold the time dependent evolution of the energy density for a simulation of a 250 spin antiferromagnetic chain is calculated, starting from an extended wave with fixed transverse amplitude plus random noise ⟨δS_n⟩ = 0.0025. For the whole range (A) to (F) covered by the experiment the extended spin wave is unstable and breaks up into localized modes with widths extending over about 10 lattice constants. Thus for these microwave powers the AFMR is driven into the interest-

FIG. 4. (a) Calculated frequency of the uniform spin wave mode as function of its transverse amplitude. (A) to (F) mark the experimentally determined position of the extended mode after the driving pulse from the corresponding traces in Fig. 2. (b) AFMR plus ILSM absorption spectra determined from molecular dynamics simulations corresponding to three different microwave power levels. Starting from extended spin waves with a given transverse amplitude of Sy = 0.01, 0.03 and 0.06 (arrow positions α, β, γ in Fig. 4a) the uniform mode breaks up into ILSMs within a time of 200 τAFMR. From the evolution over the subsequent time interval Δτ = 800 τAFMR the spectra are obtained via the auto-correlation of the net transverse magnetic moment as described in the text.

ing nonlinear region.

To compare the absorption spectrum A(ω) ∝ ωχ^{′′} measured in the experiment with results from molecular dynamic simulations, the imaginary part of the dynamic magnetic susceptibility is calculated using the Kubo expression [20] where the absorption is proportional to the Fourier transform of the auto-correlation function of the net magnetic moment, M_y(t): χ^{′′}_y (ω) ∝ ω ∫_∞ 0 dt⟨M_y(t_0 + t)M_y(t)⟩ exp(iωt). (1) For our special case the simulations are started with an extended wave of a given amplitude plus some small amount of random noise. The extended wave is unstable against breakup into localized excitations and transforms after approximately 100 periods of the antiferromagnetic resonance into a broad spectrum of ILMs. From 200 to 1000τ_{AFMR} the evolution of the net magnetic moment is recorded and then via Eq. 1 the imaginary part of the dynamic magnetic susceptibility is found.

The resulting calculated absorption spectra for a chain of 1000 spins at three different powers are shown in Fig. 4(b). To generate these spectra the starting transverse amplitudes of the AFMR are Sy = 0.01, 0.03, and 0.06, respectively. Each curve is averaged over 6 simulation runs to remove arbitrary spikes associated with single long-living ILSMs. The broad wing of the asymmetric band is due to the statistical distribution of the ILMs with different degrees of localization and thus different frequencies. To compare the simulations on the long chain with the spectra obtained in the experiment, the frequency axis in Fig. 4(b) was scaled to the same width relative to ω_{AFMR} as given in Figs. 2 and 3. Both the shape and width of the experimental onset results are in good agreement with theoretical simulations. Moreover the absorption spectra shown in Fig. 4(b) are obtained starting from amplitudes of the extended wave which are in the right range for traces A to F.

The disappearance of the instability at large amplitudes is an experimental feature not represented by curve γ in these model calculations. Since the values of the relaxation times taken from the experiment are T_1 = 1.50 ms and T_2 ≈ 0.1 μs, with the latter depending on the surface quality of the samples, T_2 is much smaller than the pulse widths used in our experiments so that energy is transferred to other degenerate spin waves during the microwave pulse. Our experimental results indicate that at the powers where the uniform mode instability occurs this transfer does not influence the positive curvature of the dispersion curve which is required for the instabilty. At the highest powers shown in Fig. 2 the uniform mode again becomes stable indicating that the finite wavevector spin waves have become so heavily populated during the microwave pulse that the dispersion curve now has negative curvature at the uniform mode, a condition for stability of the mode at large amplitude [16]. Because it takes a finite time for the uniform mode to break up into ILSMs both features can appear at intermediate powers such as displayed in trace D in Fig. 2. Here ILSMs are formed during the early part of the pulse while the population in the degenerate modes is still small, and they remain isolated in frequency space above the dispersion curve after the degenerate mode population becomes large so both features are seen.

In this series of microwave experiments the instability that appears, when the lowest lying AFMR of C(2)CuCl_4 is driven to larger amplitudes, has been used to generate nonlinear excitations which are localized on a nanolength scale. To distinguish between the ILSMs of classical simulations and the excitations observed in experiment the latter will be identified as ‘anons’. The hallmark experimental feature of the uniform mode breakup into anons is a broad and asymmetric spectral band below the AFMR. Classical MD simulations on a long 1-D antiferromagnetic spin chain show that both the amplitude of the extended spin wave at which it becomes unstable to breakup into localized modes and the resulting spectral shape of the ILSMs are in good agreement with the microwave results. At still higher experimental powers the AFMR is observed to become stable again, a feature related to the fact that the pump pulse is longer than T_2.

Simulations have played an important role in identifying the most economical experimental pathway for the detection of anons in real solids. This interplay may be expected to continue since additional MD studies on a C(2)CuCl_4 spin chain in the presence of a magnetic field gradient indicate directed anon transport should be possible.

The authors thank H. Padamsee who provided the microwave amplifier for these experiments and also R. Lai and R. H. Silsbee for helpful discussions. This work is supported by NSF-DMR-9631298. One of the authors (U. T. S.) is supported in part as a Feodor-Lynen scholar by the Alexander von Humboldt-Foundation.

[1] P. M. Chaikin and T. C. Lubensky, Principles of Condensed Matter Physics (Cambridge University Press, Cambridge, 1995), Ch. 10.

[2] A. M. Kosevich, B. A. Ivanov, and A. S. Kovalev, Phys.

Reports 194, 117 (1990).

[3] H.-J. Mikeska and M. Steiner, Advances in Physics 40, 191 (1991).

[4] A. J. Sievers and J. B. Page, in Dynamical Properties of Solids, edited by G.K. Horton and A.A. Maradudin (North Holland, Amsterdam, 1995), Vol. 7, p. 137.

[5] S. Aubry, Physica D 103, 201 (1997).

[6] S. Flach and C. R. Willis, Phys. Rep. 295, 181 (1998). [7] V. M. Burlakov, S. A. Kiselev, and V. N. Pyrkov, Phys.

Rev. B 42, 4921 (1990).

[8] T. Dauxois and M. Peyrard, Phys. Rev. Lett. 70, 3935 (1993).

[9] S. Rakhmanova and D. L. Mills, Phys. Rev. B 58, 11458 (1998).

[10] F. M. Russell, Y. Zolotaryuk, and J. C. Eilbeck, Phys.

Rev. B 55, 6304 (1997).

[11] P. Marquié, J. M. Bilbault, and M. Remoissenet, Phys.

Rev. E 51, 6304 (1995).

[12] W. Z. Wang, J. T. Gammel, A. R. Bishop, and M. I.

Salkola, Phys. Rev. Lett. 76, 3598 (1996).

[13] A. J. Sievers and S. Takeno, Phy. Rev. Lett. 61, 970 (1988).

[14] F. M. Russell and D. R. Collins, Nucl. Instrum. Meth. B 105, 30 (1995).

[15] B. I. Swanson et al., Phys. Rev. Lett. (in press, 1999). [16] R. Lai and A. J. Sievers, Phys. Rev. B 57, 3433 (1998). [17] R. Lai and A. J. Sievers, Phys. Rev. Lett. 81, 1937 (1998). [18] L. J. De Jongh, W. D. van Amstel, and A. R. Miedema, Physica 58, 277 (1972).

[19] H. Reimann, H. Hagen, F. Waldner, W. Berlinger, and A. Arend, Sol. St. Commun. 17, 1319 (1975).

[20] R. Kubo and K. Tomita, J. Phys. Soc. Jpn. 9, 888 (1954).