arXiv:0712.0302v1 [cond-mat.stat-mech] 3 Dec 2007

Hilbert fluid dynamics equations expressed in Chapman-Enskog pressure tensor and heat current

Soderholm, Lars H.

Mekanik, KTH, SE-10044 Stockholm, Sweden

lars.soderholm@mech.kth.se

1 Abstract

The connection between the Chapman-Enskog and Hilbert expansions is investigated in detail. In particular the fluid dynamics equations of any order in the Hilbert expansion are given in terms of the pressure tensor and heat current of the Chapman- Enskog expansion

Key words: Hilbert expansion; Chapman-Enskog expansion.

2 Introduction

The most convenient way to calculate heat current and pressure tensor is that of the Chapman-Enskog method, see Grad [4]. In particular, the terms up to second and higher order have been calculated and at least to second order there is an agreed convention of notation for the terms. But in many occasions the Hilbert method is preferred because of the difficulties with the Burnett equations, see Sone [6]. Already in the Handbuch article [4], Grad made clear that the Chapman-Enskog method and Hilbert method are two ways of expressing the same thing. But Grad adds ”to confirm this directly is an intricate task due to the different formalisms”. So, his proof is somewhat abstract. It is the object of the present work to do the explicit confirmation that Grad does not do.

The benefit of this is that the fluid dynamics equations of the Hilbert expansion are given explicitly in terms of the pressure tensor and heat current of the Chapman- Enskog method. This means that results that have been derived by the Chapman- Enskog method directly can be used in the Hilbert expansion. In the interesting paper [3] by Chekmarev and Chekmareva multiple scale methods are applied in the

Hilbert expansion. The results of the present paper should considerably simplify and generalize their results to second order. In the paper [5] the results by Chekmarev and Chekmareva were generalized but derived from the Burnett equations. This could be considered unsatisfactory as the Burnett equations are mathematically unstable. But here we have been able to show that this result was nevertheless correct. We have shown that the fluid dynamics equations of the Hilbert expansion in fact can be obtained from the corresponding equations of the Chapman-Enskog expansion by expanding the fluid dynamics fields.

3 Chapman-Enskog expansion and expansion of fluid dynamics variables

We write the Boltzmann equation in dimensionless variables (ε is the Knudsen number) εDf = Q(f, f), where the streaming operator is (F is the force per mass) D = ∂ ∂t + c· ∂ ∂x + F· ∂ ∂c . See Cercignani [1]The fluid dynamic fields are given by m ∫ fd^3c = ρ, m ∫ fcd^3c = ρv = j, (3.1) m 2 ∫ fc^2d^3c = ρ( v^2 2 + 3k_B T 2m ) = e

In the Chapman-Enskog expansion is based on the important auxiliary condition, that only the zero order distribution function contributes to the flud dynamics fields. Hence (3.1) is satisfied also with f replaced by f_{CE0}.We summarize the fluid dynamical fields w = ρ v T . The components of w are written w_a where a = 1...5. The Chapman-Enskog series is written (ε is the Knudsen number) f_{CE} = f_{CE0}(w, c) + εf_{CE1}(w, c) + ... Here, f_{CEr}(w, c) stands for a function of w and its r first derivatives and of c, the molecular velocity. In the sequel we don’t write out c explicitly.

Let us now assume that the fluid dynamics variables can be expanded in the Knudsen number w = w_0 + εw_1 + ...

Applying this expansion in f_{CEr}(w, c) we find f_{CEr}(w) = f_{CEr,0}(w_0) + εf_{CEr,1}(w_0, w_1) + ... Here f_{CEr,s} is a function of w_0, w_1, ...w_s and their r first derivatives.

We first of all consider the zero order term f_{CE0}. When we expand it we obtain to lowest order f_{CE0,0}(w_0). This is a Maxwellian for the fluid dynamics fields w_0. In other words, this is the zero order term in the Hilbert expansion f_{CE0,0} = f_{H0}. Let me write the sum of the first r terms in the Chapman-Enskog expansion and introduce this expansion of the fluid dynamics fields f_{CE0} + εf_{CE1} + ...ε^nf_{CEr} = f_{CE0,0} + ε(f_{CE0,1} + f_{CE1,0}) + ...ε^r r∑ s=0 f_{CEr−s,s} + O(ε^{r+1}) Thus we obtain ρ = m ∫ f_{CE0}d^3c = m ∫ (f_{CE0} + εf_{CE1} + ...ε^rf_{CEr})d^3c = m ∫ f_{CE0,0}d^3c + εm ∫ (f_{CE0,1} + f_{CE1,0})d^3c + ... +ε^rm ∫ r∑ s=0 f_{CEr−s,s}d^3c + O(ε^{s+1}) Identifying the terms we find ρ_r = m ∫ r∑ s=0 f_{CEr−s,s}d^3c. (3.2) In the same way we obtain j_r = (ρv)_r = r∑ s=0 ρ_{r−s}v_s = m ∫ r∑ s=0 f_{CEr−s,s}cd^3c. (3.3) Finally we have e_r = [ρ( v^2 2 + 3k_B T 2m )]_r = r∑ s=0 ρ_{r−s}( s∑ p=0 1 2 v_{s−p}·v_p + 3k_B 2m T_s)

= m 2 ∫ r∑ s=0 f_{CEr−s,s}c^2d^3c (3.4)

From (3.2-3.4) we conclude that if we assume that the fluid dynamics field are expanded in a series in the Knudsen number, the corresponding terms to order r of the fields are given as the projections of r∑ s=0 f_{CEr−s,s}. (3.5)

We shall see that^r ∑ s=0 f_{CEr−s,s} is in fact the coefficient f_{Hr} of ε^r in the Hilbert

expansion.

4 The Hilbert distribution function expressed in the Chapman-Enskog distribution function

Let us now consider the terms up to order r in the Chapman-Enskog expression of the collision term. We then expand the fluid dynamics fields and obtain r∑ p+q=0 ε^{p+q}Q(f_{CEp}, f_{CEq})

= r∑ p+q+i+j=0 ε^{p+q+i+j}Q(f_{CEp,i}, f_{CEq,j}) + O(ε^{r+1}) In the coefficient of ε^r we put p + i = k, q + j = l so that it becomes ∑ k+l=r Q(f_{CEk−p,p}, f_{CEl−q,q})

= ∑ k+l=r Q( k∑ p=0 f_{CEk−p,p}, l∑ q=0 f_{CEl−q,q}) We obtains sums of the kind (3.5).

If we do the corresponding thing in the streaming term we find that the coefficient of ε^{r−1}is D r−1∑ p=0 f_{CEr−1−p,p} So from the Chapman-Enskog equations of order 0, 1, ...r we find that Q( r∑ p=0 f_{CEr−p,p}, f_{CE0,0}) + Q(f_{CE0,0}, r∑ p=0 f_{CEr−p,p})

= − ∑ k+l=r Q( r−1∑ p=1 f_{CEk−p,p}, r−1∑ q=1 f_{CEl−q,q}) (4.6)

+D r−1∑ p=0 f_{CEr−1−p,p}

Now we proceed by induction. We assume that the sum (3.5) to order r − 1 is the corresponding term in the Hilbert expansion f_{Hr−1} = r−1∑ s=0 f_{CEr−1−s,s}. (4.7) We can then write (4.6) as Q( r∑ p=0 f_{CEr−p,p}, f_{H0}) + Q(f_{H0}, r∑ p=0 f_{CEr−p,p})

= − r−1∑ s=1 Q(f_{Hr−s}, f_{Hs}) + Df_{Hr−1} This means that_r ∑ s=0 f_{CEr−s,s} (4.8) satisfies the equation

Q(f_{Hr}, f_{H0}) + Q(f_{H0}, f_{Hr}) (4.9) = − r−1∑ s=1 Q(f_{Hr−s}, f_{Hs}) + Df_{Hr−1} for f_{Hr} in the Hilbert expansion. We assume the existence of a solution and its uniqueness up to a linear combination of 1, c,c^2. But according to (3.2-3.4) the function (4.8) also has the correct projections for f_{Hr} on the functions 1, c,c^2. So by induction this is the function f_{Hr} of the Hilbert expansion. We conclude that the simple relation between the Chapman-Enskog and Hilbert distribution functions is f_{Hr} = r∑ s=0 f_{CEr−s,s}. (4.10) 5 Conservation laws and the Chapman-Enskog equations

Let us to start by writing down the conservation laws. They are

ρ_{,t} + ∇ · j = 0 j_{,t} + ∇ · J = ρF (5.11) e_{,t} + ∇ · j_e = F · j

Here J =m ∫ fccd^3c = P+ρvv = P + jv, (5.12) where P =m ∫ fc^′c^′d^3c (5.13) and j_e = ∫ mc^2 2 fcd^3c (5.14)

= ev + q + P · v, q = m 2 ∫ c^{′2}fc^′d^3c. (5.15)

If we instead calculate the moments from f_{CEr} we obtain to zero order

J_{CE0}=m ∫ f_{CE0}ccd^3c = P_{CE0}+jv, (5.16)

P_{CE0}=m ∫ f_{CE0}c^′c^′d^3c = p1 (5.17)

j_{eCE0} = ∫ mc^2 2 f_{CE0}cd^3c (5.18)

= ev + q_{CE0}+P_{CE0}·v,

q_{CE0}= m 2 ∫ c^{′2}fc^′d^3c = 0. (5.19)

For r ≥ 1 we have J_{CEr}=m ∫ f_{CEr}ccd^3c = P_{CEr}, (5.20) P_{CEr}=m ∫ f_{CEr}c^′c^′d^3c (5.21)

j_{eCEr} = ∫ mc^2 2 f_{CEr}cd^3c (5.22) = q_{CEr}+P_{CEr}·v, q_{CEr}= m 2 ∫ c^{′2}f_{CEr}c^′d^3c. (5.23)

P_{CEr} and q_{CEr} and hence J_{CEr} and j_{eCEr} are functions of the fluid dynamics fields w and its r first derivatives. This means that we can expand the fluid dynamics fields in them to obtain P_{CEr} = P_{CEr,0} + εP_{CEr,1} + ..., where P_{CEr,s} is a function of w_0, w_1, ...w_s and its r first derivatives.

The Chapman-Enskog equations to order r are obtained if we make the approximations P → r∑ s=0 ε^sP_{CEs}, (5.24)

q → r∑ s=0 ε^sq_{CEs} in the expressions for J and j_e and substitute into the equations of balance. The equations are then

ρ_{,t} + ∇ · j = 0

j_{,t} + ∇ · ( r∑ s=0 ε^sJ_{CEs}) = ρF (5.25)

e_{,t} + ∇ · ( r∑ s=0 ε^sj_{eCEs}) = F · j

6 Integrability conditions for the Hilbert expansion

We consider the equation (4.9) of the Hilbert expansion where we now replace r by r + 1. The condition of integrability is that is ∫ m mc mc^2/2 Df_{Hr}d^3c = 0. (6.26)

We now use the relation (4.10) to express this condition in terms of the Chapman- Enskog distribution function. To that end we need the corresponding integrals för the Chapman-Enskog terms. To zero order we obtain m ∫ Df_{CE0}d^3c = ρ_{,t} + ∇ · j, m ∫ Df_{CEr}cd^3c = j_{,t} + ∇ · J_{CE0}−ρF, (6.27) m ∫ c^2 2 Df_{CE0}cd^3c = e_{,t} + ∇ · j_{eCE0} − F · j.

To order r ≥ 1 there will be no contributions to the time derivatives m ∫ Df_{CEr}d^3c = 0, m ∫ Df_{CEr}cd^3c = ∇ · J_{CEr}, (6.28) m ∫ c^2 2 Df_{CEr}cd^3c = ∇ · j_{eCEr}.

If we now expand the fluid dynamics fields we obtain m ∫ Df_{CE0,s}d^3c = ρ_{s,t} + ∇ · j_s, m ∫ Df_{CE0,s}cd^3c = j_{s,t} + ∇ · J_{CE0,s}−ρ_sF, (6.29) m ∫ c^2 2 Df_{CE0,s}cd^3c = e_{s,t} + ∇ · j_{eCE0,s} − F · j_s. For r ≥ 1 we have m ∫ Df_{CEr,s}d^3c = 0, m ∫ Df_{CEr,s}cd^3c = ∇ · J_{CEr,s}, (6.30) m ∫ c^2 2 Df_{CEr}cd^3c = ∇ · j_{eCEr,s}. Now, using the expression for f_{Hr} in terms of f_{CEr−s,s} we finally obtain the conditions of integrability to order r

ρ_{r,t} + ∇ · j_r = 0, j_{r,t} + ∇· r∑ s=0 J_{CEr−s,s}−ρ_rF= 0, (6.31)

e_{r,t} + ∇· r∑ s=0 j_{eCE0r−s,s} − F · j_r = 0. They are the fluid dynamics equations of the Hilbert expansion. Note that the same equations are obtained if we start with the Chapman-Enskog equations of order r, expand the fluid dynamics fields and pick out the coefficient of ε^r.

Let us now as an example consider the linearized Boltzmann equation and find the Hilbert fluid dynamics equations to second order. We have, see Chapman & Cowling P_{CE1} = −2μ < ∇v >, P_{CE2} = μ^2 ρT (ϖ_3 − ϖ_2)⟨∇∇T ⟩ − ϖ_2 μ^2 ρ^2 ⟨∇∇ρ⟩, (6.32) q_{CE1} = −κ ∇ T, q_{CE2} = μ^2 ρ [( θ_4 2 )△v + ( θ_4 6 − 2θ_2 3 )∇(∇ · v)].

Hence, the Hilbert fluid dynamics equations to second order are

ρ_{2,t} + ρ_0∇ · v_2 = 0,

ρ_0v_{2,t} = −∇p_2 + 2μ_0(△v_1 + 2 3 ∇(∇ · v_1)) (6.33) −[ 2μ^2 3ρT (ϖ_3 − ϖ_2)]_0△∇T_0 + [ϖ_2

2μ^2 3ρ^2

]_0△∇ρ_0, (6.34)

3k_B ρ_0 2m (T_{2,t} + T_0∇ · v_2) = κ_0△T_1 − [

2μ^2 3ρ (θ_4 − θ_2)]_0△(∇ · v_0).

Acknowledgements

Discussions with A.V. Bobylev and Y. Sone have been stimulating.

References

[1] Cercignani, C. (2000). Rarefied Gas Dynamics. From Basic Concepts to Actual Calculations. Cambridge: Cambridge University Press.

[2] Chapman, S., T.G. Cowling (1970). The Mathematical Theory of Non-Uniform Gases. Cambridge: Cambridge University Press.

[3] Chekmarev, I.B., Chekmareva, O.M. (2003). Multiple expansion method in the Hilbert problem. Fluid Dynamics 4: 646.

[4] Grad, H., Principles of the kinetic theory of gases (1958). Handbuch der Physik Band XII. Berlin: Springer-Verlag.

[5] Sderholm, L.H. (2007). Stable equations to second order in the fluid dynamics variables. Rarefied Gas Dynamics 25: 143-148.

[6] Sone, Y. (2002). Kinetic theory and fluid dynamics. Boston: Birkhuser.