arXiv:1108.4757v2 [nucl-ex] 5 Sep 2011

CUORE crystal validation runs: results on radioactive contamination and extrapolation to CUORE background

F. Alessandria^a, E. Andreotti^{b,c,1}, R. Ardito^d, C. Arnaboldi^e, F. T. Avignone III^f, M. Balata^g, I. Bandac^f, T. I. Banks^{h,i,g}, G. Bari^j, J. W. Beeman^k, F. Bellini^{l,m}, A. Bersani^n, M. Biassoni^{e,c}, T. Bloxham^i, C. Brofferio^{e,c}, A. Bryant^{i,h}, C. Bucci^g, X. Z. Cai^o, L. Canonica^{p,n}, S. Capelli^{e,c}, L. Carbone^c, L. Cardani^{l,m}, M. Carrettoni^{e,c}, N. Chott^f, M. Clemenza^{e,c}, C. Cosmelli^{l,m}, O. Cremonesi^c, R. J. Creswick^f, I. Dafinei^m, A. Dally^q, A. De Biasi^r, M. P. Decowski^{i,h,2}, M. M. Deninno^j, A. de Waard^s, S. Di Domizio^{p,n}, L. Ejzak^q, R. Faccini^{l,m}, D. Q. Fang^o, H. A. Farach^f, E. Ferri^{e,c}, F. Ferroni^{l,m}, E. Fiorini^c, L. Foggetta^{b,c}, S. J. Freedman^{i,h}, G. Frossati^s, A. Giachero^c, L. Gironi^{e,c}, A. Giuliani^t, P. Gorla^u, C. Gotti^{e,c}, E. Guardincerri^{g,i}, T. D. Gutierrez^v, E. E. Haller^{k,w}, K. Han^i, K. M. Heeger^q, H. Z. Huang^x, K. Ichimura^i, R. Kadel^y, K. Kazkaz^z, G. Keppel^r, L. Kogler^{i,h}, Yu. G. Kolomensky^{y,h}, S. Kraft^{e,c}, D. Lenz^q, Y. L. Li^o, X. Liu^x, E. Longo^{l,m}, Y. G. Ma^o, C. Maiano^{e,c}, G. Maier^d, C. Martinez^f, M. Martinez^{c,aa,3}, R. H. Maruyama^q, N. Moggi^j, S. Morganti^m, S. Newman^{f,g}, S. Nisi^g, C. Nones^{b,c,4}, E. B. Norman^{z,ab}, A. Nucciotti^{e,c}, F. Orio^m, D. Orlandi^g, J. Ouellet^{i,h}, M. Pallavicini^{p,n}, V. Palmieri^r, L. Pattavina^c, M. Pavan^{e,c}, M. Pedretti^z, G. Pessina^c, S. Pirro^c, E. Previtali^c, V. Rampazzo^r, F. Rimondi^{ac,j}, C. Rosenfeld^f, C. Rusconi^c, C. Salvioni^{b,c}, S. Sangiorgio^z, D. Schaeffer^{e,c}, N. D. Scielzo^z, M. Sisti^{e,c}, A. R. Smith^{ad}, F. Stivanello^r, L. Taffarello^{ae}, G. Terenziani^r, W. D. Tian^o, C. Tomei^m, S. Trentalange^x, G. Ventura^{af,ag}, M. Vignati^{l,m}, B. Wang^{z,ab}, H. W. Wang^o, C. A. Whitten Jr.^{x,5}, T. Wise^q, A. Woodcraft^{ah}, N. Xu^i, L. Zanotti^{e,c}, C. Zarra^g, B. X. Zhu^x, S. Zucchelli^{ac,j}

aINFN - Sezione di Milano, Milano I-20133 - Italy bDipartimento di Fisica e Matematica, Università dell’Insubria, Como I-22100 - Italy cINFN - Sezione di Milano Bicocca, Milano I-20126 - Italy dDipartimento di Ingegneria Strutturale, Politecnico di Milano, Milano I-20133 - Italy eDipartimento di Fisica, Università di Milano-Bicocca, Milano I-20126 - Italy fDepartment of Physics and Astronomy, University of South Carolina, Columbia, SC 29208 - USA gINFN - Laboratori Nazionali del Gran Sasso, Assergi (L’Aquila) I-67010 - Italy hDepartment of Physics, University of California, Berkeley, CA 94720 - USA iNuclear Science Division, Lawrence Berkeley National Laboratory, Berkeley, CA 94720 - USA jINFN - Sezione di Bologna, Bologna I-40127 - Italy kMaterials Science Division, Lawrence Berkeley National Laboratory, Berkeley, CA 94720 - USA lDipartimento di Fisica, Università degli Studio di Roma “La Sapienza”, Roma I-00185 - Italy mINFN - Sezione di Roma, Roma I-00185 - Italy nINFN - Sezione di Genova, Genova I-16146 - Italy oShanghai Institute of Applied Physics (Chinese Academy of Sciences), Shanghai 201800 - China pDipartimento di Fisica, Università di Genova, Genova I-16146 - Italy qDepartment of Physics, University of Wisconsin, Madison, WI 53706 - USA rINFN - Laboratori Nazionali di Legnaro, Legnaro (Padova) I-35020 - Italy sKamerlingh Onnes Laboratorium, Leiden University, Leiden, RA 2300 - The Netherlands tCentre de Spectrométrie Nucléaire et de Spectrométrie de Masse, 91405 Orsay Campus - France uINFN - Sezione di Roma Tor Vergata, Roma I-00133 - Italy vPhysics Department, California Polytechnic State University, San Luis Obispo, CA 93407 - USA wDepartment of Materials Science and Engineering, University of California, Berkeley, CA 94720 - USA xDepartment of Physics and Astronomy, University of California, Los Angeles, CA 90095 - USA yPhysics Division, Lawrence Berkeley National Laboratory, Berkeley, CA 94720 - USA zLawrence Livermore National Laboratory, Livermore, CA 94550 - USA aaLaboratorio de Fisica Nuclear y Astroparticulas, Universidad de Zaragoza, Zaragoza 50009 - Spain abDepartment of Nuclear Engineering, University of California, Berkeley, CA 94720 - USA acDipartimento di Fisica, Università di Bologna, Bologna I-40127 - Italy adEH&S Division, Lawrence Berkeley National Laboratory, Berkeley, CA 94720 - USA aeINFN - Sezione di Padova, Padova I-35131 - Italy afDipartimento di Fisica, Università di Firenze, Firenze I-50125 - Italy agINFN - Sezione di Firenze, Firenze I-50125 - Italy ahSUPA, Institute for Astronomy, University of Edinburgh, Blackford Hill, Edinburgh EH9 3HJ - UK

Abstract

The CUORE Crystal Validation Runs (CCVRs) have been carried out since the end of 2008 at the Gran Sasso National Laboratories, in order to test the performances and the radiopurity of the TeO_2 crystals produced at SICCAS (Shanghai Institute of Ceramics, Chinese Academy of Sciences) for the CUORE experiment. In this work the results of the first 5 validation runs are presented. Results have been obtained for bulk contaminations and surface contaminations from several nuclides. An extrapolation to the CUORE background has been performed.

Preprint submitted to Elsevier September 6, 2011

1. Introduction 1 The production of the CUORE [1] crystals was appointed to 2 SICCAS (Shanghai Institute of Ceramics, Chinese Academy of 3 Sciences) and began in March 2008, with the synthesis of the 4 TeO_2 powder. Given the goal of CUORE in terms of back- 5 ground (<0.01 counts/keV/kg/y at the Q-value [2]), the radiop- 6 urity of the TeO_2 crystals is a crucial issue. 7 Radioactive contaminations may come from long-lived, nat- 8 urally occurring isotopes, such as^{238}U and^{232}Th and their 9 daughters and from cosmogenic activation of the detector mate- 10 rials after their production. To minimize the influence of long- 11 lived nuclei, great care is devoted to the selection of all materi- 12 als and ancillaries used for the preparation of the detector. Sea 13 level transport and underground storage of prepared crystals are 14 necessary in order to minimize their cosmogenic activation. 15 A dedicated protocol [3] is defined for the radio-purity re- 16 lated quality control of the crystal production process, start- 17 ing from metallic tellurium synthesis to the final processing 18 of ready-to-use TeO_2 crystals. Radio-purity certification pro- 19 cedures, involving ICP-MS (Inductively Coupled Plasma Mass 20 Spectrometry) measurements, γ spectroscopy with HPGe de- 21 tectors and α spectroscopy with Surface Barriers Detectors 22 (SBD), are applied in each production phase to test the above 23 mentioned materials. 24 At the same time, cryogenic tests are designed to test the 25 ready-to-use TeO_2 crystals upon their arrival at LNGS. The 26 crystal validation is performed through experimental runs, each 27 called CCVR (CUORE Crystal Validation Run), in which 4 28 crystals randomly chosen from a batch coming from SICCAS, 29 are mounted in an setup similar to a CUORE single module and 30 operated at cryogenic temperatures for a time period of several 31 weeks in order to test the bolometric performance and the com- 32 pliance of the crystals to the contract limits in terms of radio- 33 purity (see Table 1).

Isotope Allowed Contamination 238U < 3 ·10^{−13} g/g 232Th < 3 ·10^{−13} g/g 210Pb < 1 ·10^{−5} Bq/kg 210Po < 0.1 Bq/kg

Table 1: Contamination limits for the ready-to-use TeO_2 crystals [3]. 34 In this work the results of the first 5 validation runs, carried 35 out from the end of 2008 to the middle of 2010, are presented. 36 A summary of all CCVRs detector operation is reported in Ta- 37 ble 2. The 4 crystals tested in CCVR1 (two of them were again 38 tested in CCVR2) were sent to LNGS by plane. This was neces- 39 sary in order to ensure a fast response on the radioactivity level 40 of the crystals. All the other crystals were transported by ship. 41 1Presently at: Joint Research Center, Institute for Reference Materials and Measurements, 2440 Geel - Belgium

2Presently at: Nikhef, 1098 XG Amsterdam - The Netherlands 3Presently at: Institut d’Astrophysique Spatial, 91045 Orsay - France 4Presently at: CEA / Saclay, 91191 Gif-sur-Yvette - France 5Deceased

Run Duration Livetime [d] CCVR1 Dec 20, 2008 - Mar 9, 2009 59.9 CCVR2 Jun 6, 2009 - Jun 30, 2009 19.4 CCVR3 Nov 11, 2009 - Jan 4, 2010 43.05 CCVR4 Mar 31, 2010 - May 17, 2010 25.8 CCVR5 Aug 11, 2010 - Oct 1, 2010 30.3

Table 2: Summary of CCVR data taking period and live time.

Radioactivity study was performed on the high energy re- 42 gion of the spectrum (above 4000 keV), where the contribution 43 of the α lines from uranium and thorium decay chains is ex- 44 pected. Given the short range of α particles, their signature 45 is a clear indication of a radioactive contamination within the 46 crystals or on their surface. Results (mainly upper limits) are 47 obtained for both bulk contaminations (Sec. 5) and surface con- 48 taminations (Sec. 7). For^{210}Pb, for which the study of the α 49 lines was not possible, the lower energy portion of the spectrum 50 has been used (Sec. 6). 51 An extrapolation to the CUORE background is performed in 52 Sec. 8. 53 2. Experimental setup 54 Each CCVR setup consists of an array of four crystals, ar- 55 ranged in a single floor which in a first approximation repre- 56 sents the single CUORE module. The four 5 × 5 × 5 cm^3 crys- 57 tals are enclosed in a pair of Oxygen Free High Conductivity 58 (OFHC) copper frames which serve both as mechanical support 59 and thermal bath. The two frames are connected to each other 60 by four small columns, also made of copper. Both frames and 61 copper are wrapped with several layers of polyethylene. The 62 crystals are connected to the copper frames by small Teflon 63 supports that represent the weak thermal conductance versus 64 the heat sink. 65 Each crystal is provided with a Neutron Transmutation 66 Doped Ge thermistor (NTD), which converts the phonon signal 67 into a detectable voltage pulse [4]. Some of the CCVR crystals 68 are provided with two NTD thermistors. In these cases both 69 channels are analyzed and the best performing channel (from 70 the point of view of the energy resolution) is used for the final 71 results. 72 The CCVR experimental setup is hosted in a dilution refrig- 73 erator placed in the Hall C of National Laboratory of INFN at 74 Gran Sasso and operated at ∼ 10 mK. A complete description 75 can be found in [5] and references therein for what concerns 76 the electronics and the DAQ and in [6] for what concerns the 77 cryogenic setup and the shields. 78 3. Data analysis 79 CCVR data processing, from raw data to the final spectra, 80 follows the procedure described in details in [7]. 81 The pulse amplitude is estimated by means of an Optimum 82 Filter (OF) technique [8] that reduces the noise superimposed 83 to the signal, maximizing the signal to noise ratio. 84

The mean detector response and the noise power spectral 85 density, needed to build the OF transfer function, are esti- 86 mated from bolometric pulses and noise samples (data samples 87 recorded randomly and without triggered events) by a proper 88 averaging procedure. 89 Gain instability corrections [7] are performed using the 90 5407.5 keV α line from^{210}Po. This element is always present 91 in recently grown crystals but decays away with a half life of 92 138.38 days. 93 The energy calibration is performed using^{232}Th γ sources 94 inserted inside the cryostat external lead shield. An example of 95 calibration spectrum (Channel2 - CCVR1) is shown in Fig. 1. 96 Gamma lines from the^{232}Th decay chain are clearly visible in 97 the spectrum. The calibration is performed using a third-order 98 polynomial function and the^{210}Po peak is used in addition to 99 the^{232}Th γ peaks.

Figure 1: Calibration spectrum of Channel2 - CCVR1. Gamma lines from the 232Th decay chain are visible in the spectrum. 100 Each CCVR sum spectrum is composed by events which sur- 101 vive two different type of data selection: global and event-based 102 requirements. 103 Global requirements are applied following criteria decided a 104 priori on the detector performances (an excessive noise level, 105 ADC saturation, etc..). They identify bad time intervals that 106 need to be discarded. These kind of cuts introduce a dead time 107 that is accounted for by properly reducing the live time of the 108 interested detector. 109 Event-based requirements comprise: pile-up rejection, pulse- 110 shape and coincidence selection. 111 The presence of a pile-up prevents the OF algorithm from 112 providing a correct evaluation of the pulse amplitude. The pile- 113 up rejection is performed by imposing an extendable (paralyz- 114 able) dead window of 7 seconds to each event. 115 The pulse-shape analysis is used to reject non-physical 116 events. The pulse shape parameters are the rise time and de- 117 cay time of the OF-filtered waveform and other parameters that 118 measure the deviation of filtered raw signal from the average 119 detector response. 120 As a first step, each CCVR spectrum is corrected for the cor- 121 responding efficiency of the event-based cuts (from Table 3) and 122 then the spectra are summed together. Four types of spectra are 123 produced for all CCVRs: 124 • Total Energy spectrum (TOT): it contains all the general 125 cuts and the pulse shape cuts. 126

• Anti-coincidence Energy spectrum (M1): it contains the 127 events that caused an energy deposition in one crystal only 128 (anti-coincidence cut). For what concerns α particles, this 129 corresponds to bulk events (that is decays where the emit- 130 ted α particle is absorbed within the crystal itself) and to 131 surface events, generated by decays occurring on the sur- 132 face of an inert material that hit a facing crystal, or to α de- 133 cays occurring on a crystal surface, whose escaping prod- 134 ucts are absorbed by inert materials. 135 • Coincidence Energy spectrum (M2): it contains the 136 events that caused an energy deposition in two crystals. 137 For what concerns α particles, these events arise from α 138 decays occurring on a crystal surface faced to another crys- 139 tal. 140 • Coincidence Sum Energy spectrum (M2sum): it con- 141 tains the sum energy of multiplicity 2 events. For instance 142 in the case of an α decay on the surface of a crystal, both 143 the energy of the α particle E_1 in the facing crystal and 144 the corresponding nuclear recoil energy E_2 in the original 145 crystal are detected. In the spectrum M2sum the variable 146 E_{T OT} = E_1 + E_2 is plotted. 147 Fig. 2 shows the sum spectra of all CCVRs.

Figure 2: Energy spectra for the full CCVR statistics. Top: anti-coincidence and coincidence spectra. Bottom: Sum energy spectrum of multiplicity 2 events. 148 3.1. Efficiency of event-based cuts 149 Due to the high rate of^{210}Po events, there is a significant 150 loss of efficiency due to pile-up rejection. The efficiency is es- 151 timated as: 152 ε_{pile−up} = 1 − P_{pile−up} = e^{(−r·T )} (1) 153

where P is the probability of a pile-up, r is the counting rate of 154 the events that passed the global cuts described above, and T is 155 the length of a time interval containing an event during which 156 the occurrence of another event would be considered pile-up. 157 The interval T contains some time after the event during which 158 a double pulse would result and some time before the event 159 during which the event’s baseline would be spoiled by the tail 160 of the preceding pulse. Properly, T depends on the energy of 161 the other event: the higher the energy of the other event, the 162 longer its tail remains too large. The counting-rate is channel- 163 dependent and sometimes also time-dependent. In the specific 164 case of^{210}Po events, the counting-rate obviously decreases with 165 time due to polonium decay (half-life: 138.38 days). 166 For the sake of simplicity, an average pile-up reduction ef- 167 ficiency for each CCVR is computed. This will apply to all 168 channels in the full energy range and is calculated using for- 169 mula (1) with T = 7 s and using as r the global counting rate 170 after the general cuts.

Run ε_{pile−up} ε_{PSA} ε_{AC} CCVR1 0.84 ±0.01 0.96±0.01 0.987±0.003 CCVR2 0.88 ±0.01 0.98±0.01 0.982±0.005 CCVR3 0.89 ±0.01 0.97±0.01 0.990±0.002 CCVR4 0.88 ±0.01 0.94±0.02 0.987±0.003 CCVR5 0.89 ±0.01 0.98±0.01 0.990±0.003

Table 3: Efficiencies of event-based cuts for each CCVR. 171 The pulse shape cuts efficiency ε_{PSA} is evaluated on the back- 172 ground peak at 2614.5 keV due to^{208}Tl, by a simultaneous fit 173 on both the spectra of accepted and rejected events as detailed 174 in [7]. 175 The same procedure is applied for the evaluation of the anti- 176 coincidence cut efficiency ε_{AC}. In this case, instead of the 177 2614.5 keV line (which is usually in coincidence with other γ 178 lines), the photopeak at 1460.8 keV due to^{40}K is used. Results 179 are summarized in Table 3. 180 3.2. Monte Carlo simulations 181 In order to extract numerical information on the activity 182 or contamination of a given nuclide in CUORE crystals from 183 CCVRs data, it is necessary to rely on Monte Carlo simula- 184 tions, capable of reproducing the main features of the detector 185 geometry and response. 186 CCVRs simulations are performed with the GEANT4-based 187 code developed by the CUORICINO ad CUORE collaboration 188 and described in [9] and [10]. The simulation takes into ac- 189 count the energy resolution and the threshold of each detector. 190 For bulk contaminations, an homogeneous distribution of the 191 given nuclide inside the crystals is assumed. For surface con- 192 taminations, different depths of the contamination layer (from 193 0.01 μm to 10 μm) are considered and the contamination den- 194 sity profile is assumed to decrease exponentially with the depth 195 from the surface to the bulk of the crystal. 196 In CCVR1 there is a not negligible number of measurements 197 (∼ 4%) with only 2 active facing crystals. This affects the effi- 198

ciency calculation of surface contaminations. To take into ac- 199 count this variation from the standard configuration with 4 crys- 200 tals, 2 different efficiencies are calculated for each Monte Carlo 201 simulation: 202 • ε^{2ch}_{MC} : corresponding to the CCVR1 configuration with only 203 2 active crystals; 204 • ε^{4ch}_{MC} : corresponding to the standard CCVR configuration, 205 with 4 active crystals; 206 The average efficiency, weighed on the proper lifetime Δt^i, is 207 computed using the formula: 208 ε_{MC} = ε^{2ch}_{MC} Δt^{2ch} + ε^{4ch}_{MC} Δt^{4ch} Δt^{2ch} + Δt^{4ch} (2) 209

4. Results on background rates of CUORE crystals 210 From the energy spectra of all CCVRs the background rates 211 in various energy regions can be calculated. 212 Six energy regions of interest are identified in the spectra and 213 the corresponding count rates for anticoincidence (M1) and co- 214 incidence (M2) spectra are calculated. Results for the global 215 spectra are reported in Table 4 (errors are statistical only).

Continuum^{190}Pt Continuum (2700, 3200) (3200, 3400) (3400, 3900) [keV] [keV] [keV] M1 0.19±0.02 0.38±0.04 0.09±0.01 M1-PoSub 0.13±0.02 0.34±0.04 0.06±0.01 M2 0.05±0.01 0.02±0.01 0.025±0.006 M2-PoSub 0.02±0.01 0.01±0.01 0.008±0.008 U/Th^{210}Po U/Th (4000, 5000) (5000, 6000) (6000, 8000) [keV] [keV] [keV] M1 0.19±0.01 - 0.057±0.004 M1-PoSub 0.13±0.01 - 0.057±0.004 M2 0.04±0.01 - 0.014±0.002 M2-PoSub 0.014±0.007 - 0.014±0.002

Table 4: Count rates measured in [counts/keV/kg/y]. Errors are statistical. 216 The continuum region (2700, 3200) keV is of great interest 217 since it is the region immediately above the Q-value of the neu- 218 trinoless double beta decay of^{130}Te [7]. 219 In the region (3200, 3400) keV a contribution of the α line 220 from^{190}Pt is expected. This contamination is almost unavoid- 221 able for TeO_2 crystals, as explained in Sec. 5. 222 From 4000 to 8000 keV the contribution of the various α 223 lines from U and Th decay chains is expected. 224 In between, there is the region (5000, 6000) keV, which is 225 affected by the^{210}Po contamination (see Sec. 5.1). This pro- 226 duces not only a peak at the energy of the Po α line 5407.5 227 keV but also a broad background over the entire region due to 228 mis-identified pile-up events (above the peak energy) or to the 229 escape of the α that releases part of its energy in a inert material 230 (below the peak energy). An indication of the rate in this region 231 is of no particular interest, also because of the relative short 232

half-life of^{210}Po (138.38 days) that guarantees a huge reduc- 233 tion of this count rate when CUORE will start the data taking. 234 4.1. Subtraction of^{210}Po induced rate 235 Because of the presence of^{210}Po, an excess of count rate 236 could arise in the M1 and M2 spectra below the energy of the 237 5407.5 keV α line, if the contamination of^{210}Po is close enough 238 to the surface for the α to escape and release part of its energy 239 in an inert material (M1 spectrum) or in a nearby detector (M2 240 spectrum). This contribution from the M2 spectrum can be esti- 241 mated, calculating for each energy region the rate of M2 events 242 in which the total energy E_{T OT} lies in the interval (5407.5±50) 243 keV. The M2 count rate subtracted for this contribution is de- 244 fined as M2-PoSub and reported in Table 4 for comparison. 245 In a similar way the contribution of surface^{210}Po in the M1 246 spectrum is evaluated. Because of the geometry of the CCVR 247 setup, our coincidence analysis is sensitive only to 8 faces over 248 24. So the anti-coincidence count rate due to^{210}Po of the re- 249 maining 16 faces is assumed to be two times the coincidence 250 one, calculated on the M2 spectrum as described above.^6 The 251 M1 count rate subtracted for the surface^{210}Po contribution is 252 defined as M1-PoSub and reported in Table 4. 253 4.2. Background rates comparison with previous TeO_2 detec- 254 tors 255 It is interesting to compare CCVRs rates with the ones ob- 256 tained with previous detectors, like TTT [11] or Cuoricino [7]. 257 This comparison is shown in Table 5, where the M1 and M2 258 count rates for CCVRs are after polonium subtraction, as de- 259 scribed in 4.1. 260 The notation (2700, 3900) refers to the combination of both 261 the continuum region (2700, 3200) keV and (3400, 3900) keV, 262 excluding the^{190}Pt energy region of (3200, 3400) keV. It can be 263 inferred that : 264 • in the region (2700, 3900) keV the CCVRs anti- 265 coincidence rate is compatible within 1.8 σ with the cor- 266 responding TTT value. 267 • in the region (4000, 5000) keV, as already measured in 268 the TTT run, a reduction in the count rate with respect to 269 Cuoricino is observed. 270 • in the region (5000, 6000) keV a comparison is not possi- 271 ble since CCVR is affected by the high rate of^{210}Po. This 272 is due to the fact that in CCVRs only recently grown crys- 273 tals are measured, unlike TTT or Cuoricino. 274 • in the region (6000, 8000) keV, as already measured in 275 the TTT run, a reduction in the count rate with respect to 276 Cuoricino is present. However, the CCVR count rate is 277 greater than the TTT value, probably because of the pres- 278 ence of mis-identified pile-up (in M1) or coincidences (in 279 M2) with^{210}Po events, extending above 6000 keV. This 280 contribution should decay away with^{210}Po. 281

6In some of CCVR1 measurements (∼ 4% of the CCVR lifetime) only two facing crystals were active. The extrapolation of M2 counts to M1 is performed considering that the coincidence analysis is sensitive only to 2 over 12 faces.

Continuum U/Th (2700, 3900) (4000, 5000) [keV] [keV] CCVR M1 0.09±0.02 0.13±0.01 M2 0.015±0.007 0.014±0.003 TTT M1 0.052 ±0.008 0.28±0.02 M2 0.009±0.003 0.0018±0.005 Cuoricino M1 0.104 ±0.002 0.522±0.003 M2 0.009± 0.001 0.084±0.001

210Po U/Th (5000, 6000) (6000, 8000) [keV] [keV] CCVR M1 - 0.057±0.004 M2 - 0.014±0.002 TTT M1 1.30±0.07 0.025 ± 0.004 M2 0.09±0.01 0.005 ± 0.002 Cuoricino M1 0.846±0.004 0.099 ± 0.001 M2 0.173±0.002 0.0163 ± 0.0004

Table 5: Count rate comparison with previous detectors, measured in [counts/keV/kg/y]. Here CCVR values are after polonium subtraction, as described in 4.1. Errors are statistical.

A more detailed evaluation of the comparison can be found 282 in [11]. 283 5. Results on bulk contaminations of CUORE crystals 284 Bulk contaminations in CUORE crystals are expected from: 285 •^{210}Po, as a result of the chemical affinity between polo- 286 nium and tellurium; 287 • natural contaminants, like^{238}U and^{232}Th with their ra- 288 dioactive chains; 289 •^{210}Pb, as a result of the deposition of lead nuclei produced 290 by^{222}Rn decays, during the crystal handling in free atmo- 291 sphere; 292 •^{190}Pt, due to the fact that platinum is used in several phases 293 of the crystal production cycle. Platinum crucibles are 294 used for the calcination of TeO_2 powder used for the crys- 295 tal growth and the growth crucibles are made of platinum 296 foil. The central part of the as-grown crystal ingot is se- 297 lected for the CUORE crystals in order to avoid the risk of 298 platinum contamination on the surface of the crystal due 299 to possible diffusion during the growth process. Possible 300 Pt contaminations are therefore in the bulk of the CUORE 301 crystals. 302 For^{210}Po the activity is determined from a fit to the anti- 303 coincidence rate vs. time behaviour (see Sec. 5.1). 304 For^{238}U and^{232}Th (see Sec. 5.2), the limit on the level of 305 contamination is determined from the intensities of the α peaks 306 in the anti-coincidence spectrum of all crystals, or from inte- 307 grals centered at the peak position if the peaks are not visible. 308

This is because an α decay from bulk contamination releases 309 the entire Q-value of the reaction (α energy + nuclear recoil) in 310 a single crystal. 311 For^{210}Pb, the limit on bulk contamination is determined 312 from a fit in the energy region (40, 60) keV in a subset of 313 CCVRs data with high statistics and low threshold (see Sec. 6). 314 5.1.^{210}Po bulk activity 315 The activity of^{210}Po can be measured from the intensity of 316 5407.5 keV α line in the anti-coincidence spectrum. 317 The plot in Fig. 3 shows the global rate of^{210}Po events over 318 time for CCVR1. For each channel the^{210}Po events are selected 319 in a ± 20 keV window around the energy of the α line. 320

Figure 3: Global rate of^{210}Po events over time for each CCVR1. The fit result is overlayed.

The units on the x-axis are days since the start of the first 321 background measurement. Each point represents a group of 322 measurements whose livetime is at least 5 days. 323 The horizontal error bars indicate the beginning and the end 324 of each group of runs, they are for visualization only. 325 Each point is corrected with the corresponding rate-based ef- 326 ficiency, calculated with the equation (1). A larger dead time 327 window (9 seconds instead of 7 seconds) compared to the rest 328 of the analysis is used, to be more conservative in the removal 329 of pile-up pulses. 330 The fit function is a pure exponential: 331 r(t) = r_0e^{(−ln2 t/T1/2)} (3) 332 where r_0 is the rate at the beginning of the measurement and 333 T_{1/2} is the^{210}Po half-life. The half-life of the exponential decay 334 has been evaluated for all CCVRs and it is shown in Tab 6: it is 335 in good agreement (1 σ) with the half-life of^{210}Po (138.38 d). 336 This indicates that the^{210}Po contamination is out of equilibrium 337 and it is not being fed by^{210}Pb. 338 From the value of r_0 returned by the fit for each CCVR and 339 for each crystal, the^{210}Po activity at the beginning of the mea- 340 surement is extracted as follows: 341 A[Bq/kg] = r_0 86400[s/day] m[kg] (4) 342 where m is the crystal mass. 343 Knowing the time elapsed since the ”crystal birth date” 344 (growth completed, before the cut and shape) and the start of 345 the measurement, the^{210}Po activity at production is computed. 346

Run Half-life [days] CCVR1 138.0± 2.5 CCVR2 132.3 ± 14.7 CCVR3 139.4 ± 6.3 CCVR4 137.8 ± 11.5 CCVR5 136.6 ± 9.1

Table 6:^{210}Po half-life for all CCVRs. The activity has been fitted using an exponential function. All the values are consistent (within 1 σ) with 138.38 days.

The^{210}Po activities for each CCVR and for all crystals are 347 reported in Table 7. The results for crystals 007 and 011, mea- 348 sured first in CCVR1 and again in CCVR2, are consistent. 349 All crystals tested in the first five CCVRs are well below the 350 limit of 0.1 Bq/kg imposed to the crystal producers.

CCVR Crystal^{210}Po activity [Bq/kg] 1 041 0.0257 ± 0.0001 1 011 0.0510 ± 0.0005 1 039 0.0229 ± 0.0001 1 007 0.0414 ± 0.0004 2 076 0.021 ± 0.004 2 011 0.07 ± 0.02 2 096 0.055 ± 0.006 2 007 0.047 ± 0.015 3 190 0.0078 ± 0.0005 3 236 0.0159 ± 0.0005 3 180 0.0203 ± 0.0008 3 229 0.0283 ± 0.0008 4 340 0.032 ± 0.004 4 313 0.005 ± 0.001 4 354 0.039 ± 0.004 4 380 0.040 ± 0.004 5 455 0.019 ± 0.002 5 416 0.024 ± 0.003 5 436 0.032 ± 0.003 5 421 0.020 ± 0.003

Table 7:^{210}Po activity at production time for all CCVRs crystals. 351 5.2. U/Th bulk contaminations 352 238U and^{232}Th bulk contaminations are evaluated from the 353 anti-coincidence sum spectrum of all CCVRs. For each of the 354 peaks reported in Table 8, the number of counts (corrected by 355 the efficiency of the event-based cuts from Table 3) within an 356 energy window of ±6 σ around the α Q-value is estimated. A 357 σ of 2.2 keV, corresponding to the average between the values 358 of the^{210}Po peak σs for each CCVR, weighted by the corre- 359 sponding lifetime of that run (see Table 9 for details) is used. 360 Using the Bayesian approach, the upper limits N_u at 90% C.L. 361

Chain Nuclide Energy Half-life N_u [keV] 90% C.L.

238U^{238}U 4270.0 4.47E+09 y 11.7 234U 4858.8 2.45E+05 y 20.8 230Th 4770.0 7.54E+04 y 24.9 226Ra 4870.6 1599 y 30.0 218Po 6114.7 3.05 min 7.4 232Th^{232}Th 4082.8 1.4E+10 y 5.9 212Bi 6207.1 60.55 min 13.5

Table 8: 90% C.L. limits on the number of events ascribed to several nuclides from uranium and thorium decay chain. For each nuclide is also shown the Q-value and the half-life of the α decay.

Run Livetime σ [days] [keV] CCVR1 59.9 1.6 CCVR2 19.4 1.4 CCVR3 43.05 2.2 CCVR4 25.8 3.5 CCVR5 30.3 2.8

Table 9: Summary of CCVRs energy resolutions, evaluated with a gaussian fit of the 5407.5 keV peak from^{210}Po. The average value of 2.2 keV, used for the global analysis is obtained averaging the resolution of each CCVR with the corresponding livetime.

are obtained, assuming 0 expected background counts and a flat 362 prior for the signal [12] (see Table 8). 363 The upper limit on the activity for each nuclide is calculated 364 using the following formula: 365 A_u[Bq/kg] =

N_u ε_{MC} T [s] m[kg] Γ (5) 366 where ε_{MC} is the Monte Carlo detection efficiency, T the 367 CCVRs livetime, m the crystal mass and Γ the branching ratio 368 of the nuclide. In this analysis a total containment of the anti- 369 coincidence events in the crystals is assumed (ε_{MC} =1). Results 370 are shown in Table 10. 371 The upper limit for confidence level of 90% for U/Th bulk 372 contaminations are then calculated in the hypothesis of secular 373 equilibrium within the uranium and thorium decay chains. Re- 374 sults for the total CCVRs data are shown in the last column of 375 Table 10. 376 In the most conservative approach, the bulk contamination 377 limit on^{238}U and^{232}Th is set considering the most active nu- 378 clide for each chain. The upper limit at 90% C.L. for uranium 379 and thorium bulk contamination are: 380 238U < 5.3 · 10^{−14}[g/g] 232Th < 2.1 · 10^{−13}[g/g]

Both values of the upper limits are within the contract specifica- 381 tion of 3·10^{−13}[g/g]. For the^{238}U decay chain, the contribution 382 from^{210}Pb is treated separately (see Sec. 6). 383 It is important to stress the fact that the above upper limits 384 are calculated under the hypothesis that the observed counts for 385

Chain Nuclide Upper limit Upper limit [Bq/kg] [g/g] 238U^{238}U 2.5E-07 2.0E-14 234U 4.7E-07 3.6E-14 230Th 5.7E-07 4.4E-14 226Ra 6.7E-07 5.3E-14 218Po 1.6E-07 1.3E-14 232Th^{232}Th 1.3E-07 3.1E-14 212Bi 8.4E-07 2.1E-13

Table 10: Upper limits at 90% C.L. on the activity and on the bulk contamination of uranium and thorium decay chains in the hypothesis of secular equilibrium.

each nuclide are entirely due to a bulk contamination of that 386 nuclide. This is a conservative hypothesis since there is not a 387 clear indication (for example a line) that such a bulk contami- 388 nation actually exists and that the observed counts are not due 389 to background of some other origin. 390 6.^{210}Pb activity 391 During the production of CUORE crystals great care is de- 392 voted in order to minimize the exposure of the crystals to free 393 atmosphere, to avoid contamination of radon and its daugh- 394 ters. Nevertheless, a small^{210}Pb contamination (bulk or sur- 395 face) might occur. This contamination can be very dangerous 396 because, even if the soft beta (16.96 keV and 63.5 keV) and 397 γ (46.5 keV) radiation from^{210}Pb is generally self absorbed, 398 the induced bremsstrahlung of the daughter^{210}Bi can give rise 399 to a continuum up to 1.16 MeV. Moreover, the α decay of the 400 daughter^{210}Po can contribute to the continuum background in 401 the double beta decay energy region. 402 In CCVRs crystals the^{210}Pb contamination cannot be esti- 403 mated from^{210}Po, because this contamination is out of equi- 404 librium (see Sec. 5.1). The only available signature is a com- 405 bination of a beta spectrum (end point 16.96 keV) with a de- 406 excitation energy of 46.5 keV (most of the cases through a con- 407 version electron). This produces a broad signature in the energy 408 region (40, 60) keV, whose shape depends on the location of the 409 Pb contamination. 410 Several simulations are performed both for a bulk contami- 411 nation and for a surface contamination with exponential density 412 profile [9] and contamination depth varying from 0.01 μm to 413 10 μm. Even if, for the sake of simplicity, a common energy 414 threshold of 50 keV is set for all CCVRs, there are subset of 415 data where the threshold can be set to a lower value in order to 416 look for this signature. CCVR1 data are used because they struk 417 a balance between high livetime (CCVR1 has the highest statis- 418 tic) and good bolometer performances. Only for CCVR1 data, 419 the analysis is repeated with an energy threshold of 40 keV. 420 The anti-coincidence spectrum between 40 and 60 keV is fit- 421 ted with an exponentially decreasing background and allowing 422 the presence of a^{210}Pb spectrum with shape taken from Monte 423 Carlo simulation. The free parameters of the fit are the two pa- 424 rameters of the exponential background and the total number 425

Figure 4: Top: Monte Carlo simulation of a^{210}Pb bulk contamination in CCVR1. Bottom: CCVR1 low energy anti-coincidence spectrum. The energy threshold is set to 40 keV. The red line represents the fit to the spectrum with an exponential background and allowing the presence of a^{210}Pb bulk contamination with the above shape. No hint of such contamination is found.

of counts from^{210}Pb. The fit is repeated for each Monte Carlo 426 signature. The number of^{210}Pb events is compatible with zero 427 within the error for all signatures. An example of Monte Carlo 428 spectrum for a^{210}Pb bulk contamination and the corresponding 429 fit to the experimental spectrum is shown in Fig. 4. 430 The upper limit at 90% C.L. on the number of^{210}Pb counts 431 is N_u = 1.644 σ, where σ is the error on the number of counts 432 returned from the fit. The upper limit on bulk contamination is 433 computed using Eq. 5. The upper limit on surface contamina- 434 tion is extracted using the following formula: 435 A_u[Bq/cm^2] =

N_u ε_{MC} T [s] S [cm^2] (6) 436 where ε_{MC} is the Monte Carlo detection efficiency, T is the live- 437 time and S is the surface of a crystal (150 cm^2). Results are 438 shown in Table 11. The upper limit on the activity for bulk 439 contamination is below the contract limit of 10^{−5} Bq/kg (see 440 Table 1). 441 7. Results on surface contaminations of CUORE crystals 442 Surface contaminations of CUORE crystals are expected 443 from the same nuclides listed in Sec. 5, except for^{190}Pt, which 444 is all in the bulk. Uranium and thorium surface contaminations 445 can be investigated by means of coincident events in two fac- 446 ing crystals: surface contamination of an α-decaying nuclide 447 should appear in the total energy spectrum (M2sum in Fig. 2) 448 as a peak at the Q-value of the decay because the total energy (α 449 + nuclear recoil) is collected by the two facing crystals. At the 450 same time, if the surface contamination is deep enough, the α 451 particle can be absorbed by the crystal, giving rise to the same 452 signature of a bulk event. 453

contamination Upper limit 90% C.L.

bulk 3.3E-06 surf. 0.01μm 9.8E-07 surf. 0.1μm 3.8E-08 surf. 0.2μm 2.2E-08 surf. 1μm 9.2E-09 surf. 5μm 5.6E-09 surf 10μm 4.9E-09

Table 11: Upper limits on the activity of bulk and surface contamination of 210Pb. Bulk contamination is given in [Bq/kg], surface contaminations are given in [Bq/cm^2].

7.1. U/Th surface contaminations 454 The M2sum spectrum in Fig. 2 shows a huge background for 455 energies above the polonium α line due to random coincidences 456 between^{210}Po and low energy events. At a closer inspection 457 (see Fig. 5), the peaks originated by the sum of a 5407.5 keV α 458 line and a low energy γ line arising from Te metastable isotopes 459 are clearly visible. See also Table 12 for details.

Te isotope Energy Energy + 5407.5 [keV] [keV] 127Te 88.3 5495.8 129Te 105.5 5513 125Te 144.8 5552.3 123Te 247.5 5655 121Te 294 5701.5

Table 12: Energy of the gamma lines from Tellurium metastable isotopes and corresponding sum energy when in coincidence with a^{210}Po event. 460 Because of the presence of these coincidences, only nuclides 461 with a Q-value lower than 5407.5 keV (see Table 13) are used 462 for surface contamination analysis.^{218}Po and^{212}Bi are there- 463 fore discared. The scatter plot of M2 events is shown in Fig. 6. 464 The shadowed region contains the events with a total energy 465 within 4 and 5 MeV. 466 For each nuclide listed in Table 13, the number of counts is 467 computed from the M2sum energy spectrum in an energy win- 468 dow of ± 6σ around the Q-value and divided by ε^2 (where ε 469 is the efficiency of the event-based cuts of Table 3), since two 470 coincident events have independent probabilities of passing the 471 cuts. In Table 13 are shown the corresponding upper limits at 472 90% C.L., computed using the Bayesian approach with 0 ex- 473 pected background counts and a flat prior for the signal [12]. 474 Monte Carlo spectra for^{238}U and^{232}Th contamination on 475 the crystal surface are generated with exponential profile and 476 various penetration lengths. For each contamination depth, the 477 containment efficiency is calculated in a ± 6σ interval around 478 the Q-value of each nuclide both for the M2sum spectrum and 479 for the M1 spectrum. Results are shown in Fig. 7. For penetra- 480 tion length of 0.01 and 0.1μm the higher containment efficiency 481 comes from the M2sum spectrum, whereas for depths of 1, 5 482 and 10 μm this arises from the M1 spectrum. The efficiency 483

Figure 5: Top: M2sum spectrum in the region (5300, 6000) keV. Peaks originated by the coincidence of the 5407.5 keV α line and a low energy γ line from Te metastable isotopes are clearly visible. Bottom: total and anti-coincidence spectra in the region 0-500 keV: low energy lines from Te metastable isotopes are clearly visible.

Figure 6: Scatter plot of M2 events. The shadowed region contains events with total energy between 4 and 5 MeV, used for surface analysis.

Chain Nuclide Half-life Energy range N_u [y] [keV] 90% C.L.

238U^{238}U 4.47E+09 4257 - 4283 4.6 234U 2.45E+05 4845 - 4871 4.6 230Th 7.54E+04 4757 - 4783 4.6 226Ra 1599 4857 - 4883 10.5 232Th^{232}Th 1.4E+10 4069 - 4095 2.3

Table 13: Upper limits at 90% C.L. on the number of counts ascribed to several nuclides from uranium and thorium decay chain from the M2sum spectrum. For each nuclide, the half-life of the α decay is also shown.

Figure 7: For each penetration length, the containment efficiency of surface events is computed for both M1 and M2sum Monte Carlo spectra.

containment value for 0.2 μm depth is very similar both for M1 484 and M2sum spectrum. 485 The drop in M1 containment efficiency for very thin layers 486 of contaminations is due to the fact that, of the about 50% of 487 decays where the alpha is emitted toward the bulk of the crystals 488 and the recoil is emitted towards outside, in most of the cases 489 the recoil escapes undetected, thus the full Q-value of the alpha 490 decay is not recorded. 491 The upper limits at 90% C.L. for the surface activity of each 492 nuclide are evaluated using Eq. 6 where N_u is the 90% C.L. up- 493 per limit on the number of observed events from the M2sum 494 or the M1 spectrum (see Table 13 for the M2sum counts and 495 Table 8 for the M1 counts) and ε_{MC} is the Monte Carlo aver- 496 age efficiency defined in eq. 2 for the corresponding spectrum 497 (M2sum or M1) and for the given signature. The confidence 498 intervals for surface activity contaminations are calculated for 499 both the M2sum and M1 spectra, normalizing each signature 500 with the corresponding Monte Carlo efficiency. The signature 501 giving the most stringent result is taken into account. 502 For surface contaminations of 0.01, 0.1 and 0.2 μm depths, 503 the most stringent limits come from the M2sum spectrum. For 504 the remaining depths (1, 5 and 10 μm) the surface activity re- 505 duces practically to a bulk activity and the M1 signature pro- 506 duces the most stringent limits (see Table 8 for details). 507 For the^{238}U chain, the surface contamination for 2 peaks is 508 evaluated: 509 •^{238}U, the chain parent; 510 •^{226}Ra, the most active line both in M1 and M2sum spectra. 511 The contribution from^{210}Pb is treated separately (see Sec. 6). 512 For the^{232}Th chain there is only one useable line for this 513 analysis, that is the one from^{232}Th. This means that there is 514 no way of testing the portion of the chain below^{220}Rn and take 515 into account a possible non-equilibrium of the chain, as done 516 for the bulk contamination. 517 The results for surface contaminations are shown in Table 14. 518 As explained in Sec. 5.2, the above confidence intervals are cal- 519 culated under the hypothesis that the observed counts for each 520

nuclide are entirely due to a surface contamination of that nu- 521 clide in the corresponding depth. Again, this is a very conser- 522 vative hypothesis. 523 Depth Nuclide Upper limit 90% C.L. [Bq/cm^2] 0.01μm^{238}U 3.1E-09 226Ra 6.3E-09 232Th 1.6E-09 0.2μm^{238}U 3.8E-09 226Ra 7.6E-09 232Th 2.0E-09 1μm^{238}U 3.7E-09 226Ra 8.9E-09 232Th 1.9E-09 5μm^{238}U 2.0E-09 226Ra 5.4E-09 232Th 1.0E-09 10μm^{238}U 1.7E-09 226Ra 4.4E-09 232Th 8.3E-10

Table 14: Upper limits at 90% C.L. for surface contamination, for different penetration length values. See text for details on the calculation of confidence intervals.

8. Extrapolation to CUORE background 524 In order to evaluate the contribution to the CUORE back- 525 ground arising from crystal contamination, a simulation both 526 for bulk and surface contamination reproducing the CUORE 527 geometry and studying the contribution to the double beta de- 528 cay (DBD) energy region is performed. 529 Being interested in a conservative upper limit to the CUORE 530 background, in this extrapolation it has been assumed that 531 CUORE crystals will have the same activity as crystals tested 532 in CCVRs. However, when CUORE will start the data taking, 533 most of the^{210}Po (and other short lived states) will have de- 534 cayed and the efficiency for pile-up rejection will be increased. 535 8.1. Background from bulk contamination 536 The CUORE geometrical efficiency for a uniform bulk con- 537 tamination of crystals in^{210}Pb,^{238}U and^{232}Th is estimated via 538 Monte Carlo, and the corresponding CUORE background at the 539 DBD energy region (Q-value ± 30 keV) is calculated using the 540 formula: 541 bkg_{CUORE} =

A_{CCVR−bulk} ε^{CUORE−bulk} MC ΔE (7) 542 where A_{CCVR−bulk} are the values of^{210}Pb,^{238}U and^{232}Th ac- 543 tivities from Tables 10 and 11, ε^{CUORE−bulk}_{MC} is evaluated from 544 Monte Carlo simulation and ΔE = 60 keV. 545 The results are shown in Table 15. 546 In the most conservative approach, considering the most ac- 547 tive line (^{212}Bi), the following upper limit to the CUORE back- 548 ground at the DBD energy due to bulk contamination of crystals 549 is set: 1.1 · 10^{−4} counts/keV/kg/y. 550

chain Nuclide Upper Limit 90% C.L. [counts/keV/kg/y] 210Pb 2.6E-05 238U^{238}U 8.1E-07 234U 1.4E-06 230Th 1.7E-06 226Ra 2.1E-06 218Po 5.1E-07 232Th^{232}Th 1.7E-05 212Bi 1.1E-04

Table 15: Extrapolation to CUORE background from CCVRs bulk contamination limits from Tabs. 10 and 11.

8.2. Background from surface contamination 551 In a similar way, the CUORE geometrical efficiency for a 552 surface contamination for several depths is estimated. The cor- 553 responding CUORE background is extrapolated using the for- 554 mula: 555 bkg_{CUORE} =

A_{CCVR−surf} ε^{CUORE−surf}

MC S ΔE M_{CUORE} (8) 556 where A_{CCVR−surf} are the surface contamination values from Ta- 557 bles 11 and 14, ε^{CUORE−surf}

MC is estimated via Monte Carlo, S is 558 the surface of the CUORE crystals, ΔE = 60 keV and M_{CUORE} 559 = 0.75 · 988 kg. 560 Depth Nuclide Upper limit 90% C.L. [counts/keV/kg/y] 0.01μm^{210}Pb 1.6E-03 238U 8.9E-05 226Ra 1.8E-04 232Th 1.8E-05 0.2μm^{210}Pb 2.3E-04 238U 3.9E-04 226Ra 7.7E-04 232Th 1.5E-04 1μm^{210}Pb 3.8E-04 238U 1.2E-03 226Ra 2.9E-03 232Th 4.4E-04 5μm^{210}Pb 4.3E-04 238U 1.3E-03 226Ra 3.4E-03 232Th 4.7E-04 10μm^{210}Pb 2.9E-04 238U 7.1E-04 226Ra 1.9E-03 232Th 3.0E-04

Table 16: Extrapolation to CUORE background from CCVRs surface contamination limits from Tables 11 and 14.

The results are shown in Table 16. Based on these results, 561 in the most conservative approach, a crystal surface contam- 562 ination in CUORE within the limits estimated from CCVRs 563 data, would yield a rate in the DBD energy region lower than 564

Figure 8: For each penetration depth, the upper limits at 90% C.L. for the count rate at the DBD energy region are plotted. The values are computed on^{226}Ra line, and are due only to surface crystals contaminations.

5.5 · 10^{−3} counts/keV/kg/y. This value corresponds to the worst 565 case: a contamination in^{238}U and^{232}Th at 5μm and a contam- 566 ination in^{210}Pb at 0.01μm. This result is strictly dependent on 567 the density profile assumed for the contaminants distribution, 568 as can be seen in Fig. 8, where the upper limit at the 90% C.L. 569 for the rate in the DBD energy region (computed on^{226}Ra line) 570 is plotted in function of contamination depth. 571 Conclusions 572 The CUORE Crystal Validation Runs (CCVRs) have been 573 carried out since the end of 2008 at the Gran Sasso National 574 Laboratories, in order to test the performances and the ra- 575 diopurity of the TeO_2 crystals produced at SICCAS (Shanghai 576 Institute of Ceramics, Chinese Academy of Sciences) for the 577 CUORE experiment. 578 In this work the results of the first 5 validation runs, are pre- 579 sented. The items under analysis are the background rate, the 580 bulk and surface contamination from several nuclides and the 581 extrapolation to the CUORE background. 582 The CCVRs background rate shows a reduction with respect 583 to the one measured in CUORICINO in all the energy regions 584 considered. The bulk activity of^{210}Po is measured to be within 585 the limit specified in the contract with the crystals producer. 586 No indication of a bulk contamination from uranium and tho- 587 rium decay chains, as well as from^{210}Pb (out of equilibrium), is 588 found. The upper limits are calculated to be within the contract 589 specification. No indication of a surface contamination from 590 uranium and thorium decay chains, as well as from^{210}Pb (out 591 of equilibrium), is found. Upper limits at 90% C.L. are calcu- 592 lated for surface contamination from several nuclides and for 593 different contamination depths. 594 An extrapolation to CUORE background from both bulk and 595 surface contaminations is performed, in the most conservative 596 assumption that the CCVRs observed background is entirely 597 due to the bulk and the surface contamination respectively. 598 Considering only the contribution from bulk and surface crys- 599 tals contaminations, the following upper limits to the CUORE 600 background index in the energy region around the Q-value 601 of the neutrinoless double beta decay of^{130}Te are calculated: 602

1.1 · 10^{−4} counts/keV/kg/y and 5.5 · 10^{−3} counts/keV/kg/y re- 603 spectively. 604 References 605 [1] R. Ardito et al., arXiv:hep-ex/0501010. 606 [2] C. Arnaboldi et al., Nucl. Instr. Meth. A 518 (2004) 775. 607 [3] C. Arnaboldi et al., Journal of Crystal Growth 312 (2010) 2999. 608 [4] E.E. Haller et al., edited by R. D. Larrabee (Plenum Press, New York, 609 1984) 21. 610 [5] C. Arnaboldi et al., Phys. Rev. C 78 (2008) 035502. 611 [6] S. Pirro, Nucl. Instr. Meth. A 559 (2006) 672. 612 [7] E. Andreotti et al., Astr. Phys. 34 (2011) 822. 613 [8] E. Gatti and P.F. Manfredi, Rivista del Nuovo Cimento 9 (1986) 1. 614 [9] C. Bucci et al., Eur. Phys. J A 41 (2009) 155. 615 [10] M. Pavan et al., Eur. Phys. J A 36 (2008) 159. 616 [11] CUORE Coll. ”Three Tower Test: copper surface treatments for low back- 617 ground DBD experiments with TeO_2 bolometers.” Paper in preparation. 618 [12] K. Nakamura et al. (Particle Data Group), J. Phys. G 37, 075021 (2010) 619