arXiv:1502.06098v2 [math.OC] 1 Mar 2016

Contraction and incremental stability of switched Carathéodory systems using multiple norms ⋆

Wenlian Lu^a and Mario di Bernardo^b

aSchool of Mathematical Sciences and Centre for Computational Systems Biology, Fudan University, China

bDepartment of Electrical Engineering and Information Technology, University of Naples Federico II, Italy, Department of Engineering Mathematics, University of Bristol, U.K.

Abstract

In this paper, incremental exponential asymptotic stability of a class of switched Carathéodory nonlinear systems is studied based on the novel concept of measure of switched matrices via multiple norms and the transaction coefficients between these norms. This model is rather general and includes the case of staircase switching signals as a special case. Sufficient conditions are derived for incremental stability allowing for the system to be incrementally exponentially asymptotically stable even if some of its modes are unstable in some time periods. Numerical examples on switched linear systems switching periodically and on the synchronization of switched networks of nonlinear systems are used to illustrate the theoretical results.

Key words: Contraction; Incremental stability; Switched Carathéodory system; Synchronization.

1 Introduction

Studying incremental stability of nonlinear systems is particularly important in many application areas, including observer design and, more recently, consensus and synchronisation problems in network control where convergence analysis is a fundamental step (Wang & Slotine, 2005; Russo & di Bernardo, 2009a,b; Russo et al., 2010, 2011, 2013).

Since the early work by Lewis (1949); Demidovich (1967), contraction theory has been highlighted as a promising approach to study incremental exponential asymptotic stability (δEAS) of nonlinear systems (Lohmiller & Slotine, 1998; Forni & Sepulchre, 2014; Angeli, 2002); also see Jouffroy (2005) for an historical overview. In particular, as shown by Lohmiller & Slotine (1998), sufficient conditions for δEAS of a given nonlinear system over an invariant set of interest

⋆ This work is jointly supported by the National Natural Sciences

Foundation of China under Grant No. 61273309, the Program for New Century Excellent Talents in University (NCET-13-0139), the Key Laboratory of Nonlinear Science of Chinese Ministry of Education and the Shanghai Key Laboratory for Comtemporary Applied Mathematics, Fudan University.

Corresponding Author: W. L. Lu. Tel: +86-21-65643265. Fax: +86-21-65646073.

Email addresses: wenlian@fudan.edu.cn (Wenlian Lu),

mario.dibernardo@unina.it (Mario di Bernardo).

can be obtained by studying the matrix measure of its Jacobian induced by some vector norm. It is possible to prove, as done by Lohmiller & Slotine (1998); Russo et al. (2010), that if such measure is negative definite in that set for all time then any two trajectories will exponentially converge towards each other; the rate of convergence being estimated by the negative upper bound on the Jacobian measure.

Numerous applications of contraction analysis have been presented in the literature from observer design to the synthesis of network control systems. See e.g. Lohmiller & Slotine (1998); Forni & Sepulchre (2014); Russo et al. (2011). Remarkably, the problem of studying incremental stability of switched and hybrid systems has attracted relatively little attention despite the large number of potential applications, e.g. power electronic networks, variable structure systems, walking and hopping robots, to name just a few (di Bernardo et al., 2008; Liberzon, 2003; Cortes, 2008).

It has been suggested by Russo & di Bernardo (2011); di Bernardo et al. (2014) that extending contraction analysis to this class of systems can be a viable and effective approach to obtain conditions for their incremental asymptotic stability. Related approaches include the work on convergence of piecewise affine continuous systems presented by Pavlov et al. (2005b,a, 2007); Pavlov & van de Wouw (2008) and the recent conference papers (di Bernardo & Liuzza, 2013; di Bernardo & Fiore,

Preprint submitted to Automatica 12 August 2019

2014).

One limitation of the existing extensions of contraction theory to switched systems, (e.g. di Bernardo et al., 2014), is that they rely on the use of a unique matrix measure to assess the Jacobian of each system modes. This is a particularly restricting assumption as it would be desirable to use measures induced by different norms to evaluate the Jacobian of each of the system modes. This would correspond to studying incremental stability of the switched system with multiple incremental Lyapunov functions rather than using a common one (which is much harder to find).

The aim of this paper is to address this problem and present conditions for contraction and incremental stability of a large class of switched Carathéodory systems. The key idea is to define a novel concept of matrix measure via multiple norms and exploit the transaction coefficients between these norms. In so doing, sufficient conditions are derived for incremental stability that allow for a system to be δEAS even if some of its modes are unstable (or not contracting) over some time intervals. The theoretical results are illustrated via their applications to some representative examples, including synchronisation in blinking networks.

2 Preliminaries

We focus on switched dynamical systems of the form

ẋ = f(x, r(t)) (1)

where x ∈ R^n and the switching signal r(t) is assumed to be a real-valued piecewise continuous (PWC for short) function with respect to time: there exist countable discontinuous points t_0 < t_1 < · · · < t_i < · · · such that r(t_i±) exist and r(t_i) = r(t_i+) for all t_i. A typical example is the staircase function r(t) = ξ_i, for t_i ≤ t < t_{i+1}, i = 0, 1, · · · , for the increasing time sequence {t_j }_{j≥0}, which has been widely used as switching signal in control systems (Liberzon, 2003).

Here we make the following hypothesis:

H_1: For some C ⊂ R^n , the vector field f(x, r(t)) : C × R_{≥0} → R^n is (i) continuous with respect to (x, r); (ii) continuously differentiable with respect to x, and (iii) there exists a Lebesgue measurable function m(t) such that |f(x, r(t))| ≤ m(t) for all x ∈ C and t ∈ R_{≥0} .

It can be seen that under hypothesis H_1, and with r(t) defined as above, the vector field f(x, r(t)) defines a Carathéodory switched system (Filippov, 1988). It can be proved that, given an initial condition in C, a solution of a Carathédory system exists and is unique (Hale, 1954). We define ϕ(t; t_0, x_0, r_t) as the solution of (1) with x(t_0) = x_0 and the switching signal r(t), where r_t denotes the trajectory of r(t) up to t, i.e., r_t = {r(s)}_{t0 ≤s≤t}.

In this paper, | · |_χ stands for a specific vector norm in Euclidean space and the matrix norm induced by it, which can be defined in different ways that are all equivalent. The transaction coefficients from the norm | · |_a to | · |_b is defined as β_{ab} = sup_{|x|a=1} |x|_b (Bourbaki, 1978).

A continuous function α : [0, a) → [0, ∞) is said to belong to class K if (I) it is strictly increasing; (II) α(0) = 0. And, a continuous function β(ρ, t) : [0, a) × [0, ∞) → [0, ∞) is said to belong to class KL if (1) for each fixed t, the function β(ρ, t) belongs to class K; (2) for each fixed ρ, the function β(ρ, t) is decreasing with respect to t and lim_{t→∞} β(ρ, t) = 0. In addition, if a function β(ρ, t) of class KL converges to 0 exponentially as t → ∞, β(ρ, t) is said to be of class EKL. Here, we give the following definition of incremental stability from Angeli (2002) with modifications.

Definition 1 System (1) is said to be incrementally asymptotically stable (δAS for short) with r(t) in the region C ⊂ R^n if there exists a function β(s, t) of class KL such that for any initial data x_0, y_0 ∈ C and starting time t_0, the following property holds

|ϕ(t + t_0; t_0, x_0, r_t) − ϕ(t + t_0; t_0, y_0, r_t)| ≤ β(|x_0 − y_0|, t)

for some norm | · |. If β(s, t) is picked independently of the initial time t_0, then system (1) is said to be incrementally uniformly asymptotically stable (δUAS for short). If β(s, t) is of class EKL, then system (1) is said to be incrementally exponentially asymptotically stable (δEAS for short) and incrementally uniformly exponentially asymptotically stable (δUEAS for short) if β(s, t) is chosen independently of t_0.

Definition 2 A set C ⊂ R^n is said to be a κ-reachable set if there exists a continuously differentiable curve γ(s) : [0, 1] → C that links x_0 and y_0, i.e., γ(0) = x_0 and γ(1) = y_0, and satisfies |γ^′(s)|_{χ(t0 )} ≤ κ|x_0 − y_0|_{χ(t0 )}, for all s ∈ [0, 1] and some constant κ > 0, independently of x_0 and y_0.

3 Switched matrix measures and general contraction analysis

The matrix measure induced by the vector norm | · |_χ, where χ is the index for the norm being used, is defined as

μ_χ(A) = lim_{h→0+} 1 h [|(I_n + hA)|_χ − 1]

for a square matrix A ∈ R^{n,n} and was used for the contraction analysis of smooth nonlinear systems, see e.g. Lohmiller & Slotine (1998).

Given a PWC function χ(t), the left (right) limit of |·|_{χ(t)} at time t is defined as lim_{h→0−} |x|_{χ(t+h)} (lim_{h→0+} |x|_{χ(t+h)}) if it exists for all x ∈ R^n, and is denoted by | · |_{χ(t±)} respectively. We say that the switched norm | · |_{χ(t)} is continuous at time t if |x|_{χ(t−)} = |x|_{χ(t+)} = |x|_{χ(t)} for all x ∈ R^n , i.e.

if | · |_{χ(t)} is left and right continuous. We say that | · |_{χ(t)} is uniformly equivalent if there exists a constant D > 0 such that |x|_{χ(t)} ≤ D|x|_{χ(s)} for all x ∈ R^n and t, s ∈ R.

We can now extend the definition of matrix measure to the case of multiple norms, taking the time-varying nature of χ(t) into consideration, as follows.

Definition 3 The switched matrix measure with respect to multiple norms | · |_{χ(t)} is defined as

ν_{χ(t)}(A) = lim_{h→0+} 1 h sup |x|_{χ(t)}=1 [ |(I_n + hA)x|_{χ(t+h)} − 1 ] (2)

if the limit exists, where lim stands for the limit superior.

It can be seen that if χ(t) is constant over an interval, say [t, t + δ), then ν_{χ(t)}(A) = μ_{χ(t)}(A) over that interval.

The existence of the switched matrix measure is related to the partial differential of the switched norm | · |_{χ(t)} defined as follows

∂_t(| · |_{χ(t)}) = lim_{h→0+} sup_{|x|} χ(t)=1 |x|_{χ(t+h)} − 1 h .

We say that the multiple norm |·|_{χ(t)} is right regular at time t if ∂_t(| · |_{χ(t)}) exists. Thus, we have

Proposition 1 If | · |_{r(t)} is right regular at t, then (i). | · |_{χ(t)} is right continuous at t; (ii). ν_{χ(t)}(A) exists at t.

Proof The first statement is straightforward from the definitions of ∂_t(| · |_{χ(t)}) and right continuity of | · |_{χ(t)}.

The quotient term of the definition of ν_{χ(t)}(A) gives 1 h sup |x|_{χ(t)} =1 [ |(I_n + hA)x|_{χ(t+h)} − |(I_n + hA)x|_{χ(t)} +|(I_n + hA)x|_{χ(t)} − 1 ] ≤ 1 h sup |x|_{χ(t)} =1 [ |(I_n + hA)x|_{χ(t+h)} − |(I_n + hA)x|_{χ(t)} ]

+ 1 h sup |x|_{χ(t)}=1 [ |(I_n + hA)x|_{χ(t)} − 1 ]

≤ 1 h [ h∂_t(| · |_{χ(t)})|(I_n + hA)|_{χ(t)} + μ_{χ(t)}(A)h + o(h) ]

where o(h) is an infinitesimal term with lim_{h→0} o(h)/h = 0. So, ν_{χ(t)}(A) ≤ μ_{χ(t)}(A) + ∂_t(| · |_{χ(t)}) (statement (ii)).

Using the definition of switched matrix measure, we extend Coppel inequality (Coppel, 1965) as follows.

Lemma 1 Suppose that | · |_{χ(t)} is right-regular in [t_1, t_2]. Consider the following time-varying Carathéodory dynamical system ẋ(t) = A(t)x(t) with some PWC matrix-valued function A(t) ∈ R^{n,n} and x(t) ∈ R^n . If ν_{χ(t)}(A(t)) ≤ α(t) for some measurable function α(t) for t ∈ [t_1, t_2], then

|x(t_2)|_{χ(t2 )} ≤ exp (∫_{t2} t_1 α(t)dt ) |x(t_1)|_{χ(t1 )}. (3)

Proof For any t ∈ (t_1, t_2) except discontinuous points of A(t), consider the following quotient I(h) = 1 h [|x(t + h)|_{χ(t+h)} − |x(t)|_{χ(t)}] = 1 h [|x(t) + ∫_{t+h} t A(s)x(s)ds|_{χ(t+h)} − |x(t)|_{χ(t)}] = 1 h { |(I_n + hA(t))x(t) + ∫_{t+h} t [A(s)x(s) −A(t)x(t)]ds|_{χ(t+h)} − |x(t)|_{χ(t)} } ≤ 1 h [|(I_n + hA(t))x(t)|_{χ(t+h)} − |x(t)|_{χ(t)} + o(h)], which implies that lim_{h→0}I(h) ≤ ν_{χ(t)}(A(t))|x(t)|_{χ(t)} . That is, D^+|x(t)|_{χ(t)} ≤ ν_{χ(t)}(A(t))|x(t)|_{χ(t)} ≤ α(t)|x(t)|_{χ(t)} holds for almost every t ∈ [t_1, t_2], where D^+ stands for the Dini derivative. Thus, Ineq. (3) holds, noting that x(t) is continuous with respect to t.

We make the following hypothesis on the multiple norm.

H_2: | · |_{χ(t)} is right-regular everywhere but at the time instants {t̃_j }, it is right-continuous and uniformly equivalent, and its left-limit exists at each t̃_j .

Thus, we denote by Ñ(t, s) = #{i : s < t̃_i < t}, the number of time instants t̃_i in the time interval (s, t); obviously, Ñ(t) = Ñ(t, t_0). Here, # stands for the cardinality of a set. In addition, we make the following assumption.

H_3: There exists a κ-reachable set (Russo et al., 2010) C ⊂ R^n which is a forward-invariant for (1).

Then, we have a general result on δEAS of switched dynamical system (1) by contraction analysis in multiple norms.

Theorem 1 Suppose that hypotheses H_{1,2,3} hold and that r(t) is PWC. If there exist a measurable function α(t), nonnegative constants β_j , j = 1, 2, · · · , c > 0, and T_0 > 0, such that, for all x ∈ C, the following conditions hold ν_{χ(t)} ( ∂f ∂x (x, r(t)) ) ≤ α(t), ∀ t ≠ t̃_j , x ∈ C (4) | · |_{χ(t̃j )} ≤ β_j | · |_{χ(t̃j −)}, ∀ j (5) and, for all T > T_0, 1 T ∫_{T +t0} t_0 α(t)dt + Ñ(t_0 +T ) ∑ j=1 log(β_j ) < −c, (6)

then system (1) is δEAS in C with respect to r(t); if (6) holds for some c > 0 independent of t_0, then (1) is δEUAS with respect to r(t) in C. In addition, the exponential convergence rate can be estimated as O(exp(−c(t − t_0))).

Proof For any x_0, y_0 ∈ C, C being κ-reachable for some κ > 0 implies, from Definition 2, that there exists a continuously differentiable curve γ(s) : [0, 1] → C such that γ(0) = x_0 and γ(1) = y_0, and |γ^′(s)|_{χ(t0 )} ≤ κ|x_0 − y_0|_{χ(t0 )}, for all s ∈ [0, 1].

Let ψ(t, s) = ϕ(t; t_0, γ(s), r_t), s ∈ [0, 1], be the solution of (1) with initial value ψ(t_0, s) = γ(s). Since f(x, r(t)) is continuous with respect to (x, t) except for the switching time points {t_j } and continuously differentiable with respect to x, then ϕ(t; t_0, x_0, r_t) is continuously differentiable with respect to the initial value x_0. Let x_0 = γ(s). Then, w = ∂ψ ∂s is well defined and continuous. By the same algebraic manipulations first presented by Russo et al. (2010), except for {t_j }, w(t, s) is the Carathéodory solution of: { ẇ =^{∂f}_{∂ψ} (ψ(t), r(t))w w(t_0, s) = γ^′(s) (7)

Consider the sequence |w(t̃_j , s)|_{χ(t̃j )} of Eq. (7). For all s ∈ [0, 1], by the extended Coppel inequality (3) and condition (4), we have

|w(t̃_j , s)|_{χ(t̃j −)} ≤ exp [∫_{t̃i} t̃_{j−1} α(t)dt ] |w(t̃_{j−1}, s)|_{χ(t̃j−1 )}.

Using inequality (5) between | · |_{χ(t̃j−1 )} and | · |_{χ(t̃j )}, gives |w(t̃_j , s)|_{χ(t̃j )} ≤ β_j |w(t̃_j , s)|_{χ(t̃j −)} ≤ β_j exp [∫_{t̃i} t̃_{j−1} α(t)dt ] |w(t̃_{j−1}, s)|_{χ(t̃j−1 )}

Then, iterating down to i < j, we have

|w(t̃_j , s)|_{χ(t̃j )} ≤ j∏ k=i+1 β_k exp [∫_{t̃i} t̃_i α(t)dt ] |w(t̃_i, s)|_{χ(t̃i )}.

For any t, noting that from definition t̃_{Ñ(t)+1} ≥ t > t̃_{Ñ(t)}, we have

|w(t, s)|_{χ(t)} ≤ exp [∫_t t̃_{Ñ (t)} α(τ)dτ ] |w(t̃_{Ñ (t)}, s)|_{χ(t̃Ñ (t) )}

≤ exp [∫_t t̃_{Ñ(t)} α(τ)dτ ] · exp Ñ(t)∑

i=1 log β_i

+ ∫_{t̃Ñ(t)} t_0 α(τ)dτ ) |w(t_0, s)|_{χ(t0 )}.

Hence, we obtain |w(t, s)|_{χ(t)} ≤ exp(−c(t − t_0))|γ^′(s)|_{χ(t0 )}, (8) for all t > t_0 + T_0. Since c is independent of s, δEAS can be derived by following similar arguments as presented by Russo et al. (2010). In detail, since | · |_{χ(t)} is uniformly equivalent, there exists D > 0 such that |x|_{χ(t)} ≤ D|x|_{χ(t}′_) for any x ∈ R^n and t, t^′ ≥ t_0. Then, by (8), we have

|ϕ(t; x(0), r_t) − ϕ(t; y(0), r_t)|_{χ(t0 )} (9) ≤ D|ϕ(t; x(0), r_t) − ϕ(t; y(0), r_t)|_{χ(t)} = D | | | ∫_1 0 ∂ψ(t, s) ∂s ds | | | χ(t) ≤ D ∫_1 0 |w(t, s)|_{χ(t)}ds ≤ D ∫_1 0 exp(−c(t − t_0))|γ^′(s)|_{χ(t0 )}ds = Dκ exp(−c(t − t_0))|x_0 − y_0|_{χ(t0 )} (10)

which converges to zero exponentially. This proves that system (1) is δEAS.

If (6) holds for some c > 0 independently of t_0, then (8) holds independently of t_0 if t − t_0 > T_0, which implies lim_{t→∞} |w(t)|_{χ(t0 )} = 0 is uniform with respect to t_0. By the arguments above, system (1) is δUEAS. In addition, inequality (10) implies that the exponential convergence rate can be estimated as O(exp(−c(t − t_0))).

Note that c is an estimate of the exponential convergence rate and also an index of the average contraction rate of (1).

As a simple example to illustrate this result, define a switched matrix measure based on the following multiple norms: |x|_{P (t)} = √ x^⊤P (t)x. Here, P (t) ∈ R^{n,n} is a differentiable matrix-value function where each P (t) is a symmetric positive definite matrix such that its largest eigenvalue λ_{max}(P (t)) the smallest eigenvalue λ_{min}(P (t)) is upper bounded and lower-bounded positive respectively. Then, for any A ∈ R^{n,n} , by simple algebraic manipulations, it can be shown that the induced switched matrix measure is ν_{P (t)}(A) = 1 2 λ_{max}[P^{−1/2}(t)(P (t)A + A^⊤P (t) + Ṗ (t))P^{−1/2}(t)].

Now, consider the linear time-varying (LTV) system ẋ = A(t)x + I(t) with some PWC matrix function A(t). Then, (6) in Theorem 1 can be fulfilled by assuming that it holds that P (t)A(t) + A(t)^⊤P (t) + Ṗ (t) < 0 for almost every t. A similar condition can also be obtained by using the theory of convergent systems (Pavlov et al., 2007).

Remark 1 Analogous arguments to those presented by Lohmiller & Slotine (1998) and Russo et al. (2010) can be followed to prove that the contracting system converges towards a periodic solution if r(t) is periodic. Indeed, in this case the time instants where r(t) switches, say {t_j }, are also periodic with period T and so is the function N(t, s) = N(t + T, s + T ) for all t > s. Then, inequality (6) can be fulfilled by assuming that

1 T ∫_{T +t0} t_0 α(t)dt + J∑ j=1 log(β_j ) < −c. (11)

where J is the number of switches in one period. (Note that this inequality holds independently of the initial time t_0, due to the periodicity.) From Theorem 1, one can conclude that system (1) is δEAS. The existence of a periodic solution of (1) follows by using the contraction mapping theorem.

4 Contraction analysis of staircase switching and transaction coefficients between norms

As a special case and an important application, in this section, we assume that the switching signal r(t) of the switched system (1) is a staircase function:

H_4: r(t) = ξ_i, t_i ≤ t < t_{i+1}, i = 0, 1, · · · , with an increasing time point sequence {t_i} with t_i = 0 and lim_{i→∞} t_i = ∞, where ξ_i ∈ Ξ where Ξ is a countable set.

Let Δ_i = t_{i+1} − t_i > 0 be the interval between two points, and N(t, s) = #{i : s < t_i < t}, be the number of time instants when r(t) switches that fall in the time interval [s, t], in particular, N(t) = N(t, t_0).

By using multiple norms |·|_{χ(t)} with χ(t) = r(t), we obtain the following result as a consequence of Theorem 1.

Corollary 1 Suppose that hypotheses H_{1,2,3,4} hold. If there exists constants α_i, nonnegative constants β_i, i = 1, 2, · · · , c > 0 and T_0 > 0 such that, for all i and x ∈ C, the following conditions hold

μ_{ξj} ( ∂f ∂x (x, ξ_j ) ) ≤ α_j , | · |_{ξj+1} ≤ β_j | · |_{ξj} , ∀ j (12) and, for all T > T_0, 1 T { N(t_0+T ) ∑ i=0 [α_iΔ_i + log(β_i)]

+α_{N(t0+T )+1}[t_0 + T − t_{N(t0+T )}] } < −c, (13) then (1) is δEAS with respect to r(t) in C; if (13) holds for some c > 0 independently of t_0, then (1) is δUEAS with respect to r(t) in C. Moreover, the exponential convergence rate is estimated as O(exp(−c(t − t_0))).

Proof Let α(t) = α_i if t ∈ [t_i, t_{i+1}). We have ν_{r(t)} ( ∂f ∂x (x, ξ_i) ) = μ_{r(t)} ( ∂f ∂x (x, ξ_i) ) ≤ α(t), ∀ t ≠ t_i. Note that 1 T ∫_T t_0 α(t)dt = 1 T [ α_{N(t0 +T )+1}(t_0 + T − t_{N(t0 +T )}) + α_0Δ_0

+ N(t_0+T ) ∑ i=0 α_iΔ_i ] .

Under condition (13), one can conclude that there exists T_1 > 0 such that 1 T ∫_{t0+T} t_0 α(t)dt + N(t_0+T ) ∑ i=0 β_i < −c (14)

for all T > T_1. By employing Theorem 1, δEAS of (1) can be proved. Furthermore, if (13) holds independently of the initial time t_0, and therefore (14) holds independently of t_0, then (1) is δUEAS with respect to r(t) in C. The exponential convergence rate can be derived as done in the proof of Theorem 1.

We can exploit Corollary 1 when considering the case where r(t) (ξ_i) takes values in a finite set Ω = {1, · · · , K}. Specifically, define for any t > s ≥ 0 T_k(s, t) = {τ ∈ [s, t] : r(τ) = k}, N_{kl}(s, t) = #{i : r(t_i−) = k, and r(t_i+) = l, s ≤ t_i ≤ t}, and constants α_k and β_{kl} > 0, k, l = 1, · · · , K such that μ_k ( ∂f ∂x (x, k) ) ≤ α_k, | · |_l ≤ β_{kl}| · |_k. (15) Then letting α(t) = α_i when t ∈ [t_i, t_{i+1}), it can be seen that inequality (13) in Corollary 1 can be derived if the following condition holds for all T > T_0: 1 T K∑ k=1 [ α_kT_k (t_0, t_0 + T ) + K∑ l=1 log(β_{kl})N_{kl} (t_0, t_0 + T ) ]

≤ −c. (16) Alternatively, condition (16) can be replaced by the assumption that there exists some T_1 > 0 such that for each T_1- length interval, [nT_1, (n + 1)T_1], it holds that 1 T_1 K∑ k=1 [ α_kT_k (nT_1, (n + 1)T_1) + K∑ l=1 log(β_{kl})N_{kl} (nT_1, (n + 1)T_1) ] ≤ −c, ∀ n ≥ 0. (17)

Remark 2 From Ineq. (17), in the case that all α_k < 0, k = 1, · · · , K, which implies that all subsystems are contracting and hence incrementally stable, the switched system is incrementally stable if the duration of the mode in which each subsystem is active is sufficiently long.

More specifically, if all norms |·|_k are identical – and simply denoted by | · | – then β_{kl} = 1, and inequality (13) can be fulfilled by simply assuming that (1/T ) ∑_K k=1 α_kT (t, t + T ) ≤ −c holds for all t > 0. Thus, one can see that if α_k < 0 holds for all k = 1, · · · , K (with respect to the same norm), then (1) is incrementally stable, which coincides with the results by Russo & di Bernardo (2011).

The conditions of Theorem 1 and Corollary 1 as well as (16) depend on two quantities: the matrix measures α_k of the Jacobian of the dynamical system for each constant value of r(t), and the transaction coefficients β_{kl} between norms. As system (1) is defined in a finite dimensional Euclidean space, these vector norms are equivalent, i.e., there exist positive constants β_{kl} such that |x|_l ≤ β_{kl}|x|_k holds for all x ∈ R^n . The role of such transaction coefficients will be further investigated below.

For illustration, consider the LTV system

ẋ(t) = A(r(t))x(t) + B (18)

where r(t) : [0, ∞[→ C ≡ {1, 2} with A = A(1) or A(2) and B ∈ R^2 . We assume that the linear system is switched between two constant matrices periodically with identical frequency φ_r. Consider two vector norms |·|_{1,2}, corresponding to matrix measures μ_{1,2} respectively, with transaction coefficients β_{12} and β_{21}. Corollary 1, specifically condition (17), yields that the following inequality is a sufficient conditions for δUEAS of system (18): 1 2 [μ_1(A(1)) + μ_2(A(2)) + φ_r · (log β_{12} + log β_{21})] < −c (19) for some c > 0.

We now discuss the relationship between different classes of vector norms in greater detail.

Quadratic norms. The quadratic norm is defined as |x|_P = √ x^⊤P x for some positive definite matrix P . For another |x|_Q = √ x^⊤Qx with symmetric positive definite matrix Q.

Then, we have |x|_Q ≤ √ λ_{max}(P^{−1/2}QP^{−1/2})|x|_P (20)

for all x ∈ R^n , where λ_{max}(A) denotes the largest eigenvalue of a symmetric square matrix A. The proof of this statement is straightforward and omitted here for the sake of brevity.

A a first example, we take A(1) = ( 0 −1

2 −3 ) , A(2) = ( 0 −11

2 −33 ) . It is easy to see that, using the matrix mea-

sures μ_i(·) induced by the quadratic weighted vector norm |x|_{Θi} := |Θ_ix|_2, i = 1, 2 respectively, the matrix measures μ_i [A(i)] with

Θ_1 = ( 0.707 0.447

0.707 0.894 )−1 , Θ_2 = ( 0.998 0.322

0.0618 0.947 )−1

are negative for i = 1 and i = 2. In particular, μ_1 [A(1)] ≤ −1 := α_1 and μ_2 [A(t, 2)] ≤ −0.6807 := α_2.

From the results reported in Sec. 2, we get from Ineq. (20) that: |x|_{Θ1} ≤ 1.796|x|_{Θ2} and |x|_{Θ2} ≤ 1.05|x|_{Θ1} ; therefore condition (5) remains satisfied with β_{12} := 1.796 and β_{21} := 1.05. Assuming a switching frequency of φ_r = 1 Hz between the two modes, we have Δ_i = 1 s for all i. Therefore (19) is satisfied and (18) is incrementally stable in R^2 .

The evolution of the norm of the error for two trajectories starting at initial conditions [0.5, 0.1] and [0.4, 0.1] respectively is shown in Fig. 1 when B = [0 0] and B = [1 1] respectively. In both cases we observe incremental stability as expected. Note that the use of two different weighted norms makes proving incremental stability much simpler than if one common metric had to be used for both modes as required by previous results (e.g. Russo & di Bernardo, 2011; di Bernardo et al., 2014).

Next, we take A(1) = ( −1.3481 −2.9306

−2.4538 −1.2755 ) , A(2) = ( −11.2237 7.0628

−1.7413 1.5119 ) . It can be seen that A(1) is Huwitz

Fig. 1. Evolution of the Euclidean norm of the error ‖x(t) − y(t)‖ when B = [0 0]^⊤ (top panel) and B = [1 1]^⊤ (bottom panel).

Fig. 2. Dynamics of the average error Err(t) over M = 10 independent realizations of random initial values that are picked from [−10, 10]^2 following the uniform distribution. Err(t) =^1_M ∑_M q=1 √ (x^q_1 − x̄1)^2 + (x^q_2 − x̄2)^2 with x̄u = (1/M) ∑_M q=1 x^q_u with u = 1, 2, where x^q_{1,2} stands for the state components of the m-th realization.

stable i.e., with all eigenvalues having negative real parts, but A(2) is unstable, i.e., with some eigenvalues possessing positive real parts. Choosing Θ_{1,2} as follows:

Θ_1 = ( 0.3797 0.0061

0.0061 0.4534 ) , Θ_2 = ( 0.0644 −0.1475

−0.1475 0.8267 ) .

we find that the matrix measures, μ_1(A(1)) and μ_2(A(2)), induced by the 2-norms | · |_{Θ1} and | · |_{Θ2} are: μ_1(A(1)) = −2.6178, μ_2(A(2)) = 0.9188. The transaction coefficients between the two norms | · |_{Θ1,2} can be calculated by (20) as | · |_{Θ1} ≤ β_{12}| · |_{Θ2} and | · |_{Θ2} ≤ β_{21}| · |_{Θ1} with β_{12} = 1.9079 and β_{21} = 10.4207. The LTV system switches between these two modes with an identical frequency φ_r (φ_r = 0.25 Hz in this example). Then (19) holds for c = 1.1010. Therefore, the LTV system (18) is δUEAS, as shown in Fig. 2, despite one of its modes being unstable.

Note A_m =^{A(1)+A(2)}_2 = ( −6.2859 2.0661

0.3562 0.1182 ) , which is un-

stable as it has eigenvalues of −6.3988 and 0.2311. Hence, the results presented by Porfiri et al. (2008) cannot be applied for this specific situation. Nevertheless our extension of contraction analysis to switched systems gives a simple and viable set of conditions that can be used to prove that indeed the system is incrementally stable.

More specifically, from the properties of matrix measures,

1/2(μ(A(1)) + μ(A(2))) ≥ μ(A_m) ≥ max{R⌉(λ) : λ ∈ σ((A_m))} > 0 it is not possible to find a uniform norm such that the average of the matrix measures of the switched matrices induced by this matrix norm is negative as required by condition (19). Therefore, in this case, multiple norms must be utilised for proving contraction and δEAS of the system.

Weighted L_p-norms. The weighted L_p-type norms with 1 ≤ p ≤ ∞ are defined as follows.

• Weighted L_p-norm: |x|_{ξ,p} = ( ∑_n i=1 ξ_i|x_i|^p)^{1/p} for some p ≥ 1 and ξ = [ξ_1, · · · , ξ_n]^⊤ with ξ_i > 0 for all i = 1, · · · , n; • Weighted L_∞-norm: |x|_{ξ,∞} = max_i ξ_i|x_i| for some ξ = [ξ_1, · · · , ξ_n]^⊤ with ξ_i > 0 for all i = 1, · · · , n.

Their transaction coefficients are summarised by the following proposition.

Proposition 2 For p > q ≥ 1 with p possibly equal to ∞ and two component-wise vectors ξ = [ξ_1, · · · , ξ_n]^⊤ and η = [η_1, · · · , η_n]^⊤ with ξ_i, η_i > 0 for all i = 1, · · · , n, the following hold: (1) |x|_{p,ξ} ≤ max_i^{ξ1/pi}_{η1/qi} |x|_{q,η} ; (2) |x|_{q,η} ≤ max_i^{η1/qi}_{ξ1/pi} (n^{1/q} − n^{1/p})|x|_{p,ξ} ; (3) |x|_{2,ξ} = |x|_Ξ with Ξ =

diag[ξ_1, · · · , ξ_n].

This result can be directly derived from Bourbaki (1978). Combining 20 and Proposition 2, we can derive all transaction coefficients between all quadratic norms, | · |_Q with positive definite matrix Q, and all | · |_{ξ,p} for +∞ ≥ p ≥ 1. The same transaction coefficients hold for the equivalence between the matrix norms induced by these vector norms.

Structured vector norm. We define a structured vector norm, following the approach presented in Russo et al. (2013). Specifically, assume x = [x_1, · · · , x_n]^⊤ ∈ R^n can be partitioned into K vectors x^k ∈ R^{nk} , k = 1, · · · , K, such that x = [x^{k⊤}, · · · , x^{K ⊤}]^⊤ with ∑_K k=1 n_k = n. Let |x^k|_{sk} be the norm in R^{nk} . Then, the structured norm of x is denoted by | · |_G and defined as: |x|_G = | |[|x^1|_{s1} , · · · , |x^K |_{sk} ]^⊤ | |_S (21)

where the norm | · |_S is defined in R^K .

Given the same partition of x^k, k = 1, · · · , K, consider another structured norm | · |_G′ based on using the vector norms | · |_s′_k in R^{nk} , k = 1, · · · , K, and | · |_S′ in R^K such

that |x|_G′ = | |[|x^1|_s^′_1 , · · · , |x^K |_s^′_k ]^⊤ | |_{S′} . Proposition 3 Let | · |_G and | · |_G′ be two structured norms defined as mentioned above. Let τ_S be the transaction coefficient from the norm | · |_S′ to | · |_S and τ_k be the the transaction coefficient from the norm | · |_s′_k to | · |_{sk} . Then, we have |x|_G′ ≤ τ_S |U|_S |x|_G with U = diag[τ_k]^K_{k=1}. This result can be derived as a consequence of those presented by Russo et al. (2013).

Russo et al. (2013) showed that contraction analysis can be used to carry out the hierarchical analysis and design of networked systems. Analogously, consider system (18). Partition x into several sub-vectors, K vectors: x^k ∈ R^{nk} , k = 1, · · · , K, so that x = [x^{k ⊤}, · · · , x^{K ⊤}]^⊤ with ∑_K k=1 n_k = n. Each x^k corresponds to the k-th subsystem. Then, system (18) can be equivalently written in the following form:

ẋ^k = K∑ k^′ =1 A_{kk}′ (t)x^k + B^k, k = 1, · · · , K, (22)

where

A(r) = A_{11}(r) A_{12}(r) · · · A_{1K} (r)

A_{21}(r) A_{22}(r) · · · A_{2K} (r) . . . . · · · . . A_{K1}(r) A_{K2}(r) · · · A_{KK} (r) , r = 1, 2,

and [B^⊤_1 , · · · , B^K ]^⊤ = B.

The norm of x is defined by (21). Let Ã_{ij} (t) = |A_{ij} (t)|_{ij} , where the norm | · |_{ij} is defined by |A_{ij} (r)|_{ij} = sup_{|xj |s} j =1 |A_{ij} (r)x^j |_{si} .

and consider the reduced K × K matrix

Ã(r) =

Ã_{11}(r) Ã_{12}(r) · · · Ã_{1K} (t)

Ã_{21}(r) Ã_{22}(r) · · · Ã_{2K} (r) . . . . · · · . . Ã_{K1}(r) Ã_{K2}(r) · · · Ã_{KK} (r) , r = 1, 2.

Let | · |_{S,1} and | · |_{S,2} be two norms in R^K and β^′_{12} and β^′_{21} be their transaction coefficients such that | · |_{S,1} ≤ β^′_{12}| · |_{S,2} and | · |_{S,2} ≤ β^′_{21}| · |_{S,1}. We take the multiple norms in R^n as |·|_{G,r} = |Ã(r)|_{S,r}, r = 1, 2. Let μ_{G,r} be the matrix measure induced by the vector norm | · |_{G,r} in R^n and μ_{S,r} be that of | · |_{S,r} in R^K . Then, it can be derived that μ_{G,r}(A(r)) ≤ μ_{S,r}(Ã(r)) (Russo et al., 2013). Proposition 3 implies that β^′_{12} and β^′_{21} can be the transactions coefficients between | · |_{G,1} and | · |_{G,2} as well.

Therefore, suppose that switched system (18) is in the block-wise form (22). Then, Corollary 1, specifically inequality (19), can be fulfilled assuming that it holds that (1/2) [ μ_{S,1}(Ã(1)) + μ_{S,2}(Ã(2)) + fr · (log β^′_{12} + log β^′_{21}) ] < −c. 5 Synchronization in switched networks

Finally, we consider a network example inspired from one first presented in di Bernardo et al. (2014). We assume the network equation is given by

ẋ^i = f(x^i(t)) − kσ(t) m∑ j=1 L_{ij} Γx^j (t), i = 1, · · · , m. (23)

Here, x^i ∈ R^n stands for the state vector at node i, f(·) : R^n → R^n the node dynamics, k is the coupling strength, L = [L_{ij} ]^m_{i,j=1} is the Laplacian matrix associated with a graph G = [V, E], where V = {1, · · · , m} is the node set and E the link set, by the way that for each (i, j), L_{ij} takes value −1 if there is a link from node j to i and 0 otherwise, and L_{ii} = − ∑_m j=1 L_{ij} . σ(t) takes values 0 or 1, implying that the diffusive coupling among the nodes in the graph G is only active when σ(t) = 1 while it is not present when σ(t) = 0. Γ ∈ R^{n,n} stands for the inner coupling matrix. We can rewrite (23) in compact form as:

ẋ = F (x(t)) − k [σ(t)L ⊗ Γ] x(t) (24)

where x = [x^{1⊤}, · · · , x^{m⊤}]^⊤ ∈ R^{mn} , F (x) = [f^⊤(x^1), · · · , f^⊤(x^m)]^⊤ and ⊗ is the Kronecker product. Assume that L is diagonalisable, i.e., there exists a nonsingular Q ∈ R^{m,m} such that L = Q^{−1}JQ with a diagonal matrix J = diag[λ_j ]^m_{j=1}, where λ_j , j = 1, · · · , m, are the eigenvalues of J, which are assumed to be real. Without loss of generality, we can assume that 0 = λ_1 ≥ λ_2 ≥ · · · ≥ λ_m. Note that λ_1 = 0 is associated with the synchronization eigenvector [1, · · · , 1]^⊤.

Following similar arguments to those by Carroll & Pecora (1991); Russo & di Bernardo (2011); di Bernardo et al. (2014); Yi et al. (2013), synchronization of network (24) can be achieved if the following linear systems (obtained via linearisation and block diagonalization of (24)): ϕ̇ = [Df(w(t)) − kλ_iσ(t)]ϕ, i = 2, · · · , m, (25) are contracting, where w(t) is a solution of the uncoupled system

ẇ = f(w), (26)

and Df(·) is the Jacobian of f(·). Assume

H_5: System (26) has an asymptotically stable attractor A (see Yi et al., 2013, Assumption 2).

Definition 4 System (23) is said to synchronize if there exists δ > 0 such that for any x^i(t_0) ∈ B(A, δ), lim_{t→∞} |x^i(t) − x^j (t)| = 0 for all i, j = 1, · · · , m. Here, B(A, δ) = {y : inf_{z∈A} |y − z| ≤ δ} denotes δneighbourhood of set A.

According to Corollary 1, in particular, equation (16), we have the following result:

Proposition 4 Consider two vector norms | · |_0 and | · |_1, which induce two matrix measures μ_0(·) and μ_1(·) respectively. Suppose that H_4 holds and μ_1(−Γ) ≤ 0. If there exist T_0 > 0 and c > 0 such that 1 T [ μ_0(Df(w))T_0(nT, (n + 1)T )

+μ_1(Df(w) − kλ_2Γ)T_1(nT, (n + 1)T ) +N_{01}(nT, (n + 1)T ) log β_{01}

+N_{01}(nT, (n + 1)T ) log β_{10} ] < −c (27)

holds for all T > T_0 and w ∈ A, where T_u(s, t) stands for the duration of σ(t) = u in the time interval (s, t] and N_{uv} (s, t) is the number of switches from σ(t) = u to σ(t) = v, for all u ≠ v, u, v = 0, 1, then system (24) synchronises.

Proof Note that for each i = 2, · · · , m, μ_1(Df(w) − kλ_iΓ) ≤ μ_1(Df(w) − kλ_2Γ) + k(λ_i − λ_2)μ_1(−Γ) ≤ μ_1(Df(w) − kλ_2Γ). Due to μ_1(−Γ) ≤ 0, then (27) holds for all i = 2, · · · , m. It can then be proved in a straightforward manner that the variational equations (25) are asymptotically stable for all i ≥ 2 by verifying condition (16) and following the same steps of the proof of Theorem 5.1 in di Bernardo et al. (2014). Thus, following the arguments in the proof of Theorem 17 in Yi et al. (2013), there is an invariant open convex set U ∈ R^{mn,mn} such that U ⊃ S, where S = {x = [x^{1⊤}, · · · , x^{m⊤}]^⊤ : x^i = x^j ∈ A, ∀ i, j}, is invariant for the coupled system (24). Furthermore, S is an asymptotically stable set for system (24). This proves synchronization.

Fig. 3. The underlying graph topology.

Fig. 4. Synchronisation dynamics of the network system (24) with random initial values that are picked from [−1, 1]^2,

i = 1, 2, · · · , 10. Here, Err(t) =^1_m ∑_m i=1 √∑_3 j=1(x^i_j − x̄j )^2

with x̄j = (1/m) ∑_m i=1 x^i_j .

To illustrate this result, we take

f(w) = p{G[−w_1 + w_2] − g(w_1)} G[w_1 − w_2] + w_3 −qw_2, where g(w_1) = m_0w_1 +1/2(m_1 −m_0)(|w_1 +1|−|w_1 −1|) as the Chua’ circuit with m_0 = −0.5, m_1 = −0.8, G = 0.7, p = 9 and q = 7, which was reported to exhibit a double-scroll chaotic attractor for the node dynamics (26) Matsumoto et al. (1985). Moreover, we take Γ as the identity matrix, and assume the underlining graph of 10 nodes has the structure shown in Fig. 3, associated with a Laplacian L with λ_2(L) = 2.7142. To study convergence, we choose weighted 1-norms: |y|_0 = |y_1| + r_2|y_2| + r_3|y_3|, with r_2 = 3.4042 and r_3 = 1.0369, and |y|_1 = √ |y_1|^2 + |y_2|^2 + |y_3|^2, which implies (i) β_{01} = 4.3163 and β_{10} = 1; (ii) μ_0(Df(w)) ≤ 3.2829 for all t. We take k = 1, so that μ_1(Df(w) − kλ_2(L)Γ) ≤ −7.4714, for all t. The switching signal σ(t) is taken as follows: σ(t) = { 0 t ∈ [kT, kT + 1/4T ) 1 t ∈ (kT + 1/4T, (k + 1)T )

for some T > 0. Condition (27) in Proposition 4 implies that if T > 13.08, then system (24) synchronises. To illustrate this result, we take T = 14. Fig. 4 shows that, as expected, all nodes synchronise.

6 Conclusions

We have presented an extension of contraction analysis to switched Carathéodory systems. The key step was the definition of switched matrix measures induced by multiple norms. Using these measures, it was possible to derive different sets of sufficient conditions for asymptotic incremental stability of the systems of interest. Most notably, it was possible to prove contraction and hence incremental stability by using different norms, each associated to a different mode of the switched system under investigation. This complements and extends in a highly nontrivial manner to the case of multiple norms, previous results presented by some of the authors (see Russo et al., 2013; di Bernardo et al., 2014), where contraction was studied by using a common metric. The theoretical results were illustrated on a set of representative examples and applications showing the effectiveness of the proposed method.

References

Angeli, D. (2002). A Lyapunov approach to incremental stability properties. IEEE Transactions on Automatic Control, 47, 410–421.

di Bernardo, M., Budd, C., Champneys, A., & Kowalczyk, P. (2008). Piecewise Smooth Dynamical Systems: Theory and Applications. Springer-Verlag (London).

di Bernardo, M., & Fiore, D. (2014). Incremental stability of bimodal filippov systems in r^n. In Proc. IEEE Conference on Decision and Control (pp. 4679–4684).

di Bernardo, M., & Liuzza, D. (2013). A criterion for incremental stability of planar filippov systems. In Proceedings of the European Control Conference (pp. 3706–3711).

di Bernardo, M., Liuzza, D., & Russo, G. (2014). Contraction analysis for a class of nondifferentiable systems with applications to stability and network synchronization. SIAM Journal on Control and Optimization, 52, 3203–3227.

Bourbaki, N. (1978). Topological Vector Spaces. Spriger- Verlag.

Carroll, T. L., & Pecora, L. M. (1991). Synchronizing chaotic circuits. IEEE Transactions on Circuits and Systems, 38, 453–456.

Coppel, W. (1965). Stability and asymptotic behavior of differential equations. Boston, Mass.: D.C. Heath.

Cortes, J. (2008). Discontinuous dynamical systems. IEEE Control Systems Magazine, 28, 36–73.

Demidovich, B. P. (1967). Lectures on Stability Theory.

Nauka Moscow.

Filippov, A. (1988). Differential equations with discontinuous righthand sides. Kluwer.

Forni, F., & Sepulchre, R. (2014). A differential lyapunov framework for contraction analysis. IEEE Transactions on Automatic Control, 59, 614–628.

Hale, J. (1954). Ordinary Differential Equations. New York:

John Wiley.

Jouffroy, J. (2005). Some ancestors of contraction analysis.

In Proceedings of the International Conference on Decision and Control.

Lewis, D. C. (1949). Metric properties of differential equations. American Journal of Mathematics, 71, 294–312.

Liberzon, D. (2003). Switching in Systems and Control.

Birkhauser (Berlin).

Lohmiller, W., & Slotine, J. J. E. (1998). On contraction analysis for non-linear systems. Automatica, 34, 683–696.

Matsumoto, T., Chua, L. O., & Komoru, M. (1985). The double scroll. IEEE Transactions on Circuits and Systems, 32, 798–818.

Pavlov, A., Pogromsky, A., von de Wouw, N., Nijmeijer, H., & Rooda, K. (2005a). Convergent piecewise affine systems: anaysis and design part 2: discontinuous case. In Proceedings of the Conference Decision and Control (pp. 5391 – 5396).

Pavlov, A., Pogromsky, N., van de Wouw, N., & Nijmeier, H. (2007). On convergence properties of piecewise affine systems. International Journal of Control, 80, 1233–1247.

Pavlov, A., & van de Wouw, N. (2008). Convergent discretetime nonlinear systems: the case of PWA systems. In Proc. American Control Conference.

Pavlov, A., van de Wouw, N., & Nijmeier, H. (2005b). Convergent piecewise affine systems: analysis and design - part i: continuous case. In Proceedings of the Conference Decision and Control.

Porfiri, M., Robertson, D. G., & Stilwell, D. J. (2008). Fast switching analysis of linear switched systems using exponential splitting. SIAM Journal on Control and Optimization, 47, 2582–2597.

Russo, G., & di Bernardo, M. (2009a). Contraction theory and the master stability function: linking two approaches to study synchronization in complex networks. IEEE Transactions on Circuit and Systems II, 56, 177–181.

Russo, G., & di Bernardo, M. (2009b). How to synchronize biological clocks. Journal of Computationa Biology, 16, 379–393.

Russo, G., & di Bernardo, M. (2011). On contraction of piecewise smooth dynamical systems. In Proceedings of IFAC World Congress.

Russo, G., di Bernardo, M., & Slotine, J. (2011). A graphical algorithm to prove contraction of nonlinear circuits and systems. IEEE Transactions on Circuits And Systems I, 58, 336–348.

Russo, G., di Bernardo, M., & Sontag, E. (2013). A contraction approach to the hierarchical analysis and design of networked systems. IEEE Transactions on Automatic Control, 58, 1328–1331.

Russo, G., di Bernardo, M., & Sontag, E. D. (2010). Global entrainment of transcriptional systems to periodic inputs. PLoS Computational Biology, 6, e1000739.

Wang, W., & Slotine, J. J. E. (2005). On partial contraction analysis for coupled nonlinear oscillators. Biological Cybernetics, 92, 38–53.

Yi, X., Lu, W. L., & Chen, T. P. (2013). Achieving synchronization in arrays of coupled differential systems with time-varying couplings. Abstract and Applied Analysis, 2013, 134265.